(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~60~ubuntu17.10.1)
  (general
    (links 60)
    (no_connects 0)
    (area 178.377 33.579999 213.689001 135.965001)
    (thickness 1.6)
    (drawings 21)
    (tracks 194)
    (zones 0)
    (modules 31)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.8 3.8)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory plot))
  )
  (net 0 "")
  (net 1 /AUDIO_L)
  (net 2 GND)
  (net 3 /AUDIO_R)
  (net 4 "Net-(C1-Pad1)")
  (net 5 +12V)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 /SW_AUDIO_R)
  (net 9 /SW_AUDIO_L)
  (net 10 /AUDIO)
  (net 11 /CSYNC)
  (net 12 "Net-(C4-Pad2)")
  (net 13 /CVBS_CSYNC)
  (net 14 /R-RY)
  (net 15 /GY)
  (net 16 /B-BY)
  (net 17 /HD_CS)
  (net 18 "Net-(C2-Pad1)")
  (net 19 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net /AUDIO)
    (add_net /AUDIO_L)
    (add_net /AUDIO_R)
    (add_net /B-BY)
    (add_net /CSYNC)
    (add_net /CVBS_CSYNC)
    (add_net /GY)
    (add_net /HD_CS)
    (add_net /R-RY)
    (add_net /SW_AUDIO_L)
    (add_net /SW_AUDIO_R)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
  )
  (module molex-fpc:52852-1472 (layer F.Cu) (tedit 5AD3A4E5)
    (at 203.454 72.263 90)
    (fp_text reference J4 (at 16.2306 4.9784 90) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 6.45 3.5 90) (layer F.Fab))
    (pad "" smd rect (at 16.15 2.35 90) (size 2.1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /GY))
    (pad 2 smd rect (at 1 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /B-BY))
    (pad 4 smd rect (at 3 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 4 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /R-RY))
    (pad 6 smd rect (at 5 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 6 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /HD_CS))
    (pad 8 smd rect (at 7 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 8 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 9 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 10 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /AUDIO))
    (pad 12 smd rect (at 11 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 12 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 14 smd rect (at 13 0 90) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" smd rect (at -3.15 2.35 90) (size 2.1 2.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB3FBE3)
    (at 181.102 58.801 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.921 0.127 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /CVBS_CSYNC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AD3A37F)
    (at 186.69 54.229 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.4224 1.4986 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 186.563 62.357 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 183.388 46.99 270)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AD3A3B1)
    (at 197.739 60.579 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.4986 1.6002 270) (layer F.SilkS))
    (fp_text value R_LED (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5AD3A38A)
    (at 186.69 58.293)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -3.7084 -3.7338 270) (layer F.SilkS))
    (fp_text value LM1881 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /CSYNC))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C4-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AD39700)
    (at 193.548 60.325 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -1.4605 1.5875 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AD8D9C1)
    (at 193.548 63.119 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.302 0.0254 270) (layer F.SilkS))
    (fp_text value 680k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module eswitch-dpdt:eswitch-dpdt-m2 (layer F.Cu) (tedit 5AB17F78)
    (at 210.312 94.234 180)
    (fp_text reference SW1 (at 5.1 12.15 180) (layer F.SilkS))
    (fp_text value SW_DPDT_x2 (at 2.55 -2.8 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 9 /SW_AUDIO_L))
    (pad 4 thru_hole circle (at 4.83 0 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 8 /SW_AUDIO_R))
    (pad 2 thru_hole circle (at 0 4.7 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 /AUDIO_L))
    (pad 5 thru_hole circle (at 4.83 4.7 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 3 /AUDIO_R))
    (pad 3 thru_hole circle (at 0 9.4 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 10 /AUDIO))
    (pad 6 thru_hole circle (at 4.83 9.4 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 10 /AUDIO))
  )
  (module eswitch-dpdt:eswitch-dpdt-m2 (layer F.Cu) (tedit 5AB17F78)
    (at 198.501 49.53 180)
    (fp_text reference SW2 (at 5.1 12.15 180) (layer F.SilkS))
    (fp_text value SW_DPDT_x2 (at 2.55 -2.8 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 13 /CVBS_CSYNC))
    (pad 4 thru_hole circle (at 4.83 0 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 4.7 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 17 /HD_CS))
    (pad 5 thru_hole circle (at 4.83 4.7 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at 0 9.4 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 11 /CSYNC))
    (pad 6 thru_hole circle (at 4.83 9.4 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AB2A467)
    (at 183.388 130.429)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J5 (at 0 -4.2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AB2A46E)
    (at 183.388 39.116)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J6 (at 0 -4.2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AB2BBC9)
    (at 208.788 39.116)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J7 (at 0 -4.2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 208.788 130.429)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (zone_connect 2)
    (fp_text reference J8 (at 0 -4.2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5ABA700E)
    (at 200.406 76.962)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J9 (at 0 -4.2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 202.5015 54.6735 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AD3A4F1)
    (at 206.2988 45.5168)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -3.0861 0.0635 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AD3A0EE)
    (at 206.1972 59.1312)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J10 (at 2.032 1.2192) (layer B.SilkS))
    (fp_text value TEST_12V (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 5 +12V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AD3A0D9)
    (at 206.1972 61.2648)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J11 (at 2.032 1.1176) (layer B.SilkS))
    (fp_text value TEST_GND (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AD3A0AF)
    (at 206.1972 68.2244)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J12 (at 2.0828 0.9144) (layer B.SilkS))
    (fp_text value TEST_R/R-Y (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 /R-RY))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AD3A0A3)
    (at 206.248 72.2884)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J13 (at 2.0828 1.3208) (layer B.SilkS))
    (fp_text value TEST_G/G-Y (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 15 /GY))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AD3A09C)
    (at 206.248 70.2564)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J14 (at 2.1336 0.8636) (layer B.SilkS))
    (fp_text value TEST_B/B-Y (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 16 /B-BY))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AD3A0BE)
    (at 206.1972 66.1924)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J16 (at 2.032 1.1684) (layer B.SilkS))
    (fp_text value TEST_HD/CS (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 17 /HD_CS))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5AD3A0C9)
    (at 206.1972 64.1604)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J17 (at 2.032 1.3208) (layer B.SilkS))
    (fp_text value TEST_AUDIO (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 10 /AUDIO))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5AD77948)
    (at 208.407 50.292)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.0734 4.5212) (layer F.SilkS))
    (fp_text value AZ1117-5.0 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rca:RCJ-02 (layer F.Cu) (tedit 5AD8D9FF)
    (at 205.105 119.507)
    (fp_text reference J3 (at -0.0254 -3.0734 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -4.15 -2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.7) (layers *.Cu *.Mask)
      (net 9 /SW_AUDIO_L))
  )
  (module rca:RCJ-02 (layer F.Cu) (tedit 5AD8D9F9)
    (at 205.105 105.791)
    (fp_text reference J2 (at -0.0254 -2.9718 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -4.15 -2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.7) (layers *.Cu *.Mask)
      (net 8 /SW_AUDIO_R))
  )
  (module scart-conn:K-SCARTX-024 (layer F.Cu) (tedit 5AE62249)
    (at 190.373 91.313 270)
    (fp_text reference J1 (at -22.225 -2.54 270) (layer F.SilkS))
    (fp_text value SCART-F (at -26.035 2.54 360) (layer F.Fab))
    (pad "" np_thru_hole oval (at -22.86 2.54 270) (size 2 4.8) (drill oval 2 4.8) (layers *.Cu *.SilkS *.Mask Dwgs.User Eco1.User Eco2.User))
    (pad 20 thru_hole circle (at -17.145 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 13 /CVBS_CSYNC))
    (pad 18 thru_hole circle (at -13.335 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at -9.525 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at -1.905 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 1.905 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at 9.525 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 /AUDIO_L))
    (pad 4 thru_hole circle (at 13.335 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 17.145 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 /AUDIO_R))
    (pad 21 thru_hole circle (at -19.04 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 19 thru_hole circle (at -15.23 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at -11.42 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole circle (at -7.61 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 14 /R-RY))
    (pad 13 thru_hole circle (at -3.8 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole circle (at 0.01 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 /GY))
    (pad 9 thru_hole circle (at 3.82 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole circle (at 7.63 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 /B-BY))
    (pad 5 thru_hole circle (at 11.44 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 15.25 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 19.06 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole oval (at 22.86 2.54 270) (size 2 4.8) (drill oval 2 4.8) (layers *.Cu *.Mask))
  )
  (module smd-jumper:SMD-JUMPER (layer F.Cu) (tedit 5AE7840C)
    (at 193.3575 57.3405)
    (fp_text reference JP1 (at -1.8415 -0.1397 90) (layer F.SilkS))
    (fp_text value 5V (at 0 -1.7) (layer F.Fab))
    (pad 2 smd trapezoid (at 0.5 0) (size 0.8 1.27) (rect_delta 0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 1 smd trapezoid (at -0.5 0) (size 0.8 1.27) (rect_delta -0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
  )
  (module smd-jumper:SMD-JUMPER (layer F.Cu) (tedit 5AE78405)
    (at 191.897 54.356)
    (fp_text reference JP2 (at -0.0762 -1.8288 180) (layer F.SilkS))
    (fp_text value 12V (at 0 -1.7) (layer F.Fab))
    (pad 2 smd trapezoid (at 0.5 0) (size 0.8 1.27) (rect_delta 0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 1 smd trapezoid (at -0.5 0) (size 0.8 1.27) (rect_delta -0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
  )
  (gr_line (start 186.309 114.173) (end 189.357 114.173) (angle 90) (layer Edge.Cuts) (width 2))
  (gr_line (start 186.309 68.453) (end 189.357 68.453) (angle 90) (layer Edge.Cuts) (width 2))
  (gr_text 12V (at 196.6976 56.9468) (layer F.SilkS))
  (gr_text 5V (at 194.564 54.356) (layer F.SilkS))
  (gr_text G/Y (at 202.4888 72.39) (layer B.SilkS))
  (gr_text B/B-Y (at 200.8632 70.4088) (layer B.SilkS))
  (gr_text R/R-Y (at 200.8124 68.4276) (layer B.SilkS))
  (gr_text HD/CS (at 200.914 66.2432) (layer B.SilkS))
  (gr_text AUDIO (at 201.168 64.1096) (layer B.SilkS))
  (gr_text GND (at 202.438 61.3156) (layer B.SilkS))
  (gr_text 12V (at 202.5396 59.1312) (layer B.SilkS))
  (gr_line (start 213.614 75.311) (end 213.614 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.614 56.134) (end 213.614 33.655) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 209.677 75.311) (end 213.614 75.311) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 209.677 56.134) (end 209.677 75.311) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.614 56.134) (end 209.677 56.134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text LEFT (at 205.0796 123.444) (layer F.SilkS))
  (gr_text RIGHT (at 205.1304 109.7788) (layer F.SilkS))
  (gr_line (start 213.614 33.655) (end 178.562 33.655) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.562 135.89) (end 178.562 33.655) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.614 135.89) (end 178.562 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.943 34.036) (xy 197.612 34.036) (xy 213.36 34.036) (xy 213.36 55.88) (xy 209.423 55.88)
        (xy 209.423 75.565) (xy 213.36 75.565) (xy 213.36 135.636) (xy 178.816 135.636) (xy 178.816 34.036)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.943 34.036) (xy 197.612 34.036) (xy 213.36 34.036) (xy 213.36 55.88) (xy 209.423 55.88)
        (xy 209.423 75.565) (xy 213.36 75.565) (xy 213.36 135.636) (xy 178.816 135.636) (xy 178.816 34.036)
      )
    )
  )
)
