(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 31)
    (zones 0)
    (modules 4)
    (nets 12)
  )
  (page B)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 145.669 145.669)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers_1"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad12)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
  )
  (module Daves_footprints:RJ45_panel_RA_MRJR-5381-01 (layer F.Cu) (tedit 5CF2FD5F)
    (at 143.129 160.8455 270)
    (fp_text reference J1 (at 0.05 -20.5 270) (layer F.SilkS))
    (fp_text value 8P8C_LED_Shielded (at -0.05 -1.2 270) (layer F.Fab) hide)
    (pad SH thru_hole circle (at -5 -6.5 270) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad SH thru_hole circle (at 5 -6.5 270) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 thru_hole circle (at -4.44 -14.5 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -3.17 -17.04 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -1.9 -14.5 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -0.63 -17.04 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 0.64 -14.5 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 1.91 -17.04 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 3.18 -14.5 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 4.45 -17.04 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 12 thru_hole circle (at -6.53 -10.5 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (pad 11 thru_hole circle (at -3.99 -10.5 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 10 thru_hole circle (at 3.99 -10.5 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 thru_hole circle (at 6.53 -10.5 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Dave.3dshapes/RJ45_panel_RA_MRJR_5381_01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Ethernet_RA_2-406541-2 (layer F.Cu) (tedit 5CF2E666)
    (at 181.2925 160.7185 90)
    (fp_text reference J2 (at 0 -8.128 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 0 9.652 90) (layer F.Fab) hide)
    (pad SH thru_hole circle (at -8.128 0 90) (size 2.54 2.54) (drill 1.5748) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad SH thru_hole circle (at 8.128 0 90) (size 2.54 2.54) (drill 1.5748) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad "" np_thru_hole circle (at -6.35 3.429 90) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 3.429 90) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -3.556 -0.889 90) (size 1.3 1.3) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 7 thru_hole circle (at -2.54 0.889 90) (size 1.3 1.3) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 6 thru_hole circle (at -1.524 -0.889 90) (size 1.3 1.3) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at -0.508 0.889 90) (size 1.3 1.3) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at 0.508 -0.889 90) (size 1.3 1.3) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 1.524 0.889 90) (size 1.3 1.3) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 -0.889 90) (size 1.3 1.3) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 3.556 0.889 90) (size 1.3 1.3) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Dave.3dshapes/Ethernet_RA_2_406541_2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 165.862 153.3525 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at -2.3495 2.286 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daves_footprints:Steward_Logo (layer B.Cu) (tedit 5BF5C8E2)
    (at 186.817 160.4645)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (dimension 19.812 (width 0.3) (layer Dwgs.User)
    (gr_text "19.812 mm" (at 196.7275 160.7185 270) (layer Dwgs.User))
    (feature1 (pts (xy 190.5 170.6245) (xy 195.213921 170.6245)))
    (feature2 (pts (xy 190.5 150.8125) (xy 195.213921 150.8125)))
    (crossbar (pts (xy 194.6275 150.8125) (xy 194.6275 170.6245)))
    (arrow1a (pts (xy 194.6275 170.6245) (xy 194.041079 169.497996)))
    (arrow1b (pts (xy 194.6275 170.6245) (xy 195.213921 169.497996)))
    (arrow2a (pts (xy 194.6275 150.8125) (xy 194.041079 151.939004)))
    (arrow2b (pts (xy 194.6275 150.8125) (xy 195.213921 151.939004)))
  )
  (dimension 45.212045 (width 0.3) (layer Dwgs.User)
    (gr_text "45.212 mm" (at 168.252609 134.90128 0.08047154753) (layer Dwgs.User))
    (feature1 (pts (xy 190.881 150.8125) (xy 190.860734 136.383107)))
    (feature2 (pts (xy 145.669 150.876) (xy 145.648734 136.446607)))
    (crossbar (pts (xy 145.649558 137.033028) (xy 190.861558 136.969528)))
    (arrow1a (pts (xy 190.861558 136.969528) (xy 189.735879 137.55753)))
    (arrow1b (pts (xy 190.861558 136.969528) (xy 189.734232 136.38469)))
    (arrow2a (pts (xy 145.649558 137.033028) (xy 146.776884 137.617866)))
    (arrow2b (pts (xy 145.649558 137.033028) (xy 146.775237 136.445026)))
  )
  (gr_text "Version 1.0\nD. Hamara\n2019/06/02" (at 169.7355 162.1155) (layer B.SilkS))
  (gr_text GUSTO-UA-DWG-00067 (at 170.4975 158.9405) (layer B.SilkS))
  (gr_text "GUSTO Ethernet Adapter" (at 170.4975 157.4165) (layer B.SilkS))
  (gr_text "STEWARD OBSERVATORY" (at 170.18 155.6385) (layer B.SilkS))
  (gr_line (start 145.669 170.6245) (end 145.669 150.8125) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.881 170.6245) (end 145.669 170.6245) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.881 150.8125) (end 190.881 170.6245) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.669 150.8125) (end 190.881 150.8125) (layer Edge.Cuts) (width 0.15))
  (zone (net 11) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.8595 145.8595) (xy 190.6905 145.8595) (xy 190.6905 175.768) (xy 145.8595 175.8315)
      )
    )
  )
  (zone (net 11) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.8595 145.8595) (xy 190.6905 145.8595) (xy 190.6905 175.768) (xy 145.8595 175.8315)
      )
    )
  )
)
