(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 25)
    (no_connects 0)
    (area 131.949735 88.836499 165.163501 123.99518)
    (thickness 1.6002)
    (drawings 21)
    (tracks 176)
    (zones 0)
    (modules 10)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(JL1-Pad3)")
  (net 4 "Net-(JL1-Pad4)")
  (net 5 "Net-(JN1-Pad1)")
  (net 6 "Net-(JN1-Pad2)")
  (net 7 "Net-(JN1-Pad3)")
  (net 8 "Net-(JN1-Pad4)")
  (net 9 "Net-(JN1-Pad5)")
  (net 10 "Net-(JN1-Pad6)")
  (net 11 "Net-(JN1-Pad7)")
  (net 12 "Net-(JN1-Pad8)")
  (net 13 "Net-(JN1-Pad9)")
  (net 14 "Net-(JN1-Pad10)")
  (net 15 "Net-(JN1-Pad11)")
  (net 16 "Net-(JN1-Pad12)")
  (net 17 "Net-(JR1-Pad1)")
  (net 18 "Net-(LED1-Pad1-DO)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(JL1-Pad3)")
    (add_net "Net-(JL1-Pad4)")
    (add_net "Net-(JN1-Pad1)")
    (add_net "Net-(JN1-Pad10)")
    (add_net "Net-(JN1-Pad11)")
    (add_net "Net-(JN1-Pad12)")
    (add_net "Net-(JN1-Pad2)")
    (add_net "Net-(JN1-Pad3)")
    (add_net "Net-(JN1-Pad4)")
    (add_net "Net-(JN1-Pad5)")
    (add_net "Net-(JN1-Pad6)")
    (add_net "Net-(JN1-Pad7)")
    (add_net "Net-(JN1-Pad8)")
    (add_net "Net-(JN1-Pad9)")
    (add_net "Net-(JR1-Pad1)")
    (add_net "Net-(LED1-Pad1-DO)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module mynixies:mynixies-CD11 (layer F.Cu) (tedit 59829424)
    (at 148.62302 105.42524)
    (attr virtual)
    (fp_text reference NX1 (at 12.66698 -13.35024) (layer F.SilkS))
    (fp_text value CD11ALLPINS (at -10.16 0) (layer F.SilkS) hide)
    (fp_text user Top (at 6.57098 -11.69924) (layer F.SilkS) hide)
    (fp_text user Bottom (at 6.82498 11.66876) (layer F.SilkS) hide)
    (pad 0 thru_hole circle (at -3.82524 -9.23798) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(JN1-Pad11)"))
    (pad 1 thru_hole circle (at -9.23798 3.82524) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(JN1-Pad2)"))
    (pad 2 thru_hole circle (at -7.06882 7.06882) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(JN1-Pad3)"))
    (pad 3 thru_hole circle (at -3.82524 9.23798) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(JN1-Pad4)"))
    (pad 4 thru_hole circle (at 3.82524 9.23798) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(JN1-Pad5)"))
    (pad 5 thru_hole circle (at 7.06882 7.06882) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(JN1-Pad6)"))
    (pad 6 thru_hole circle (at 9.23798 3.82524) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(JN1-Pad7)"))
    (pad 7 thru_hole circle (at 9.23798 -3.82524) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(JN1-Pad8)"))
    (pad 8 thru_hole circle (at 7.06882 -7.06882) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(JN1-Pad9)"))
    (pad 9 thru_hole circle (at 3.82524 -9.23798) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(JN1-Pad10)"))
    (pad A thru_hole circle (at -9.23798 -3.82524) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(JR1-Pad1)"))
    (pad NC@1 thru_hole circle (at -7.06882 -7.06882) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask))
    (pad NC@2 thru_hole circle (at 0 -9.99998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask))
    (pad NC@3 thru_hole circle (at 0 9.99998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 11.1125 11.1125) (drill 11.1125) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 5.08) (size 3.96748 3.96748) (drill 3.96748) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5982873D)
    (at 135.255 105.41 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 270) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 161.417 112.649)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7) (layer F.SilkS))
    (fp_text value R (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(JR1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(JN1-Pad12)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:mermaid_l (layer F.Cu) (tedit 0)
    (at 135.255 93.98)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X04_NO_SILK (layer F.Cu) (tedit 59828BB1)
    (at 152.4 90.17 180)
    (descr "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference JL1 (at 0.254 -1.7018 180) (layer F.SilkS) hide)
    (fp_text value led (at -2.794 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(JL1-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(JL1-Pad4)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X12_NO_SILK (layer F.Cu) (tedit 59828BD5)
    (at 162.56 120.65 180)
    (descr "PLATED THROUGH HOLE -12 PIN NO SILK")
    (tags "PLATED THROUGH HOLE -12 PIN NO SILK")
    (attr virtual)
    (fp_text reference JN1 (at 0.254 -1.7018 180) (layer F.SilkS) hide)
    (fp_text value nixie (at 2.667 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(JN1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(JN1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(JN1-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(JN1-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(JN1-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(JN1-Pad6)"))
    (pad 7 thru_hole circle (at 15.24 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(JN1-Pad7)"))
    (pad 8 thru_hole circle (at 17.78 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(JN1-Pad8)"))
    (pad 9 thru_hole circle (at 20.32 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(JN1-Pad9)"))
    (pad 10 thru_hole circle (at 22.86 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(JN1-Pad10)"))
    (pad 11 thru_hole circle (at 25.4 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(JN1-Pad11)"))
    (pad 12 thru_hole circle (at 27.94 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 16 "Net-(JN1-Pad12)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X02_NO_SILK (layer F.Cu) (tedit 59828BF0)
    (at 160.147 115.443)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference JR1 (at 0.254 -1.7018) (layer F.SilkS) hide)
    (fp_text value jumper (at 1.27 1.778) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(JR1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 16 "Net-(JN1-Pad12)"))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5987AF4D)
    (at 161.925 105.41 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 270) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0.127 -1.524 450) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5987AF1A)
    (at 139.22248 105.39476 180)
    (attr smd)
    (fp_text reference LED1 (at -3.01752 -0.01524 270) (layer F.SilkS))
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54 180) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 270) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED1-Pad1-DO)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 270) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3-DI smd rect (at -1.74752 -0.87376 270) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(JL1-Pad3)"))
    (pad 4-VD smd rect (at -1.74752 0.87376 270) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5987AF12)
    (at 157.95752 105.39476 180)
    (attr smd)
    (fp_text reference LED2 (at 3.175 -0.254 270) (layer F.SilkS))
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54 180) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 270) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(JL1-Pad4)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 270) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3-DI smd rect (at -1.74752 -0.87376 270) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED1-Pad1-DO)"))
    (pad 4-VD smd rect (at -1.74752 0.87376 270) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (gr_text Dout (at 144.907 91.694) (layer F.SilkS))
  (gr_text Din (at 147.447 91.694) (layer F.SilkS))
  (gr_text Vcc (at 149.987 91.694) (layer F.SilkS))
  (gr_text Gnd (at 152.527 91.694) (layer F.SilkS))
  (gr_text NC (at 162.56 118.745) (layer F.SilkS))
  (gr_text 1 (at 160.02 118.745) (layer F.SilkS))
  (gr_text 2 (at 157.48 118.745) (layer F.SilkS))
  (gr_text 3 (at 154.94 118.745) (layer F.SilkS))
  (gr_text 4 (at 152.4 118.745) (layer F.SilkS))
  (gr_text 5 (at 149.86 118.745) (layer F.SilkS))
  (gr_text 6 (at 147.32 118.745) (layer F.SilkS))
  (gr_text 7 (at 144.78 118.745) (layer F.SilkS))
  (gr_text 8 (at 142.24 118.745) (layer F.SilkS))
  (gr_text 9 (at 139.7 118.745) (layer F.SilkS))
  (gr_text 0 (at 137.16 118.745) (layer F.SilkS))
  (gr_text A (at 134.62 118.745) (layer F.SilkS))
  (gr_line (start 132.08 121.92) (end 132.08 88.9) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.1 88.9) (end 165.1 121.92) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 132.08 88.9) (end 165.1 88.9) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.1 121.92) (end 132.08 121.92) (layer Edge.Cuts) (width 0.127))
  (gr_text nixies.us (at 138.43 93.98 90) (layer F.Mask))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.715 89.535) (xy 132.715 98.425) (xy 139.7 98.425) (xy 139.7 89.535)
      )
    )
  )
)
