(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6002)
    (drawings 54)
    (tracks 307)
    (zones 0)
    (modules 40)
    (nets 77)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.27)
    (user_trace_width 1.778)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.762 0.508)
    (user_via 0.889 0.635)
    (user_via 1.016 0.762)
    (user_via 1.143 0.889)
    (user_via 1.27 1.016)
    (user_via 1.524 1.143)
    (user_via 1.778 1.27)
    (user_via 2.032 1.397)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad49)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 /1)
  (net 4 /3)
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 /5)
  (net 8 /7)
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(D5-Pad2)")
  (net 11 /9)
  (net 12 /11)
  (net 13 "Net-(D6-Pad2)")
  (net 14 "Net-(D7-Pad2)")
  (net 15 /13)
  (net 16 /15)
  (net 17 "Net-(D8-Pad2)")
  (net 18 /17)
  (net 19 "Net-(D9-Pad2)")
  (net 20 /19)
  (net 21 "Net-(D10-Pad2)")
  (net 22 "Net-(D11-Pad2)")
  (net 23 /21)
  (net 24 /23)
  (net 25 "Net-(D12-Pad2)")
  (net 26 "Net-(D13-Pad2)")
  (net 27 /25)
  (net 28 /27)
  (net 29 "Net-(D14-Pad2)")
  (net 30 "Net-(D15-Pad2)")
  (net 31 /29)
  (net 32 /31)
  (net 33 "Net-(D16-Pad2)")
  (net 34 "Net-(D17-Pad2)")
  (net 35 /33)
  (net 36 "Net-(D18-Pad2)")
  (net 37 /35)
  (net 38 /37)
  (net 39 "Net-(D19-Pad2)")
  (net 40 "Net-(D20-Pad2)")
  (net 41 /39)
  (net 42 /41)
  (net 43 "Net-(D21-Pad2)")
  (net 44 "Net-(D22-Pad2)")
  (net 45 /43)
  (net 46 /45)
  (net 47 "Net-(D23-Pad2)")
  (net 48 "Net-(D24-Pad2)")
  (net 49 /48)
  (net 50 /49)
  (net 51 "Net-(D25-Pad2)")
  (net 52 "Net-(J1-Pad1)")
  (net 53 "Net-(J1-Pad2)")
  (net 54 "Net-(J1-Pad3)")
  (net 55 "Net-(J1-Pad4)")
  (net 56 "Net-(J1-Pad5)")
  (net 57 "Net-(J1-Pad6)")
  (net 58 "Net-(J1-Pad7)")
  (net 59 "Net-(J1-Pad8)")
  (net 60 "Net-(J1-Pad9)")
  (net 61 "Net-(J1-Pad10)")
  (net 62 "Net-(J1-Pad11)")
  (net 63 "Net-(J1-Pad12)")
  (net 64 "Net-(J1-Pad13)")
  (net 65 "Net-(J1-Pad14)")
  (net 66 "Net-(J1-Pad15)")
  (net 67 "Net-(J1-Pad16)")
  (net 68 "Net-(J1-Pad17)")
  (net 69 "Net-(J1-Pad18)")
  (net 70 "Net-(J1-Pad19)")
  (net 71 "Net-(J1-Pad20)")
  (net 72 "Net-(J1-Pad21)")
  (net 73 "Net-(J1-Pad22)")
  (net 74 "Net-(J1-Pad23)")
  (net 75 "Net-(J1-Pad24)")
  (net 76 "Net-(J1-Pad25)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /1)
    (add_net /11)
    (add_net /13)
    (add_net /15)
    (add_net /17)
    (add_net /19)
    (add_net /21)
    (add_net /23)
    (add_net /25)
    (add_net /27)
    (add_net /29)
    (add_net /3)
    (add_net /31)
    (add_net /33)
    (add_net /35)
    (add_net /37)
    (add_net /39)
    (add_net /41)
    (add_net /43)
    (add_net /45)
    (add_net /48)
    (add_net /49)
    (add_net /5)
    (add_net /7)
    (add_net /9)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D21-Pad2)")
    (add_net "Net-(D22-Pad2)")
    (add_net "Net-(D23-Pad2)")
    (add_net "Net-(D24-Pad2)")
    (add_net "Net-(D25-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad49)")
  )
  (module Custom_footprints:50pin_edge_header (layer B.Cu) (tedit 5EA5C232)
    (at 170.18 66.04 180)
    (fp_text reference J2 (at 0.254 5.588 90) (layer B.SilkS))
    (fp_text value Conn_02x25_Odd_Even (at 0 2.54) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 /1))
    (pad 2 smd roundrect (at 0 0 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 smd roundrect (at 0 -2.54 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 /3))
    (pad 4 smd roundrect (at 0 -2.54 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D2-Pad2)"))
    (pad 5 smd roundrect (at 0 -5.08 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 /5))
    (pad 6 smd roundrect (at 0 -5.08 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D3-Pad2)"))
    (pad 7 smd roundrect (at 0 -7.62 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 /7))
    (pad 8 smd roundrect (at 0 -7.62 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D4-Pad2)"))
    (pad 9 smd roundrect (at 0 -10.16 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 /9))
    (pad 10 smd roundrect (at 0 -10.16 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D5-Pad2)"))
    (pad 11 smd roundrect (at 0 -12.7 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /11))
    (pad 12 smd roundrect (at 0 -12.7 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D6-Pad2)"))
    (pad 13 smd roundrect (at 0 -15.24 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /13))
    (pad 14 smd roundrect (at 0 -15.24 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D7-Pad2)"))
    (pad 15 smd roundrect (at 0 -17.78 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 /15))
    (pad 16 smd roundrect (at 0 -17.78 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D8-Pad2)"))
    (pad 17 smd roundrect (at 0 -20.32 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 /17))
    (pad 18 smd roundrect (at 0 -20.32 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D9-Pad2)"))
    (pad 19 smd roundrect (at 0 -22.86 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 /19))
    (pad 20 smd roundrect (at 0 -22.86 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(D10-Pad2)"))
    (pad 21 smd roundrect (at 0 -25.4 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /21))
    (pad 22 smd roundrect (at 0 -25.4 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D11-Pad2)"))
    (pad 23 smd roundrect (at 0 -27.94 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 /23))
    (pad 24 smd roundrect (at 0 -27.94 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D12-Pad2)"))
    (pad 25 smd roundrect (at 0 -30.48 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /25))
    (pad 26 smd roundrect (at 0 -30.48 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D13-Pad2)"))
    (pad 27 smd roundrect (at 0 -33.02 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /27))
    (pad 28 smd roundrect (at 0 -33.02 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(D14-Pad2)"))
    (pad 29 smd roundrect (at 0 -35.56 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 /29))
    (pad 30 smd roundrect (at 0 -35.56 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(D15-Pad2)"))
    (pad 31 smd roundrect (at 0 -38.1 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 /31))
    (pad 32 smd roundrect (at 0 -38.1 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(D16-Pad2)"))
    (pad 33 smd roundrect (at 0 -40.64 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 /33))
    (pad 34 smd roundrect (at 0 -40.64 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(D17-Pad2)"))
    (pad 35 smd roundrect (at 0 -43.18 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 /35))
    (pad 36 smd roundrect (at 0 -43.18 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(D18-Pad2)"))
    (pad 37 smd roundrect (at 0 -45.72 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 /37))
    (pad 38 smd roundrect (at 0 -45.72 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(D19-Pad2)"))
    (pad 39 smd roundrect (at 0 -48.26 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 /39))
    (pad 40 smd roundrect (at 0 -48.26 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(D20-Pad2)"))
    (pad 41 smd roundrect (at 0 -50.8 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 42 /41))
    (pad 42 smd roundrect (at 0 -50.8 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(D21-Pad2)"))
    (pad 43 smd roundrect (at 0 -53.34 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 /43))
    (pad 44 smd roundrect (at 0 -53.34 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(D22-Pad2)"))
    (pad 45 smd roundrect (at 0 -55.88 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 /45))
    (pad 46 smd roundrect (at 0 -55.88 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(D23-Pad2)"))
    (pad 47 smd roundrect (at 0 -58.42 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 49 /48))
    (pad 48 smd roundrect (at 0 -58.42 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(D24-Pad2)"))
    (pad 49 smd roundrect (at 0 -60.96 270) (size 1.524 4.572) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J2-Pad49)"))
    (pad 50 smd roundrect (at 0 -60.96 270) (size 1.524 4.572) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(D25-Pad2)"))
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 66.04 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /3))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 71.12 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 /5))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 8 /7))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(J1-Pad4)"))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 76.2 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(J1-Pad5)"))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 12 /11))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 81.28 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 /13))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 16 /15))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(J1-Pad8)"))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(J1-Pad7)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 86.36 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN5 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 18 /17))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 20 /19))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(J1-Pad10)"))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(J1-Pad9)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 91.44 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN6 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(J1-Pad11)"))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(J1-Pad12)"))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 24 /23))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 23 /21))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 96.52 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN7 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 27 /25))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 28 /27))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(J1-Pad14)"))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(J1-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 101.6 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN8 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(J1-Pad15)"))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(J1-Pad16)"))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 32 /31))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 31 /29))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 106.68 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN9 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 35 /33))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 37 /35))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(J1-Pad18)"))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(J1-Pad17)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 111.76 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN10 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(J1-Pad19)"))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(J1-Pad20)"))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 41 /39))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 38 /37))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 116.84 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN11 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 42 /41))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 45 /43))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(J1-Pad22)"))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(J1-Pad21)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 121.92 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN12 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(J1-Pad23)"))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(J1-Pad24)"))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 49 /48))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 46 /45))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_2x0603 (layer B.Cu) (tedit 58E0A873)
    (at 162.56 127 180)
    (descr "Chip Resistor Network, ROHM MNR12 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN13 (at 0 1.75) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J2-Pad49)"))
    (pad 2 smd rect (at -0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 50 /49))
    (pad 3 smd rect (at 0.9 -0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(J1-Pad25)"))
    (pad 4 smd rect (at 0.9 0.5 180) (size 0.8 0.5) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(J1-Pad25)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 66.04)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at -2.794 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 /1))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 68.58)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at -2.794 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 /3))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 71.12)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at -2.794 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /5))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 73.66)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at -2.794 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 /7))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 76.2)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at -2.794 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 /9))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 78.74)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at -2.794 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 /11))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 81.28)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D7 (at -2.794 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 /13))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 83.82)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D8 (at -2.794 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 /15))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 86.36)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D9 (at -2.794 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 /17))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 88.9)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D10 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /19))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 91.44)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D11 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 /21))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 93.98)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D12 (at -3.048 0.254) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 /23))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 96.52)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D13 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 /25))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 99.06)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D14 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 /27))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D14-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 101.6)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D15 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 /29))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 104.14)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D16 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 /31))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D16-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 106.68)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D17 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D17-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 /33))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 109.22)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D18 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D18-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 /35))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 111.76)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D19 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 /37))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D19-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 114.3)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D20 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D20-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 /39))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 116.84)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D21 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 /41))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D21-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 119.38)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D22 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D22-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 /43))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 121.92)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D23 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 /45))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D23-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 124.46)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D24 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D24-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 49 /48))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 162.56 127)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D25 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Zener_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 /49))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D25-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x25_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 156.21 66.04)
    (descr "Through hole straight pin header, 1x25, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x25 2.54mm single row")
    (fp_text reference J1 (at 0 -4.572) (layer F.SilkS))
    (fp_text value Conn_01x25_Male (at 0 63.29) (layer F.Fab))
    (fp_text user %R (at 0 30.48 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J1-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J1-Pad19)"))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(J1-Pad20)"))
    (pad 21 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(J1-Pad21)"))
    (pad 22 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(J1-Pad22)"))
    (pad 23 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(J1-Pad23)"))
    (pad 24 thru_hole oval (at 0 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(J1-Pad24)"))
    (pad 25 thru_hole oval (at 0 60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(J1-Pad25)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x25_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text +5V (at 165.862 127) (layer B.SilkS))
  (gr_text +5V (at 165.862 127) (layer F.SilkS))
  (gr_text 37 (at 166.37 111.76) (layer F.SilkS))
  (gr_text 23 (at 166.37 93.98) (layer F.SilkS))
  (gr_text 45 (at 166.37 121.92) (layer F.SilkS))
  (gr_text 39 (at 166.37 114.3) (layer F.SilkS))
  (gr_text 31 (at 166.37 104.14) (layer F.SilkS))
  (gr_text 33 (at 166.37 106.68) (layer F.SilkS))
  (gr_text 25 (at 166.37 96.52) (layer F.SilkS))
  (gr_text 47 (at 166.37 124.46) (layer F.SilkS))
  (gr_text 27 (at 166.37 99.06) (layer F.SilkS))
  (gr_text 35 (at 166.37 109.22) (layer F.SilkS))
  (gr_text 43 (at 166.37 119.38) (layer F.SilkS))
  (gr_text 41 (at 166.37 116.84) (layer F.SilkS))
  (gr_text 29 (at 166.37 101.6) (layer F.SilkS))
  (gr_text 21 (at 166.37 91.44) (layer F.SilkS))
  (gr_text 11 (at 166.37 78.74) (layer F.SilkS))
  (gr_text 13 (at 166.37 81.28) (layer F.SilkS))
  (gr_text 5 (at 166.37 71.12) (layer F.SilkS))
  (gr_text 19 (at 166.37 88.9) (layer F.SilkS))
  (gr_text 9 (at 166.37 76.2) (layer F.SilkS))
  (gr_text 7 (at 166.37 73.66) (layer F.SilkS))
  (gr_text 1 (at 166.37 66.04) (layer F.SilkS))
  (gr_text 3 (at 166.37 68.58) (layer F.SilkS))
  (gr_text 15 (at 166.37 83.82) (layer F.SilkS))
  (gr_text 17 (at 166.37 86.36) (layer F.SilkS))
  (gr_text 47 (at 166.37 124.46) (layer B.SilkS))
  (gr_text 45 (at 166.37 121.92) (layer B.SilkS))
  (gr_text 43 (at 166.37 119.38) (layer B.SilkS))
  (gr_text 41 (at 166.37 116.84) (layer B.SilkS))
  (gr_text 39 (at 166.37 114.3) (layer B.SilkS))
  (gr_text 37 (at 166.37 111.76) (layer B.SilkS))
  (gr_text 35 (at 166.37 109.22) (layer B.SilkS))
  (gr_text 33 (at 166.37 106.68) (layer B.SilkS))
  (gr_text 31 (at 166.37 104.14) (layer B.SilkS))
  (gr_text 29 (at 166.37 101.6) (layer B.SilkS))
  (gr_text 27 (at 166.37 99.06) (layer B.SilkS))
  (gr_text 25 (at 166.37 96.52) (layer B.SilkS))
  (gr_text 23 (at 166.37 93.98) (layer B.SilkS))
  (gr_text 21 (at 166.37 91.44) (layer B.SilkS))
  (gr_text 19 (at 166.37 88.9) (layer B.SilkS))
  (gr_text 17 (at 166.37 86.36) (layer B.SilkS))
  (gr_text 15 (at 166.37 83.82) (layer B.SilkS))
  (gr_text 13 (at 166.37 81.28) (layer B.SilkS))
  (gr_text 11 (at 166.37 78.74) (layer B.SilkS))
  (gr_text 9 (at 166.37 76.2) (layer B.SilkS))
  (gr_text 7 (at 166.37 73.66) (layer B.SilkS))
  (gr_text 5 (at 166.37 71.12) (layer B.SilkS))
  (gr_text 3 (at 166.37 68.58) (layer B.SilkS))
  (gr_text 1 (at 166.37 66.04) (layer B.SilkS))
  (gr_line (start 172.72 63.5) (end 172.72 129.54) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.4 63.5) (end 172.72 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.4 129.54) (end 152.4 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 172.72 129.54) (end 152.4 129.54) (layer Edge.Cuts) (width 0.1))
)
