(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 83)
    (no_connects 0)
    (area 33.478572 27.4 136.571429 107.575)
    (thickness 1.6)
    (drawings 36)
    (tracks 423)
    (zones 0)
    (modules 36)
    (nets 32)
  )
  (page USLegal)
  (title_block
    (title "AX5043 Raspberry Pi HAT")
    (date 2018-03-24)
    (rev V1.3)
    (company "Brandenburg Tech, LLC")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.381)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.13)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.75 2.75)
    (pad_drill 2.75)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x000f8_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C7-Pad2)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 "Net-(C8-Pad2)")
  (net 9 "Net-(C8-Pad1)")
  (net 10 "Net-(C9-Pad1)")
  (net 11 "Net-(C10-Pad1)")
  (net 12 +3V3)
  (net 13 "Net-(L8-Pad1)")
  (net 14 "Net-(L8-Pad2)")
  (net 15 AX5043_DATA)
  (net 16 AX5043_DCLK)
  (net 17 AX5043_IRQ)
  (net 18 AX5043_SYSCLK)
  (net 19 I2C_SDA)
  (net 20 I2C_SCL)
  (net 21 AX5043_MOSI)
  (net 22 AX5043_MISO)
  (net 23 AX5043_CLK)
  (net 24 AX5043_SEL)
  (net 25 AX5043_GPADC2)
  (net 26 AX5043_GPADC1)
  (net 27 "Net-(P3-Pad4)")
  (net 28 "Net-(P3-Pad5)")
  (net 29 "Net-(U1-Pad27)")
  (net 30 "Net-(U1-Pad28)")
  (net 31 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net AX5043_CLK)
    (add_net AX5043_DATA)
    (add_net AX5043_DCLK)
    (add_net AX5043_GPADC1)
    (add_net AX5043_GPADC2)
    (add_net AX5043_IRQ)
    (add_net AX5043_MISO)
    (add_net AX5043_MOSI)
    (add_net AX5043_SEL)
    (add_net AX5043_SYSCLK)
    (add_net GND)
    (add_net I2C_SCL)
    (add_net I2C_SDA)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(L8-Pad1)")
    (add_net "Net-(L8-Pad2)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
  )
  (module AX5043-1-TA05:QFN50P500X500X95-29N (layer F.Cu) (tedit 5A7A3E2D)
    (at 77.0255 59.8805 90)
    (descr "QFN28 5 mm x 5 mm")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference U1 (at 4.318 3.4925 180) (layer F.SilkS))
    (fp_text value AX5043 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.7305 -2.032 180) (layer F.SilkS))
    (pad 29a smd rect (at 0 0 90) (size 0.9 0.9) (layers F.Cu F.Paste))
    (pad 29a smd rect (at 1.0795 0 90) (size 0.9 0.9) (layers F.Cu F.Paste))
    (pad 29a smd rect (at -1.0795 0 90) (size 0.9 0.9) (layers F.Cu F.Paste))
    (pad 29a smd rect (at 1.0795 1.0795 90) (size 0.9 0.9) (layers F.Cu F.Paste))
    (pad 29a smd rect (at -1.0795 1.0795 90) (size 0.9 0.9) (layers F.Cu F.Paste))
    (pad 29a smd rect (at 0 1.0795 90) (size 0.9 0.9) (layers F.Cu F.Paste))
    (pad 29a smd rect (at 1.0795 -1.0795 90) (size 0.9 0.9) (layers F.Cu F.Paste))
    (pad 29a smd rect (at -1.0795 -1.0795 90) (size 0.9 0.9) (layers F.Cu F.Paste))
    (pad 1 smd rect (at -2.35 -1.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 2 smd rect (at -2.35 -1 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.1))
    (pad 3 smd rect (at -2.35 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 4 smd rect (at -2.35 0 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 5 smd rect (at -2.35 0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.1))
    (pad 6 smd rect (at -2.35 1 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.1))
    (pad 7 smd rect (at -2.35 1.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 8 smd rect (at -1.5 2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.1))
    (pad 9 smd rect (at -1 2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(L8-Pad2)") (solder_paste_margin_ratio -0.1))
    (pad 10 smd rect (at -0.5 2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(L8-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 11 smd rect (at 0 2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 15 AX5043_DATA) (solder_paste_margin_ratio -0.1))
    (pad 12 smd rect (at 0.5 2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 16 AX5043_DCLK) (solder_paste_margin_ratio -0.1))
    (pad 13 smd rect (at 1 2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 18 AX5043_SYSCLK) (solder_paste_margin_ratio -0.1))
    (pad 14 smd rect (at 1.5 2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 24 AX5043_SEL) (solder_paste_margin_ratio -0.1))
    (pad 15 smd rect (at 2.35 1.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 23 AX5043_CLK) (solder_paste_margin_ratio -0.1))
    (pad 16 smd rect (at 2.35 1 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 22 AX5043_MISO) (solder_paste_margin_ratio -0.1))
    (pad 17 smd rect (at 2.35 0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 21 AX5043_MOSI) (solder_paste_margin_ratio -0.1))
    (pad 18 smd rect (at 2.35 0 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.1))
    (pad 19 smd rect (at 2.35 -0.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 17 AX5043_IRQ) (solder_paste_margin_ratio -0.1))
    (pad 20 smd rect (at 2.35 -1 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P3-Pad5)") (solder_paste_margin_ratio -0.1))
    (pad 21 smd rect (at 2.35 -1.5 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P3-Pad4)") (solder_paste_margin_ratio -0.1))
    (pad 22 smd rect (at 1.5 -2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.1))
    (pad 23 smd rect (at 1 -2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3) (solder_paste_margin_ratio -0.1))
    (pad 24 smd rect (at 0.5 -2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.1))
    (pad 25 smd rect (at 0 -2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 26 AX5043_GPADC1) (solder_paste_margin_ratio -0.1))
    (pad 26 smd rect (at -0.5 -2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 25 AX5043_GPADC2) (solder_paste_margin_ratio -0.1))
    (pad 27 smd rect (at -1 -2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad27)") (solder_paste_margin_ratio -0.1))
    (pad 28 smd rect (at -1.5 -2.35 90) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad28)") (solder_paste_margin_ratio -0.1))
    (pad 29 smd rect (at 0 0 90) (size 3.3 3.3) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 29a smd rect (at 0 -1.0795 90) (size 0.9 0.9) (layers F.Cu F.Paste))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5A7A0CA2)
    (at 54.737 49.403)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25) (layer F.SilkS))
    (fp_text value LED (at 1.524 1.397) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module ECX42:Crystal_SMD_ECX42-4pin_4.0x2.5mm (layer F.Cu) (tedit 5A7A0A96)
    (at 67.818 61.595 90)
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at -3.556 -0.127 180) (layer F.SilkS))
    (fp_text value 16M (at 0.5 2.45 90) (layer F.Fab))
    (fp_text user 1 (at -2.921 1.9685 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0.8 90) (size 1.4 1.15) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad28)"))
    (pad 2 smd rect (at 1.5 0.8 90) (size 1.4 1.15) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.5 -0.8 90) (size 1.4 1.15) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad27)"))
    (pad 4 smd rect (at -1.5 -0.8 90) (size 1.4 1.15) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_Abracon_ABM3C-4pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-8-1EP_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 5A7A0D0E)
    (at 95.631 58.547 270)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.65")
    (attr smd)
    (fp_text reference U2 (at 1.3335 -2.54 270) (layer F.SilkS))
    (fp_text value MAX31725 (at 0 2.55 270) (layer F.Fab))
    (fp_text user 1 (at -2.286 -1.5875 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.55 -0.975 270) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 I2C_SDA))
    (pad 2 smd rect (at -1.55 -0.325 270) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 20 I2C_SCL))
    (pad 3 smd rect (at -1.55 0.325 270) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.55 0.975 270) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.55 0.975 270) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.55 0.325 270) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 1.55 -0.325 270) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.55 -0.975 270) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 9 smd rect (at 0.3875 0.6 270) (size 0.775 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.3875 -0.6 270) (size 0.775 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.3875 0.6 270) (size 0.775 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.3875 -0.6 270) (size 0.775 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RPi_Hat:Pin_Header_Straight_2x20 locked (layer F.Cu) (tedit 59FA221C)
    (at 76.4 42.1 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -4.1915 -22.679 90) (layer F.SilkS))
    (fp_text value CONN_13X2 (at -1.27 -27.23 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 +3V3))
    (pad 2 thru_hole oval (at 1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at -1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 AX5043_DATA))
    (pad 4 thru_hole oval (at 1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at -1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 AX5043_DCLK))
    (pad 6 thru_hole oval (at 1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole oval (at -1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at -1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at -1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 AX5043_IRQ))
    (pad 12 thru_hole oval (at 1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at -1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 AX5043_SYSCLK))
    (pad 14 thru_hole oval (at 1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at -1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole oval (at 1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 I2C_SDA))
    (pad 17 thru_hole oval (at -1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole oval (at 1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 I2C_SCL))
    (pad 19 thru_hole oval (at -1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 AX5043_MOSI))
    (pad 20 thru_hole oval (at 1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole oval (at -1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 AX5043_MISO))
    (pad 22 thru_hole oval (at 1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole oval (at -1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 AX5043_CLK))
    (pad 24 thru_hole oval (at 1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 AX5043_SEL))
    (pad 25 thru_hole oval (at -1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole oval (at 1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 27 thru_hole oval (at -1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 28 thru_hole oval (at 1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 29 thru_hole oval (at -1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole oval (at 1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole oval (at -1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 32 thru_hole oval (at 1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 33 thru_hole oval (at -1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 34 thru_hole oval (at 1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 35 thru_hole oval (at -1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole oval (at 1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole oval (at -1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 38 thru_hole oval (at 1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 39 thru_hole oval (at -1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 40 thru_hole oval (at 1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217C7B)
    (at 105.4 42.1)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 105.4 91.1)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CB9)
    (at 47.4 91.1)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CA2)
    (at 47.4 42.1)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D799)
    (at 74.8665 83.6295 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 3.175 -0.0635 270) (layer F.SilkS))
    (fp_text value NS (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D790)
    (at 77.1525 81.5975 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.0635 -2.667 270) (layer F.SilkS))
    (fp_text value NS (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D7A2)
    (at 74.8665 79.5655 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 3.1115 -0.0635 270) (layer F.SilkS))
    (fp_text value NS (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D78B)
    (at 77.4065 77.5335 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0.1905 -2.667 270) (layer F.SilkS))
    (fp_text value 5p1 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D7D9)
    (at 74.8665 73.7235 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 3.175 -0.0635 450) (layer F.SilkS))
    (fp_text value 11p (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D68F)
    (at 78.1685 73.7235)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 3.175 0.0635 90) (layer F.SilkS))
    (fp_text value 5p6 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D80D)
    (at 75.6285 68.8975 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 2.7305 270) (layer F.SilkS))
    (fp_text value 4p3 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D49B)
    (at 77.4065 68.8975 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -2.7305 270) (layer F.SilkS))
    (fp_text value 4p3 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F66051)
    (at 73.4695 63.8175 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.286 0.127 270) (layer F.SilkS))
    (fp_text value 10n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D6A3)
    (at 80.5815 63.8175)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 3.302 0.635 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59FA222D)
    (at 72.263 57.15 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 2.413 0.3175 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59F7D6B2)
    (at 96.647 62.865 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 3.556 -0.0635 360) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59F7D79E)
    (at 75.6285 81.5975 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 0 2.7305 270) (layer F.SilkS))
    (fp_text value 0R (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59F7D7A9)
    (at 75.6285 77.5335 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at 0.0635 2.667 270) (layer F.SilkS))
    (fp_text value 27n (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59F7D694)
    (at 78.1685 75.2475 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L3 (at -3.175 -0.508 270) (layer F.SilkS))
    (fp_text value 27n (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59F7D806)
    (at 75.6285 71.6915 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L4 (at -0.127 2.7305 270) (layer F.SilkS))
    (fp_text value 43n (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59F7D68B)
    (at 77.4065 71.6915 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L5 (at -0.127 -2.794 270) (layer F.SilkS))
    (fp_text value 43n (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59F7D4A1)
    (at 78.1685 66.6115 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L6 (at -2.8575 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59F7D82D)
    (at 74.8665 66.6115)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L7 (at -3.302 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59F7D6AB)
    (at 81.5975 61.6585 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L8 (at 0.127 -1.9685 270) (layer F.SilkS))
    (fp_text value 0R (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(L8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(L8-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 58C301F2)
    (at 75.6285 89.0905 270)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference P1 (at 0 -5 270) (layer F.SilkS))
    (fp_text value SMA (at 0 5 270) (layer F.Fab))
    (fp_text user %R (at 0 -5 270) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 270) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 270) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 270) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 61.722 63.754 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 15.03 180) (layer F.Fab))
    (fp_text user %R (at 0 6.35 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 AX5043_GPADC2))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 AX5043_GPADC1))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59FA2212)
    (at 57.912 61.214 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.6985 -1.7145 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 AX5043_GPADC2))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59FA220E)
    (at 57.912 58.674 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.889 1.8415 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 AX5043_GPADC1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59F7D6BB)
    (at 97.155 54.356 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3.683 -0.3175 360) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 I2C_SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59F7D6BF)
    (at 95.377 54.356 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -3.81 0.3175 360) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 I2C_SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A4A38CF)
    (at 54.737 51.689)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.0635 1.524) (layer F.SilkS))
    (fp_text value R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Brandenburg Tech, LLC.\nAX 5043 Raspberry Pi Board\n\nV1.3    SN: _____________" (at 103.3145 74.6125 90) (layer F.Cu))
  (gr_text "Dimensions taken from\nhttps://github.com/raspberrypi/hats/blob/master/hat-board-mechanical.pdf" (at 80.4 105.1) (layer Cmts.User))
  (dimension 56 (width 0.15) (layer Dwgs.User)
    (gr_text "56 mm (Thru-hole socket J2)" (at 119.25 66.6 270) (layer Dwgs.User))
    (feature1 (pts (xy 109.9 94.6) (xy 120.6 94.6)))
    (feature2 (pts (xy 109.9 38.6) (xy 120.6 38.6)))
    (crossbar (pts (xy 117.9 38.6) (xy 117.9 94.6)))
    (arrow1a (pts (xy 117.9 94.6) (xy 117.313579 93.473496)))
    (arrow1b (pts (xy 117.9 94.6) (xy 118.486421 93.473496)))
    (arrow2a (pts (xy 117.9 38.6) (xy 117.313579 39.726504)))
    (arrow2b (pts (xy 117.9 38.6) (xy 118.486421 39.726504)))
  )
  (gr_arc (start 105.9 41.6) (end 105.9 38.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 46.9 38.6) (end 105.9 38.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 46.9 41.6) (end 43.9 41.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 11.5 (width 0.15) (layer Dwgs.User)
    (gr_text "11.5 mm" (at 83.050001 88.85 270) (layer Dwgs.User))
    (feature1 (pts (xy 86.9 94.6) (xy 81.700001 94.6)))
    (feature2 (pts (xy 86.9 83.1) (xy 81.700001 83.1)))
    (crossbar (pts (xy 84.400001 83.1) (xy 84.400001 94.6)))
    (arrow1a (pts (xy 84.400001 94.6) (xy 83.81358 93.473496)))
    (arrow1b (pts (xy 84.400001 94.6) (xy 84.986422 93.473496)))
    (arrow2a (pts (xy 84.400001 83.1) (xy 83.81358 84.226504)))
    (arrow2b (pts (xy 84.400001 83.1) (xy 84.986422 84.226504)))
  )
  (dimension 2 (width 0.15) (layer Dwgs.User)
    (gr_text "2 mm" (at 93.65 71.1) (layer Dwgs.User))
    (feature1 (pts (xy 89.9 73.6) (xy 89.9 68.400001)))
    (feature2 (pts (xy 87.9 73.6) (xy 87.9 68.400001)))
    (crossbar (pts (xy 87.9 71.100001) (xy 89.9 71.100001)))
    (arrow1a (pts (xy 89.9 71.100001) (xy 88.773496 71.686422)))
    (arrow1b (pts (xy 89.9 71.100001) (xy 88.773496 70.51358)))
    (arrow2a (pts (xy 87.9 71.100001) (xy 89.026504 71.686422)))
    (arrow2b (pts (xy 87.9 71.100001) (xy 89.026504 70.51358)))
  )
  (dimension 17 (width 0.15) (layer Dwgs.User)
    (gr_text "17 mm" (at 95.25 83.1 270) (layer Dwgs.User))
    (feature1 (pts (xy 90.9 91.6) (xy 96.6 91.6)))
    (feature2 (pts (xy 90.9 74.6) (xy 96.6 74.6)))
    (crossbar (pts (xy 93.9 74.6) (xy 93.9 91.6)))
    (arrow1a (pts (xy 93.9 91.6) (xy 93.313579 90.473496)))
    (arrow1b (pts (xy 93.9 91.6) (xy 94.486421 90.473496)))
    (arrow2a (pts (xy 93.9 74.6) (xy 93.313579 75.726504)))
    (arrow2b (pts (xy 93.9 74.6) (xy 94.486421 75.726504)))
  )
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 52.4 98.1) (layer Dwgs.User))
    (feature1 (pts (xy 47.4 95.6) (xy 47.4 100.8)))
    (feature2 (pts (xy 43.9 95.6) (xy 43.9 100.8)))
    (crossbar (pts (xy 43.9 98.1) (xy 47.4 98.1)))
    (arrow1a (pts (xy 47.4 98.1) (xy 46.273496 98.686421)))
    (arrow1b (pts (xy 47.4 98.1) (xy 46.273496 97.513579)))
    (arrow2a (pts (xy 43.9 98.1) (xy 45.026504 98.686421)))
    (arrow2b (pts (xy 43.9 98.1) (xy 45.026504 97.513579)))
  )
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 54.15 86.35 270) (layer Dwgs.User))
    (feature1 (pts (xy 50.9 94.6) (xy 56.6 94.6)))
    (feature2 (pts (xy 50.9 91.1) (xy 56.6 91.1)))
    (crossbar (pts (xy 53.9 91.1) (xy 53.9 94.6)))
    (arrow1a (pts (xy 53.9 94.6) (xy 53.313579 93.473496)))
    (arrow1b (pts (xy 53.9 94.6) (xy 54.486421 93.473496)))
    (arrow2a (pts (xy 53.9 91.1) (xy 53.313579 92.226504)))
    (arrow2b (pts (xy 53.9 91.1) (xy 54.486421 92.226504)))
  )
  (dimension 49 (width 0.15) (layer Dwgs.User)
    (gr_text "49 mm" (at 114.249999 66.6 270) (layer Dwgs.User))
    (feature1 (pts (xy 109.9 91.1) (xy 115.599999 91.1)))
    (feature2 (pts (xy 109.9 42.1) (xy 115.599999 42.1)))
    (crossbar (pts (xy 112.899999 42.1) (xy 112.899999 91.1)))
    (arrow1a (pts (xy 112.899999 91.1) (xy 112.313578 89.973496)))
    (arrow1b (pts (xy 112.899999 91.1) (xy 113.48642 89.973496)))
    (arrow2a (pts (xy 112.899999 42.1) (xy 112.313578 43.226504)))
    (arrow2b (pts (xy 112.899999 42.1) (xy 113.48642 43.226504)))
  )
  (dimension 19.5 (width 0.15) (layer Dwgs.User)
    (gr_text "19.5 mm" (at 38.55 84.85 270) (layer Dwgs.User))
    (feature1 (pts (xy 42.9 94.6) (xy 37.2 94.6)))
    (feature2 (pts (xy 42.9 75.1) (xy 37.2 75.1)))
    (crossbar (pts (xy 39.9 75.1) (xy 39.9 94.6)))
    (arrow1a (pts (xy 39.9 94.6) (xy 39.313579 93.473496)))
    (arrow1b (pts (xy 39.9 94.6) (xy 40.486421 93.473496)))
    (arrow2a (pts (xy 39.9 75.1) (xy 39.313579 76.226504)))
    (arrow2b (pts (xy 39.9 75.1) (xy 40.486421 76.226504)))
  )
  (dimension 17 (width 0.15) (layer Dwgs.User)
    (gr_text "17 mm" (at 53.25 66.6 270) (layer Dwgs.User))
    (feature1 (pts (xy 49.9 75.1) (xy 54.6 75.1)))
    (feature2 (pts (xy 49.9 58.1) (xy 54.6 58.1)))
    (crossbar (pts (xy 51.9 58.1) (xy 51.9 75.1)))
    (arrow1a (pts (xy 51.9 75.1) (xy 51.313579 73.973496)))
    (arrow1b (pts (xy 51.9 75.1) (xy 52.486421 73.973496)))
    (arrow2a (pts (xy 51.9 58.1) (xy 51.313579 59.226504)))
    (arrow2b (pts (xy 51.9 58.1) (xy 52.486421 59.226504)))
  )
  (dimension 5 (width 0.15) (layer Dwgs.User)
    (gr_text "5 mm" (at 52.65 56.1) (layer Dwgs.User))
    (feature1 (pts (xy 48.9 58.1) (xy 48.9 53.4)))
    (feature2 (pts (xy 43.9 58.1) (xy 43.9 53.4)))
    (crossbar (pts (xy 43.9 56.1) (xy 48.9 56.1)))
    (arrow1a (pts (xy 48.9 56.1) (xy 47.773496 56.686421)))
    (arrow1b (pts (xy 48.9 56.1) (xy 47.773496 55.513579)))
    (arrow2a (pts (xy 43.9 56.1) (xy 45.026504 56.686421)))
    (arrow2b (pts (xy 43.9 56.1) (xy 45.026504 55.513579)))
  )
  (dimension 29 (width 0.15) (layer Dwgs.User)
    (gr_text "29 mm" (at 61.9 49.949999) (layer Dwgs.User))
    (feature1 (pts (xy 76.4 46.1) (xy 76.4 51.299999)))
    (feature2 (pts (xy 47.4 46.1) (xy 47.4 51.299999)))
    (crossbar (pts (xy 47.4 48.599999) (xy 76.4 48.599999)))
    (arrow1a (pts (xy 76.4 48.599999) (xy 75.273496 49.18642)))
    (arrow1b (pts (xy 76.4 48.599999) (xy 75.273496 48.013578)))
    (arrow2a (pts (xy 47.4 48.599999) (xy 48.526504 49.18642)))
    (arrow2b (pts (xy 47.4 48.599999) (xy 48.526504 48.013578)))
  )
  (dimension 58 (width 0.15) (layer Dwgs.User)
    (gr_text "58 mm" (at 76.4 33.25) (layer Dwgs.User))
    (feature1 (pts (xy 105.4 37.1) (xy 105.4 31.9)))
    (feature2 (pts (xy 47.4 37.1) (xy 47.4 31.9)))
    (crossbar (pts (xy 47.4 34.6) (xy 105.4 34.6)))
    (arrow1a (pts (xy 105.4 34.6) (xy 104.273496 35.186421)))
    (arrow1b (pts (xy 105.4 34.6) (xy 104.273496 34.013579)))
    (arrow2a (pts (xy 47.4 34.6) (xy 48.526504 35.186421)))
    (arrow2b (pts (xy 47.4 34.6) (xy 48.526504 34.013579)))
  )
  (dimension 65 (width 0.15) (layer Dwgs.User)
    (gr_text "65 mm" (at 76.4 28.75) (layer Dwgs.User))
    (feature1 (pts (xy 108.9 37.1) (xy 108.9 27.4)))
    (feature2 (pts (xy 43.9 37.1) (xy 43.9 27.4)))
    (crossbar (pts (xy 43.9 30.1) (xy 108.9 30.1)))
    (arrow1a (pts (xy 108.9 30.1) (xy 107.773496 30.686421)))
    (arrow1b (pts (xy 108.9 30.1) (xy 107.773496 29.513579)))
    (arrow2a (pts (xy 43.9 30.1) (xy 45.026504 30.686421)))
    (arrow2b (pts (xy 43.9 30.1) (xy 45.026504 29.513579)))
  )
  (gr_text "Camera Flex Slot\n(Optional)" (at 88.65 98.35) (layer Cmts.User))
  (gr_arc (start 88.9 90.6) (end 87.9 90.6) (angle -180) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 88.9 75.6) (end 87.9 75.6) (angle 180) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.9 75.6) (end 89.9 90.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 87.9 75.6) (end 87.9 90.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 44.9 76.1) (end 43.9 76.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 47.9 74.1) (end 48.9 74.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 47.9 59.1) (end 47.9 58.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 44.9 57.1) (end 44.9 58.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.9 91.6) (end 108.9 91.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 46.9 91.6) (end 46.9 94.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 43.9 76.1) (end 43.9 91.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 43.9 41.1) (end 43.9 57.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 44.9 75.1) (end 47.9 75.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 44.9 58.1) (end 47.9 58.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.9 59.1) (end 48.9 74.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 46.9 94.6) (end 105.9 94.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.9 41.1) (end 108.9 91.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 39.116) (xy 50.8 45.72) (xy 44.45 45.72) (xy 44.45 57.404) (xy 44.704 57.658)
        (xy 48.514 57.658) (xy 49.276 58.42) (xy 49.276 75.692) (xy 44.831 75.692) (xy 44.45 75.946)
        (xy 44.45 87.63) (xy 51.054 87.63) (xy 51.054 93.98) (xy 101.854 93.98) (xy 101.854 87.63)
        (xy 108.458 87.63) (xy 108.204 45.72) (xy 101.981 45.72) (xy 101.981 39.116)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 39.116) (xy 50.8 45.72) (xy 44.45 45.72) (xy 44.45 57.404) (xy 44.704 57.658)
        (xy 48.514 57.658) (xy 49.276 58.42) (xy 49.276 75.692) (xy 44.831 75.692) (xy 44.45 75.946)
        (xy 44.45 87.63) (xy 51.054 87.63) (xy 51.054 93.98) (xy 101.854 93.98) (xy 101.854 87.63)
        (xy 108.458 87.63) (xy 108.204 45.72) (xy 101.981 45.72) (xy 101.981 39.116)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 39.116) (xy 50.8 45.72) (xy 44.45 45.72) (xy 44.45 57.404) (xy 44.704 57.658)
        (xy 48.514 57.658) (xy 49.276 58.42) (xy 49.276 75.692) (xy 44.831 75.692) (xy 44.45 75.946)
        (xy 44.45 87.63) (xy 51.054 87.63) (xy 51.054 93.98) (xy 101.854 93.98) (xy 101.854 87.63)
        (xy 108.458 87.63) (xy 108.204 45.72) (xy 101.981 45.72) (xy 101.981 39.116)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 39.116) (xy 50.8 45.72) (xy 44.45 45.72) (xy 44.45 57.404) (xy 44.704 57.658)
        (xy 48.514 57.658) (xy 49.276 58.42) (xy 49.276 75.692) (xy 44.831 75.692) (xy 44.45 75.946)
        (xy 44.45 87.63) (xy 51.054 87.63) (xy 51.054 93.98) (xy 101.854 93.98) (xy 101.854 87.63)
        (xy 108.458 87.63) (xy 108.204 45.72) (xy 101.981 45.72) (xy 101.981 39.116)
      )
    )
  )
)
