(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 1741)
    (zones 0)
    (modules 183)
    (nets 91)
  )
  (page A4)
  (title_block
    (title "LED Watch, STM32L0")
    (date 2017-01-14)
    (rev A)
    (company "Kevin Cuzner")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.635 0.635)
    (mod_text_width 0.127)
    (pad_size 0.9 0.29)
    (pad_drill 0)
    (pad_to_mask_clearance 0.1524)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000007)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /LEDs/LED_A_R0)
  (net 4 /LEDs/LED_SEG0)
  (net 5 /LEDs/LED_A_R1)
  (net 6 /LEDs/LED_A_R2)
  (net 7 /LEDs/LED_A_R3)
  (net 8 /LEDs/LED_A_R4)
  (net 9 /LEDs/LED_SEG1)
  (net 10 /LEDs/LED_SEG2)
  (net 11 /LEDs/LED_SEG3)
  (net 12 /LEDs/LED_SEG4)
  (net 13 /LEDs/LED_SEG5)
  (net 14 /LEDs/LED_SEG6)
  (net 15 /LEDs/LED_SEG7)
  (net 16 /LEDs/LED_SEG8)
  (net 17 /LEDs/LED_SEG9)
  (net 18 /LEDs/LED_SEG10)
  (net 19 /LEDs/LED_SEG11)
  (net 20 /LEDs/LED_A_R5)
  (net 21 "/Power Supply/VBAT")
  (net 22 "/Power Supply/VUSB")
  (net 23 "Net-(P3-Pad4)")
  (net 24 "Net-(Q1-Pad1)")
  (net 25 /Control/~USB_PRES)
  (net 26 "Net-(Q2-Pad1)")
  (net 27 "Net-(Q2-Pad3)")
  (net 28 "Net-(D4-Pad2)")
  (net 29 /Control/CHG_STAT)
  (net 30 "/Power Supply/CHG_PROG")
  (net 31 "Net-(U2-Pad10)")
  (net 32 "Net-(U3-Pad2)")
  (net 33 "Net-(U3-Pad5)")
  (net 34 "Net-(U3-Pad6)")
  (net 35 /Control/STM32_RESET)
  (net 36 /Control/LED_A0)
  (net 37 /Control/LED_A1)
  (net 38 /Control/LED_A2)
  (net 39 /Control/LED_A3)
  (net 40 /Control/LED_A4)
  (net 41 /Control/LED_A5)
  (net 42 /Control/BUZ_OUTPUT)
  (net 43 "Net-(U3-Pad17)")
  (net 44 /Control/~ACCEL_INT)
  (net 45 "Net-(U3-Pad21)")
  (net 46 /Control/BTN0)
  (net 47 /Control/BTN1)
  (net 48 /Control/BTN2)
  (net 49 /Control/BTN3)
  (net 50 "Net-(U3-Pad28)")
  (net 51 "Net-(U3-Pad29)")
  (net 52 "Net-(U3-Pad30)")
  (net 53 "Net-(U3-Pad31)")
  (net 54 /Control/SWDIO)
  (net 55 /Control/SWCLK)
  (net 56 "Net-(U3-Pad38)")
  (net 57 /Control/LED_C_MUX0)
  (net 58 /Control/LED_C_MUX1)
  (net 59 /Control/LED_C_MUX2)
  (net 60 /Control/LED_C_MUX3)
  (net 61 /Control/~LED_C_EN)
  (net 62 /Control/I2C_SCL)
  (net 63 /Control/I2C_SDA)
  (net 64 "Net-(C18-Pad1)")
  (net 65 "Net-(U4-Pad5)")
  (net 66 /Control/USB_D+)
  (net 67 /Control/USB_D-)
  (net 68 "Net-(U6-Pad17)")
  (net 69 "/Power Supply/+3.3V_REG_SRC")
  (net 70 /Control/USB_D_R-)
  (net 71 /Control/USB_D_R+)
  (net 72 /USB/USB_SHIELD)
  (net 73 "/Power Supply/+3.3V_REG_SW")
  (net 74 /USB/USB_C_D-)
  (net 75 /USB/USB_C_D+)
  (net 76 "/Power Supply/+3.3V_REG_VRDIV")
  (net 77 "/Power Supply/+3.3V_REG_VOUT_SET")
  (net 78 "/Power Supply/+3.3V_REG_OUT")
  (net 79 "Net-(R20-Pad2)")
  (net 80 "Net-(R22-Pad2)")
  (net 81 "Net-(R24-Pad2)")
  (net 82 "Net-(R26-Pad2)")
  (net 83 /Control/STM32_OSC32+)
  (net 84 /Control/STM32_OSC32-)
  (net 85 /LEDs/LED_R_R)
  (net 86 /LEDs/LED_G_R)
  (net 87 /LEDs/LED_B_R)
  (net 88 /LEDs/LED_R_C)
  (net 89 /LEDs/LED_G_C)
  (net 90 /LEDs/LED_B_C)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Control/BTN0)
    (add_net /Control/BTN1)
    (add_net /Control/BTN2)
    (add_net /Control/BTN3)
    (add_net /Control/BUZ_OUTPUT)
    (add_net /Control/CHG_STAT)
    (add_net /Control/I2C_SCL)
    (add_net /Control/I2C_SDA)
    (add_net /Control/LED_A0)
    (add_net /Control/LED_A1)
    (add_net /Control/LED_A2)
    (add_net /Control/LED_A3)
    (add_net /Control/LED_A4)
    (add_net /Control/LED_A5)
    (add_net /Control/LED_C_MUX0)
    (add_net /Control/LED_C_MUX1)
    (add_net /Control/LED_C_MUX2)
    (add_net /Control/LED_C_MUX3)
    (add_net /Control/STM32_OSC32+)
    (add_net /Control/STM32_OSC32-)
    (add_net /Control/STM32_RESET)
    (add_net /Control/SWCLK)
    (add_net /Control/SWDIO)
    (add_net /Control/USB_D+)
    (add_net /Control/USB_D-)
    (add_net /Control/USB_D_R+)
    (add_net /Control/USB_D_R-)
    (add_net /Control/~ACCEL_INT)
    (add_net /Control/~LED_C_EN)
    (add_net /Control/~USB_PRES)
    (add_net /LEDs/LED_A_R0)
    (add_net /LEDs/LED_A_R1)
    (add_net /LEDs/LED_A_R2)
    (add_net /LEDs/LED_A_R3)
    (add_net /LEDs/LED_A_R4)
    (add_net /LEDs/LED_A_R5)
    (add_net /LEDs/LED_B_C)
    (add_net /LEDs/LED_B_R)
    (add_net /LEDs/LED_G_C)
    (add_net /LEDs/LED_G_R)
    (add_net /LEDs/LED_R_C)
    (add_net /LEDs/LED_R_R)
    (add_net /LEDs/LED_SEG0)
    (add_net /LEDs/LED_SEG1)
    (add_net /LEDs/LED_SEG10)
    (add_net /LEDs/LED_SEG11)
    (add_net /LEDs/LED_SEG2)
    (add_net /LEDs/LED_SEG3)
    (add_net /LEDs/LED_SEG4)
    (add_net /LEDs/LED_SEG5)
    (add_net /LEDs/LED_SEG6)
    (add_net /LEDs/LED_SEG7)
    (add_net /LEDs/LED_SEG8)
    (add_net /LEDs/LED_SEG9)
    (add_net "/Power Supply/+3.3V_REG_VOUT_SET")
    (add_net "/Power Supply/+3.3V_REG_VRDIV")
    (add_net "/Power Supply/CHG_PROG")
    (add_net /USB/USB_C_D+)
    (add_net /USB/USB_C_D-)
    (add_net /USB/USB_SHIELD)
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad21)")
    (add_net "Net-(U3-Pad28)")
    (add_net "Net-(U3-Pad29)")
    (add_net "Net-(U3-Pad30)")
    (add_net "Net-(U3-Pad31)")
    (add_net "Net-(U3-Pad38)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U6-Pad17)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net "/Power Supply/+3.3V_REG_OUT")
    (add_net "/Power Supply/+3.3V_REG_SRC")
    (add_net "/Power Supply/+3.3V_REG_SW")
    (add_net "/Power Supply/VBAT")
    (add_net "/Power Supply/VUSB")
    (add_net GND)
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 167.005 93.726)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 167.894 93.853)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 159.258 84.1375)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 161.29 80.137)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 172.085 94.742)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 159.004 90.551 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 0 1.016 270) (layer B.SilkS))
    (fp_text value 8.2p (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 83 /Control/STM32_OSC32+))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 156.3497 81.3181)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 173.7995 96.7105)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 173.863 80.899)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 155.194 96.012)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 158.3309 79.1591)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 155.067 81.915)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 164.846 97.282)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 158.3436 97.6884)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 157.353 84.201)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 159.8676 83.5152)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 169.3672 99.06)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 167.7035 89.535)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 174.9044 85.598)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 172.9232 85.598)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 169.799 91.567)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 166.497 90.932)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 165.989 96.393)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 160.655 93.345)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 163.957 90.805)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 161.163 91.694)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 159.004 92.0496)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 159.3596 86.9188)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 162.179 86.614)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 170.053 83.439)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 169.545 84.328)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 176.8856 91.0336)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 175.1076 90.0684)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 172.339 89.281)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082A4C)
    (at 161.4932 79.3496)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 +3V3) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 167.2635 82.1735)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 166.243 82.169)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 166.243 81.153)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 160.783032 102.186259 252)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D38 (at 0 -1.5 252) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 252) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 72) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 72) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 14 /LEDs/LED_SEG6))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 159.417889 101.66223 246)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D39 (at 0 -1.5 246) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 246) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 66) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 66) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 14 /LEDs/LED_SEG6))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 159.639 98.358729 60)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D73 (at 0 -1.5 60) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 60) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 240) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 240) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 15 /LEDs/LED_SEG7))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 162.195473 102.564721 258)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D37 (at 0 -1.5 258) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 258) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 78) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 78) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 14 /LEDs/LED_SEG6))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 158.115 100.998374 240)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D40 (at 0 -1.5 240) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 240) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 60) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 60) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 15 /LEDs/LED_SEG7))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 175.481733 98.247754 318)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D27 (at 0 -1.5 318) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 318) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 138) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 138) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 12 /LEDs/LED_SEG4))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 176.401967 97.111359 324)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D26 (at 0 -1.5 324) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 324) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 144) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 144) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 12 /LEDs/LED_SEG4))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 174.447754 99.281733 312)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D28 (at 0 -1.5 312) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 312) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 132) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 132) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 12 /LEDs/LED_SEG4))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 156.88864 100.201967 234)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D41 (at 0 -1.5 234) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 234) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 54) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 54) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 15 /LEDs/LED_SEG7))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 154.718266 98.247754 222)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D43 (at 0 -1.5 222) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 222) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 42) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 42) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 15 /LEDs/LED_SEG7))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 155.752245 99.281733 228)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D42 (at 0 -1.5 228) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 228) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 48) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 48) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 15 /LEDs/LED_SEG7))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 153.798032 97.111359 216)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D44 (at 0 -1.5 216) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 216) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 36) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 36) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 15 /LEDs/LED_SEG7))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 170.78211 101.66223 294)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D31 (at 0 -1.5 294) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 294) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 114) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 114) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 13 /LEDs/LED_SEG5))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 173.311359 100.201967 306)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D29 (at 0 -1.5 306) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 306) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 126) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 126) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 12 /LEDs/LED_SEG4))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 172.085 100.998374 300)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D30 (at 0 -1.5 300) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 300) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 120) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 120) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 13 /LEDs/LED_SEG5))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 170.561 98.358729 120)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D71 (at 0 -1.5 120) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 120) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 300) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 300) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 13 /LEDs/LED_SEG5))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 163.639737 102.79347 264)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D36 (at 0 -1.5 264) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 264) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 84) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 84) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 14 /LEDs/LED_SEG6))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 169.416967 102.186259 288)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D32 (at 0 -1.5 288) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 288) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 108) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 108) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 13 /LEDs/LED_SEG5))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 168.004526 102.564721 282)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D33 (at 0 -1.5 282) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 282) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 102) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 102) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 13 /LEDs/LED_SEG5))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 166.560262 102.79347 276)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D34 (at 0 -1.5 276) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 276) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 96) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 96) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 13 /LEDs/LED_SEG5))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 165.1 102.87 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D35 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 14 /LEDs/LED_SEG6))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 165.1 99.822 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D72 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 14 /LEDs/LED_SEG6))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 170.78211 76.137769 66)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D9 (at 0 -1.5 66) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 66) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 246) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 246) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 /LEDs/LED_SEG0))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 172.085 76.801625 60)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D10 (at 0 -1.5 60) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 60) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 240) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 240) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED_SEG1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 169.416967 75.61374 72)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D8 (at 0 -1.5 72) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 72) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 252) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 252) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 /LEDs/LED_SEG0))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 170.561 79.44127 240)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D67 (at 0 -1.5 240) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 240) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 60) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 60) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED_SEG1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 160.783032 75.61374 108)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D62 (at 0 -1.5 108) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 108) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 288) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 288) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 19 /LEDs/LED_SEG11))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 163.639737 75.006529 96)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D64 (at 0 -1.5 96) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 96) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 276) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 276) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 19 /LEDs/LED_SEG11))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 162.195473 75.235278 102)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D63 (at 0 -1.5 102) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 102) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 282) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 282) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 19 /LEDs/LED_SEG11))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 159.417889 76.137769 114)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D61 (at 0 -1.5 114) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 114) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 294) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 294) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 19 /LEDs/LED_SEG11))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 158.115 76.801625 120)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D60 (at 0 -1.5 120) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 120) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 300) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 300) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 19 /LEDs/LED_SEG11))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 159.639 79.44127 300)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D77 (at 0 -1.5 300) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 300) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 120) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 120) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 19 /LEDs/LED_SEG11))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 0)
    (at 157.2768 81.6864 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D4 (at 0 1.1303 90) (layer F.SilkS))
    (fp_text value RB521S30T5G (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 166.560262 75.006529 84)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 0 -1.5 84) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 84) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 264) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 264) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 /LEDs/LED_SEG0))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 165.1 77.978 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D66 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 /LEDs/LED_SEG0))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 168.004526 75.235278 78)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 0 -1.5 78) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 78) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 258) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 258) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 /LEDs/LED_SEG0))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 165.1 74.93 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 /LEDs/LED_SEG0))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 166.751 86.36 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 1.905 0.635) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 166.751 84.836 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 1.905 0.635) (layer F.SilkS))
    (fp_text value 22u (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 160.655 82.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.032 0 90) (layer F.SilkS))
    (fp_text value 22u (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 78 "/Power Supply/+3.3V_REG_OUT"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 154.718266 79.552245 138)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D57 (at 0 -1.5 138) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 138) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 318) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 318) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 18 /LEDs/LED_SEG10))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 155.752245 78.518266 132)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D58 (at 0 -1.5 132) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 132) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 312) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 312) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 18 /LEDs/LED_SEG10))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 153.798032 80.68864 144)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D56 (at 0 -1.5 144) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 144) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 324) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 324) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 18 /LEDs/LED_SEG10))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 153.001625 81.915 150)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D55 (at 0 -1.5 150) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 150) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 330) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 330) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 18 /LEDs/LED_SEG10))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 155.64127 83.439 330)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D76 (at 0 -1.5 330) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 330) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 150) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 150) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 18 /LEDs/LED_SEG10))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 156.88864 77.598032 126)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D59 (at 0 -1.5 126) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 126) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 306) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 306) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 18 /LEDs/LED_SEG10))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 167.386 95.377 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at 2.032 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 167.767 92.456 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 0 -1.143 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 /Control/I2C_SDA))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 174.558729 94.361 150)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D70 (at 0 -1.5 150) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 150) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 330) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 330) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 12 /LEDs/LED_SEG4))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 178.386259 93.216967 342)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D23 (at 0 -1.5 342) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 342) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 162) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 162) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 11 /LEDs/LED_SEG3))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 177.198374 95.885 330)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D25 (at 0 -1.5 330) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 330) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 150) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 150) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 12 /LEDs/LED_SEG4))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 177.86223 94.58211 336)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D24 (at 0 -1.5 336) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 336) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 156) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 156) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 11 /LEDs/LED_SEG3))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 177.198374 81.915 30)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D15 (at 0 -1.5 30) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 30) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 210) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 210) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 /LEDs/LED_SEG2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 178.386259 84.583032 18)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D17 (at 0 -1.5 18) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 18) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 198) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 198) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 /LEDs/LED_SEG2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 174.558729 83.439 210)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D68 (at 0 -1.5 210) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 210) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 30) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 30) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 /LEDs/LED_SEG2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 177.86223 83.217889 24)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D16 (at 0 -1.5 24) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 24) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 204) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 204) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 /LEDs/LED_SEG2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 178.764721 85.995473 12)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D18 (at 0 -1.5 12) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 12) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 192) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 192) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 /LEDs/LED_SEG2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 176.022 88.9 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D69 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 11 /LEDs/LED_SEG3))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 178.764721 91.804526 348)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D22 (at 0 -1.5 348) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 348) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 168) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 168) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 11 /LEDs/LED_SEG3))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 178.99347 87.439737 6)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D19 (at 0 -1.5 6) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 6) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 186) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 186) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 /LEDs/LED_SEG2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 179.07 88.9)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D20 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 11 /LEDs/LED_SEG3))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 178.99347 90.360262 354)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D21 (at 0 -1.5 354) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 354) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 174) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 174) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 11 /LEDs/LED_SEG3))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 162.56 98.425 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C26 (at 1.905 1.905 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 167.64 78.232 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at -1.27 -0.254) (layer F.SilkS))
    (fp_text value 475K (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "/Power Supply/+3.3V_REG_VOUT_SET"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 162.56 80.137)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 -1.0795 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "/Power Supply/+3.3V_REG_OUT"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 176.401967 80.68864 36)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D14 (at 0 -1.5 36) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 36) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 216) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 216) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED_SEG1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 175.481733 79.552245 42)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D13 (at 0 -1.5 42) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 42) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 222) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 222) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED_SEG1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58081721)
    (at 174.447754 78.518266 48)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D12 (at 0 -1.5 48) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 48) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 228) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 228) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED_SEG1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 173.311359 77.598032 54)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D11 (at 0 -1.5 54) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 54) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 234) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 234) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED_SEG1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 155.64127 94.361 30)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D74 (at 0 -1.5 30) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5 30) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 210) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 210) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 16 /LEDs/LED_SEG8))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 157.48 87.1728)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R31 (at -1.905 -0.4318) (layer F.SilkS))
    (fp_text value 150 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /Control/LED_A4))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 157.48 88.4936)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R32 (at -1.905 -0.8636) (layer F.SilkS))
    (fp_text value 47 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /Control/LED_A5))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 154.178 88.9)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D75 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value BLUE (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /LEDs/LED_A_R5))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 17 /LEDs/LED_SEG9))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 151.81374 84.583032 162)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D53 (at 0 -1.5 162) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 162) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 342) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 342) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 17 /LEDs/LED_SEG9))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 152.337769 83.217889 156)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D54 (at 0 -1.5 156) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 156) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 336) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 336) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 17 /LEDs/LED_SEG9))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 151.206529 87.439737 174)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D51 (at 0 -1.5 174) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 174) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 354) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 354) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 17 /LEDs/LED_SEG9))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 151.13 88.9 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D50 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 17 /LEDs/LED_SEG9))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 151.435278 85.995473 168)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D52 (at 0 -1.5 168) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 168) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 348) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 348) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 17 /LEDs/LED_SEG9))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 151.435278 91.804526 192)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D48 (at 0 -1.5 192) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 192) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 12) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 1 smd rect (at -0.7493 0 12) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 16 /LEDs/LED_SEG8))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 152.337769 94.58211 204)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D46 (at 0 -1.5 204) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 204) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 24) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 1 smd rect (at -0.7493 0 24) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 16 /LEDs/LED_SEG8))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 151.81374 93.216967 198)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D47 (at 0 -1.5 198) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 198) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 18) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 1 smd rect (at -0.7493 0 18) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 16 /LEDs/LED_SEG8))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 153.001625 95.885 210)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D45 (at 0 -1.5 210) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 210) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 30) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 1 smd rect (at -0.7493 0 30) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 16 /LEDs/LED_SEG8))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 151.206529 90.360262 186)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D49 (at 0 -1.5 186) (layer F.SilkS) hide)
    (fp_text value LTST-C190KRKT (at 0 1.5 186) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 6) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /LEDs/LED_A_R4))
    (pad 1 smd rect (at -0.7493 0 6) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 16 /LEDs/LED_SEG8))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 165.1 91.186)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at 0 -0.889 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 169.037 78.232 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.143 90) (layer F.SilkS))
    (fp_text value 825K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "/Power Supply/+3.3V_REG_VRDIV"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "/Power Supply/+3.3V_REG_VOUT_SET"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 157.48 92.329)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R29 (at -1.9685 0) (layer F.SilkS))
    (fp_text value 150 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /LEDs/LED_A_R2))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /Control/LED_A2))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 157.48 89.789)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R27 (at -1.9685 0.381) (layer F.SilkS))
    (fp_text value 150 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /LEDs/LED_A_R0))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /Control/LED_A0))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 157.48 91.059)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R28 (at -1.9685 0.254) (layer F.SilkS))
    (fp_text value 150 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /LEDs/LED_A_R1))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /Control/LED_A1))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5805B3D5)
    (at 161.417 89.408 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R34 (at 1.651 0.0381 270) (layer F.SilkS))
    (fp_text value 68 (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 86 /LEDs/LED_G_R) (solder_mask_margin 0.1524))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 /LEDs/LED_G_C))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5805B3CF)
    (at 160.147 89.408 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R33 (at 1.651 -0.0127 270) (layer F.SilkS))
    (fp_text value 150 (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 85 /LEDs/LED_R_R) (solder_mask_margin 0.1524))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 88 /LEDs/LED_R_C))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 157.48 85.852)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R30 (at -1.905 0) (layer F.SilkS))
    (fp_text value 150 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED_A_R3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /Control/LED_A3))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5805B3DB)
    (at 162.687 89.1032 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R35 (at 1.7018 0.381 270) (layer F.SilkS))
    (fp_text value 68 (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 87 /LEDs/LED_B_R) (solder_mask_margin 0.1524))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 /LEDs/LED_B_C))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 162.814 93.218 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at 1.905 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 /Control/I2C_SCL))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 162.814 96.647)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C18 (at -2.159 -1.016) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 165.1 92.456)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at -1.905 -0.508) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 0)
    (at 169.799 87.503)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D1 (at -1.651 0.635 180) (layer F.SilkS))
    (fp_text value CDSU101A (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Supply/VUSB"))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC"))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 172.466 80.391)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C19 (at 1.5875 0.889 270) (layer F.SilkS))
    (fp_text value C (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 46 /Control/BTN0))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 172.212 90.678 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.0955 90) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 25 /Control/~USB_PRES))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 175.768 85.725 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at -1.778 -0.0635 90) (layer B.SilkS))
    (fp_text value 4.7u (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 22 "/Power Supply/VUSB"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 174.498 82.931 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 1.0795 180) (layer B.SilkS))
    (fp_text value 4.7u (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 21 "/Power Supply/VBAT"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer B.Cu) (tedit 55360473)
    (at 173.355 85.598 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0.5715 2.032 270) (layer B.SilkS))
    (fp_text value MCP73832 (at -0.05 -2.35 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 29 /Control/CHG_STAT))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 21 "/Power Supply/VBAT"))
    (pad 4 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 "/Power Supply/VUSB"))
    (pad 5 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 30 "/Power Supply/CHG_PROG"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 0)
    (at 169.799 85.852)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D2 (at 1.778 0.508 180) (layer F.SilkS))
    (fp_text value RB521S30T5G (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "/Power Supply/VBAT"))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC"))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 172.085 87.942 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -0.323 1.143 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Power Supply/VUSB"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5415CBB8)
    (at 174.752 98.425)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R22 (at 0 1.2065) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 47 /Control/BTN1))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(R22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5805A2B0)
    (at 171.831 91.948 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 0 1.143 270) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 71 /Control/USB_D_R+) (solder_mask_margin 0.1524))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 /Control/USB_D+) (solder_mask_margin 0.1524))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 169.7482 90.043 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0.635 1.0668 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 172.72 95.758 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C20 (at 2.032 0.0635 90) (layer F.SilkS))
    (fp_text value C (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 47 /Control/BTN1))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 174.879 96.393 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C27 (at 0 1.0795 270) (layer B.SilkS))
    (fp_text value ANY (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 72 /USB/USB_SHIELD))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5805A29A)
    (at 173.228 91.948 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 1.905 0 270) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 70 /Control/USB_D_R-) (solder_mask_margin 0.1524))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 /Control/USB_D-) (solder_mask_margin 0.1524))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5415CBB8)
    (at 176.276 95.123 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R36 (at -0.6985 1.0795 270) (layer B.SilkS))
    (fp_text value ANY (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 72 /USB/USB_SHIELD))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 172.085 83.693 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -1.143 0.889 90) (layer F.SilkS))
    (fp_text value 20K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "/Power Supply/CHG_PROG"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 173.736 88.265 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 -1.143 180) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 22 "/Power Supply/VUSB"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 172.466 81.915)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R20 (at -1.397 -0.127 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /Control/BTN0))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R20-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 161.417 92.964 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 0 1.143 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 159.004 88.138 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 0 -1.016 90) (layer B.SilkS))
    (fp_text value 8.2p (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 84 /Control/STM32_OSC32-))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 154.305 95.377 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at 0.5715 -1.0795 270) (layer B.SilkS))
    (fp_text value C (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 48 /Control/BTN2))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5415CBB8)
    (at 151.638 93.472 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R24 (at 0 1.143 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 48 /Control/BTN2))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(R24-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer B.Cu) (tedit 54130A77)
    (at 165.1 87.884)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U3 (at -4.3815 3.937) (layer B.SilkS))
    (fp_text value STM32L052x8 (at 0 -6) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -4.35 2.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -4.35 2.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -4.35 1.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 83 /Control/STM32_OSC32+))
    (pad 4 smd rect (at -4.35 1.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 84 /Control/STM32_OSC32-))
    (pad 5 smd rect (at -4.35 0.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -4.35 0.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -4.35 -0.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 /Control/STM32_RESET))
    (pad 8 smd rect (at -4.35 -0.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 -1.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 10 smd rect (at -4.35 -1.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 36 /Control/LED_A0))
    (pad 11 smd rect (at -4.35 -2.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 37 /Control/LED_A1))
    (pad 12 smd rect (at -4.35 -2.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 /Control/LED_A2))
    (pad 13 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 39 /Control/LED_A3))
    (pad 14 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 40 /Control/LED_A4))
    (pad 15 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 41 /Control/LED_A5))
    (pad 16 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 42 /Control/BUZ_OUTPUT))
    (pad 17 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U3-Pad17)"))
    (pad 18 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 25 /Control/~USB_PRES))
    (pad 19 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 29 /Control/CHG_STAT))
    (pad 20 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 44 /Control/~ACCEL_INT))
    (pad 21 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(U3-Pad21)"))
    (pad 22 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 46 /Control/BTN0))
    (pad 23 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 25 smd rect (at 4.35 -2.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 47 /Control/BTN1))
    (pad 26 smd rect (at 4.35 -2.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 48 /Control/BTN2))
    (pad 27 smd rect (at 4.35 -1.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 49 /Control/BTN3))
    (pad 28 smd rect (at 4.35 -1.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(U3-Pad28)"))
    (pad 29 smd rect (at 4.35 -0.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(U3-Pad29)"))
    (pad 30 smd rect (at 4.35 -0.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(U3-Pad30)"))
    (pad 31 smd rect (at 4.35 0.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(U3-Pad31)"))
    (pad 32 smd rect (at 4.35 0.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 70 /Control/USB_D_R-))
    (pad 33 smd rect (at 4.35 1.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 71 /Control/USB_D_R+))
    (pad 34 smd rect (at 4.35 1.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 54 /Control/SWDIO))
    (pad 35 smd rect (at 4.35 2.25) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 2.75) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 37 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 55 /Control/SWCLK))
    (pad 38 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(U3-Pad38)"))
    (pad 39 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 57 /Control/LED_C_MUX0))
    (pad 40 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 58 /Control/LED_C_MUX1))
    (pad 41 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 59 /Control/LED_C_MUX2))
    (pad 42 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 60 /Control/LED_C_MUX3))
    (pad 43 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 61 /Control/~LED_C_EN))
    (pad 44 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 45 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 /Control/I2C_SCL))
    (pad 46 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 63 /Control/I2C_SDA))
    (pad 47 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 168.3512 90.043 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at -0.381 -0.9652 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 170.688 83.693 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 159.9692 86.2584 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at -0.0254 1.0922 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 161.1884 86.2584 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 -1.1811 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 553634F8)
    (at 155.194 83.185 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0.6985 2.0955 270) (layer B.SilkS))
    (fp_text value MMBT3904 (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.00076 270) (size 0.8001 0.8001) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.95 -1.00076 270) (size 0.8001 0.8001) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 0.99822 270) (size 0.8001 0.8001) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(Q2-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 154.559 80.01 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at -1.2065 1.0795 270) (layer B.SilkS))
    (fp_text value C (at 0 -1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 49 /Control/BTN3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5415CBB8)
    (at 155.76 78.105 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R26 (at -0.0055 1.0795 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 /Control/BTN3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(R26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5415CBB8)
    (at 155.956 80.137 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at -0.508 -1.0795 270) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(Q2-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 5415CBB8)
    (at 158.496 83.312)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 0 1.143) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.8) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 42 /Control/BUZ_OUTPUT))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module simple-led-watch:1PIN_VIA (layer F.Cu) (tedit 58082089)
    (at 167.259 81.153)
    (fp_text reference REF** (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1PIN_VIA (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module simple-led-watch:SOT-666 (layer B.Cu) (tedit 580824CF)
    (at 175.133 92.075)
    (fp_text reference U5 (at 1.5875 0 270) (layer B.SilkS))
    (fp_text value USBLC6-2 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.5 -0.805) (size 0.3 0.99) (layers B.Cu B.Paste B.Mask)
      (net 74 /USB/USB_C_D-) (solder_mask_margin 0.08))
    (pad 2 smd rect (at 0 -0.805) (size 0.3 0.99) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.08))
    (pad 3 smd rect (at 0.5 -0.805) (size 0.3 0.99) (layers B.Cu B.Paste B.Mask)
      (net 75 /USB/USB_C_D+) (solder_mask_margin 0.08))
    (pad 6 smd rect (at -0.5 0.805) (size 0.3 0.99) (layers B.Cu B.Paste B.Mask)
      (net 67 /Control/USB_D-) (solder_mask_margin 0.08))
    (pad 5 smd rect (at 0 0.805) (size 0.3 0.99) (layers B.Cu B.Paste B.Mask)
      (net 22 "/Power Supply/VUSB") (solder_mask_margin 0.08))
    (pad 4 smd rect (at 0.5 0.805) (size 0.3 0.99) (layers B.Cu B.Paste B.Mask)
      (net 66 /Control/USB_D+) (solder_mask_margin 0.08))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 162.56 99.949 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C25 (at 2.032 0 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module simple-led-watch:JST-ACH-2PIN (layer B.Cu) (tedit 580AD322)
    (at 168.783 79.121 180)
    (fp_text reference P1 (at 2.159 2.667) (layer B.SilkS))
    (fp_text value BATTERY (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 4.175 0.6 180) (size 0.85 0.6) (layers B.Cu B.Paste B.Mask)
      (net 21 "/Power Supply/VBAT"))
    (pad 2 smd rect (at 4.175 -0.6 180) (size 0.85 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.4 -1.75 180) (size 0.8 0.7) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 0.4 1.75 180) (size 0.8 0.7) (layers B.Cu B.Paste B.Mask))
    (model ${KIPRJMOD}/../cad/JST-ACH.wrl
      (offset (xyz 2.158999967575074 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz -90 0 90))
    )
  )
  (module simple-led-watch:AMP-10104110-USB (layer B.Cu) (tedit 580AD32C)
    (at 180.269 88.9 270)
    (fp_text reference P3 (at -4.318 2.215) (layer B.SilkS))
    (fp_text value USB_OTG (at 0.1 6.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.3 2.85 270) (size 0.4 1.4) (layers B.Cu B.Paste B.Mask)
      (net 22 "/Power Supply/VUSB"))
    (pad 2 smd rect (at -0.65 2.85 270) (size 0.4 1.4) (layers B.Cu B.Paste B.Mask)
      (net 74 /USB/USB_C_D-))
    (pad 3 smd rect (at 0 2.85 270) (size 0.4 1.4) (layers B.Cu B.Paste B.Mask)
      (net 75 /USB/USB_C_D+))
    (pad 4 smd rect (at 0.65 2.85 270) (size 0.4 1.4) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(P3-Pad4)"))
    (pad 5 smd rect (at 1.3 2.85 270) (size 0.4 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.75 0 270) (size 2.3 1.9) (layers B.Cu B.Paste B.Mask)
      (net 72 /USB/USB_SHIELD))
    (pad 6 smd rect (at -3.75 0 270) (size 2.3 1.9) (layers B.Cu B.Paste B.Mask)
      (net 72 /USB/USB_SHIELD))
    (pad 6 smd rect (at -1.15 0 270) (size 1.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 72 /USB/USB_SHIELD))
    (pad 6 smd rect (at 1.15 0 270) (size 1.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 72 /USB/USB_SHIELD))
    (model ${KIPRJMOD}/../cad/10104110-0001LF.wrl
      (offset (xyz 0 2.539999961853027 6.730999898910523))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module simple-led-watch:PAN-EVPAV (layer B.Cu) (tedit 580AD2DA)
    (at 151.13 80.772 60)
    (fp_text reference SW4 (at -2.199705 1.27 150) (layer B.SilkS))
    (fp_text value SPST-4PIN (at 0 4.2 60) (layer B.Fab))
    (pad 1 smd rect (at -1.03 1.745 60) (size 1.14 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.03 1.745 60) (size 1.14 0.65) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at -1.175 0.65 60) (size 0.85 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.175 0.65 60) (size 0.85 0.4) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(R26-Pad2)"))
    (model ${KIPRJMOD}/../cad/EVPAV.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
  )
  (module simple-led-watch:PAN-EVPAV (layer B.Cu) (tedit 580AD2E5)
    (at 151.13 97.028 120)
    (fp_text reference SW3 (at -2.242852 1.344734 210) (layer B.SilkS))
    (fp_text value SPST-4PIN (at 0 4.2 120) (layer B.Fab))
    (pad 1 smd rect (at -1.03 1.745 120) (size 1.14 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.03 1.745 120) (size 1.14 0.65) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(R24-Pad2)"))
    (pad 2 smd rect (at -1.175 0.65 120) (size 0.85 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.175 0.65 120) (size 0.85 0.4) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(R24-Pad2)"))
    (model ${KIPRJMOD}/../cad/EVPAV.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
  )
  (module simple-led-watch:PAN-EVPAV (layer B.Cu) (tedit 580AD30A)
    (at 179.07 80.772 300)
    (fp_text reference SW1 (at 0 3 300) (layer B.SilkS))
    (fp_text value SPST-4PIN (at 0 4.2 300) (layer B.Fab))
    (pad 1 smd rect (at -1.03 1.745 300) (size 1.14 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.03 1.745 300) (size 1.14 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(R20-Pad2)"))
    (pad 2 smd rect (at -1.175 0.65 300) (size 0.85 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.175 0.65 300) (size 0.85 0.4) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(R20-Pad2)"))
    (model ${KIPRJMOD}/../cad/EVPAV.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
  )
  (module simple-led-watch:PAN-EVPAV (layer B.Cu) (tedit 580AD2FD)
    (at 179.07 97.028 240)
    (fp_text reference SW2 (at 2.242852 1.344734 330) (layer B.SilkS))
    (fp_text value SPST-4PIN (at 0 4.2 240) (layer B.Fab))
    (pad 1 smd rect (at -1.03 1.745 240) (size 1.14 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.03 1.745 240) (size 1.14 0.65) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(R22-Pad2)"))
    (pad 2 smd rect (at -1.175 0.65 240) (size 0.85 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.175 0.65 240) (size 0.85 0.4) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(R22-Pad2)"))
    (model ${KIPRJMOD}/../cad/EVPAV.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 5844F958)
    (at 158.9532 82.3976 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D3 (at 1.8034 0.4572 90) (layer F.SilkS))
    (fp_text value 3.6V (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 78 "/Power Supply/+3.3V_REG_OUT"))
  )
  (module simple-led-watch:CSS-0575A-SMT (layer B.Cu) (tedit 587AA6C6)
    (at 160.274 79.629)
    (fp_text reference SP1 (at 0 -3.175) (layer B.SilkS))
    (fp_text value CSS-0575A-SMT (at 0 3.5) (layer B.Fab))
    (pad 1 smd rect (at -1.9 -1.75) (size 2.1 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1.9 -1.75) (size 2.1 1.7) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at -1.9 1.75) (size 2.1 1.7) (layers B.Cu B.Paste B.Mask))
    (model ${KIPRJMOD}/../cad/css-0575a-smt.wrl
      (offset (xyz 0 0 0.8889999866485596))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module simple-led-watch:JST-SH-4 (layer B.Cu) (tedit 58081EEC)
    (at 168.402 97.536 270)
    (fp_text reference P2 (at 0 0.9 270) (layer B.SilkS))
    (fp_text value SWD (at 0 -1.4 270) (layer B.Fab))
    (pad 4 smd rect (at -1.5 -3.425 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 54 /Control/SWDIO))
    (pad 3 smd rect (at -0.5 -3.425 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 55 /Control/SWCLK))
    (pad 2 smd rect (at 0.5 -3.425 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 35 /Control/STM32_RESET))
    (pad 1 smd rect (at 1.5 -3.425 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad NC smd rect (at -2.8 -0.9 270) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
    (pad NC smd rect (at 2.8 -0.9 270) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
    (model ${KIPRJMOD}/../cad/JST-SH.wrl
      (offset (xyz 0 -0.8889999866485596 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module simple-led-watch:14-VQFN (layer F.Cu) (tedit 587AA7B1)
    (at 166.751 81.661 90)
    (fp_text reference U2 (at 1.778 -2.667 180) (layer F.SilkS))
    (fp_text value TPS62736 (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.795 0.75 90) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1 1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -0.5 1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 4 smd rect (at 0 1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 0.5 1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 1 1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC") (solder_mask_margin 0.07))
    (pad 7 smd rect (at 1.795 0.75 90) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 76 "/Power Supply/+3.3V_REG_VRDIV") (solder_mask_margin 0.07))
    (pad 8 smd rect (at 1.795 -0.75 90) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC") (solder_mask_margin 0.07))
    (pad 9 smd rect (at 1 -1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 77 "/Power Supply/+3.3V_REG_VOUT_SET") (solder_mask_margin 0.07))
    (pad 10 smd rect (at 0.5 -1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad10)") (solder_mask_margin 0.07))
    (pad 11 smd rect (at 0 -1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 78 "/Power Supply/+3.3V_REG_OUT") (solder_mask_margin 0.07))
    (pad 12 smd rect (at -0.5 -1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 13 smd rect (at -1 -1.795 180) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 73 "/Power Supply/+3.3V_REG_SW") (solder_mask_margin 0.07))
    (pad 14 smd rect (at -1.795 -0.75 90) (size 0.71 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 15 smd rect (at -0.5125 -0.5125 90) (size 1.025 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.08) (solder_paste_margin -0.15))
    (pad 15 smd rect (at 0.5125 -0.5125 90) (size 1.025 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.08) (solder_paste_margin -0.15))
    (pad 15 smd rect (at 0.5125 0.5125 90) (size 1.025 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.08) (solder_paste_margin -0.15))
    (pad 15 smd rect (at -0.5125 0.5125 90) (size 1.025 1.025) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.08) (solder_paste_margin -0.15))
    (pad 2 smd circle (at -1 1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 3 smd circle (at -0.5 1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 4 smd circle (at 0 1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 5 smd circle (at 0.5 1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 6 smd circle (at 1 1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC") (solder_mask_margin 0.07))
    (pad 7 smd circle (at 1.465 0.75 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 76 "/Power Supply/+3.3V_REG_VRDIV") (solder_mask_margin 0.07))
    (pad 8 smd circle (at 1.465 -0.75 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC") (solder_mask_margin 0.07))
    (pad 9 smd circle (at 1 -1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 77 "/Power Supply/+3.3V_REG_VOUT_SET") (solder_mask_margin 0.07))
    (pad 10 smd circle (at 0.5 -1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad10)") (solder_mask_margin 0.07))
    (pad 11 smd circle (at 0 -1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 78 "/Power Supply/+3.3V_REG_OUT") (solder_mask_margin 0.07))
    (pad 12 smd circle (at -0.5 -1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 13 smd circle (at -1 -1.465 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 73 "/Power Supply/+3.3V_REG_SW") (solder_mask_margin 0.07))
    (pad 14 smd circle (at -1.465 -0.75 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 1 smd circle (at -1.465 0.75 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Power Supply/+3.3V_REG_SRC") (solder_mask_margin 0.07))
  )
  (module simple-led-watch:SMD_1008 (layer F.Cu) (tedit 587AA77F)
    (at 162.941 82.534 90)
    (fp_text reference L1 (at -2.175 -0.127 90) (layer F.SilkS))
    (fp_text value 10u (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 73 "/Power Supply/+3.3V_REG_SW"))
    (pad 2 smd rect (at 1 0 90) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 78 "/Power Supply/+3.3V_REG_OUT"))
    (model ${KIPRJMOD}/../cad/SMD-1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module simple-led-watch:LED-0606 (layer F.Cu) (tedit 587AA835)
    (at 165.1 88.9 180)
    (fp_text reference D65 (at 0 1.397 180) (layer F.SilkS))
    (fp_text value APTF1616LSEEZGKQBKC (at 0 -1.6 180) (layer F.Fab))
    (pad 1 smd rect (at -0.875 0.5 180) (size 0.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /Control/LED_A0))
    (pad 2 smd rect (at 0.875 0.5 180) (size 0.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 85 /LEDs/LED_R_R))
    (pad 3 smd rect (at 0.875 -0.5 180) (size 0.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 /LEDs/LED_G_R))
    (pad 4 smd rect (at -0.875 -0.5 180) (size 0.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 87 /LEDs/LED_B_R))
    (model ${KIPRJMOD}/../cad/LED-0606.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module simple-led-watch:10-DFN (layer F.Cu) (tedit 587AA8D3)
    (at 165.1 94.742)
    (solder_mask_margin 0.2032)
    (clearance 0.1524)
    (fp_text reference U4 (at 0 1.8) (layer F.SilkS))
    (fp_text value MMA8652FC (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -0.8) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -0.9 -0.4) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 62 /Control/I2C_SCL))
    (pad 3 smd rect (at -0.9 0) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 44 /Control/~ACCEL_INT))
    (pad 4 smd rect (at -0.9 0.4) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C18-Pad1)"))
    (pad 5 smd rect (at -0.9 0.8) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at 0.9 0.8) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.9 0.4) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.9 0) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 9 smd rect (at 0.9 -0.4) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 0.9 -0.8) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 63 /Control/I2C_SDA))
  )
  (module simple-led-watch:Crystal-Abracon-ABS07 (layer B.Cu) (tedit 587AB387)
    (at 156.591 89.281 90)
    (fp_text reference Y1 (at 0 -1.778 90) (layer B.SilkS))
    (fp_text value 32.767KHz (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 83 /Control/STM32_OSC32+))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 84 /Control/STM32_OSC32-))
  )
  (module simple-led-watch:DHVQFN24 (layer B.Cu) (tedit 588CDF69)
    (at 162.052 97.409 180)
    (solder_mask_margin 0.127)
    (clearance 0.1524)
    (fp_text reference U6 (at -3.683 0 90) (layer B.SilkS))
    (fp_text value 74HC154 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2.8 -0.75 180) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 4 /LEDs/LED_SEG0))
    (pad 2 smd rect (at -2.25 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 9 /LEDs/LED_SEG1))
    (pad 3 smd rect (at -1.75 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 10 /LEDs/LED_SEG2))
    (pad 4 smd rect (at -1.25 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 11 /LEDs/LED_SEG3))
    (pad 5 smd rect (at -0.75 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 12 /LEDs/LED_SEG4))
    (pad 6 smd rect (at -0.25 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 13 /LEDs/LED_SEG5))
    (pad 7 smd rect (at 0.25 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 14 /LEDs/LED_SEG6))
    (pad 8 smd rect (at 0.75 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 15 /LEDs/LED_SEG7))
    (pad 9 smd rect (at 1.25 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 16 /LEDs/LED_SEG8))
    (pad 10 smd rect (at 1.75 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 17 /LEDs/LED_SEG9))
    (pad 11 smd rect (at 2.25 -1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 18 /LEDs/LED_SEG10))
    (pad 12 smd rect (at 2.8 -0.75 180) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 2.8 0.75 180) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 19 /LEDs/LED_SEG11))
    (pad 14 smd rect (at 2.25 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 88 /LEDs/LED_R_C))
    (pad 15 smd rect (at 1.75 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 89 /LEDs/LED_G_C))
    (pad 16 smd rect (at 1.25 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 90 /LEDs/LED_B_C))
    (pad 17 smd rect (at 0.75 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(U6-Pad17)"))
    (pad 18 smd rect (at 0.25 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -0.25 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 61 /Control/~LED_C_EN))
    (pad 20 smd rect (at -0.75 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 60 /Control/LED_C_MUX3))
    (pad 21 smd rect (at -1.25 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 59 /Control/LED_C_MUX2))
    (pad 22 smd rect (at -1.75 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 58 /Control/LED_C_MUX1))
    (pad 23 smd rect (at -2.25 1.8 90) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 57 /Control/LED_C_MUX0))
    (pad 24 smd rect (at -2.8 0.75 180) (size 0.9 0.29) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 25 smd rect (at -1 0.5 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin -0.3))
    (pad 25 smd rect (at 1 0.5 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin -0.3))
    (pad 25 smd rect (at 1 -0.5 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin -0.3))
    (pad 25 smd rect (at -1 -0.5 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin -0.3))
  )
  (gr_text "D Young" (at 170.18 95.25) (layer F.SilkS))
  (dimension 3.81 (width 0.3) (layer Dwgs.User)
    (gr_text "0.1500 in" (at 150.622 68.373) (layer Dwgs.User))
    (feature1 (pts (xy 152.527 88.9) (xy 152.527 67.023)))
    (feature2 (pts (xy 148.717 88.9) (xy 148.717 67.023)))
    (crossbar (pts (xy 148.717 69.723) (xy 152.527 69.723)))
    (arrow1a (pts (xy 152.527 69.723) (xy 151.400496 70.309421)))
    (arrow1b (pts (xy 152.527 69.723) (xy 151.400496 69.136579)))
    (arrow2a (pts (xy 148.717 69.723) (xy 149.843504 70.309421)))
    (arrow2b (pts (xy 148.717 69.723) (xy 149.843504 69.136579)))
  )
  (dimension 25.146 (width 0.3) (layer Dwgs.User)
    (gr_text "0.9900 in" (at 137.842 88.9 270) (layer Dwgs.User))
    (feature1 (pts (xy 165.1 101.473) (xy 136.492 101.473)))
    (feature2 (pts (xy 165.1 76.327) (xy 136.492 76.327)))
    (crossbar (pts (xy 139.192 76.327) (xy 139.192 101.473)))
    (arrow1a (pts (xy 139.192 101.473) (xy 138.605579 100.346496)))
    (arrow1b (pts (xy 139.192 101.473) (xy 139.778421 100.346496)))
    (arrow2a (pts (xy 139.192 76.327) (xy 138.605579 77.453504)))
    (arrow2b (pts (xy 139.192 76.327) (xy 139.778421 77.453504)))
  )
  (dimension 1.143 (width 0.3) (layer Dwgs.User)
    (gr_text "0.0450 in" (at 181.0385 74.723) (layer Dwgs.User))
    (feature1 (pts (xy 181.61 83.439) (xy 181.61 73.373)))
    (feature2 (pts (xy 180.467 83.439) (xy 180.467 73.373)))
    (crossbar (pts (xy 180.467 76.073) (xy 181.61 76.073)))
    (arrow1a (pts (xy 181.61 76.073) (xy 180.483496 76.659421)))
    (arrow1b (pts (xy 181.61 76.073) (xy 180.483496 75.486579)))
    (arrow2a (pts (xy 180.467 76.073) (xy 181.593504 76.659421)))
    (arrow2b (pts (xy 180.467 76.073) (xy 181.593504 75.486579)))
  )
  (dimension 10.922 (width 0.3) (layer Dwgs.User)
    (gr_text "0.4300 in" (at 196.803 88.9 270) (layer Dwgs.User))
    (feature1 (pts (xy 181.61 94.361) (xy 198.153 94.361)))
    (feature2 (pts (xy 181.61 83.439) (xy 198.153 83.439)))
    (crossbar (pts (xy 195.453 83.439) (xy 195.453 94.361)))
    (arrow1a (pts (xy 195.453 94.361) (xy 194.866579 93.234496)))
    (arrow1b (pts (xy 195.453 94.361) (xy 196.039421 93.234496)))
    (arrow2a (pts (xy 195.453 83.439) (xy 194.866579 84.565504)))
    (arrow2b (pts (xy 195.453 83.439) (xy 196.039421 84.565504)))
  )
  (gr_text - (at 163.957 81.661) (layer B.SilkS))
  (gr_text - (at 164.846 81.661) (layer B.SilkS))
  (gr_text - (at 163.957 80.772) (layer B.SilkS))
  (gr_text + (at 163.957 76.454) (layer B.SilkS))
  (gr_text + (at 164.846 76.454) (layer B.SilkS))
  (gr_text + (at 163.957 77.343) (layer B.SilkS))
  (gr_text "3.7V\nLi-Ion/Li-Poly" (at 172.72 78.994) (layer B.SilkS))
  (gr_text SWD (at 168.91 101.473) (layer B.SilkS))
  (gr_text "D\nC\nR\nG" (at 173.101 97.536) (layer B.SilkS))
  (gr_text "Rev. A" (at 171.196 76.454) (layer B.SilkS))
  (gr_text 2016 (at 170.942 81.788) (layer B.SilkS))
  (gr_text "LED Watch" (at 165.1635 74.7395) (layer B.SilkS))
  (gr_line (start 181.61 83.439) (end 181.61 94.361) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.1 88.9) (end 180.467 94.361) (angle 320.8724328) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.61 94.361) (end 180.467 94.361) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.467 83.439) (end 181.61 83.439) (layer Edge.Cuts) (width 0.15))
  (dimension 32.893 (width 0.3) (layer Dwgs.User)
    (gr_text "1.2950 in" (at 165.1635 115.65) (layer Dwgs.User))
    (feature1 (pts (xy 181.61 88.9) (xy 181.61 117)))
    (feature2 (pts (xy 148.717 88.9) (xy 148.717 117)))
    (crossbar (pts (xy 148.717 114.3) (xy 181.61 114.3)))
    (arrow1a (pts (xy 181.61 114.3) (xy 180.483496 114.886421)))
    (arrow1b (pts (xy 181.61 114.3) (xy 180.483496 113.713579)))
    (arrow2a (pts (xy 148.717 114.3) (xy 149.843504 114.886421)))
    (arrow2b (pts (xy 148.717 114.3) (xy 149.843504 113.713579)))
  )
  (dimension 32.766 (width 0.3) (layer Dwgs.User)
    (gr_text "1.2900 in" (at 200.867 88.9 270) (layer Dwgs.User))
    (feature1 (pts (xy 165.1 105.283) (xy 202.217 105.283)))
    (feature2 (pts (xy 165.1 72.517) (xy 202.217 72.517)))
    (crossbar (pts (xy 199.517 72.517) (xy 199.517 105.283)))
    (arrow1a (pts (xy 199.517 105.283) (xy 198.930579 104.156496)))
    (arrow1b (pts (xy 199.517 105.283) (xy 200.103421 104.156496)))
    (arrow2a (pts (xy 199.517 72.517) (xy 198.930579 73.643504)))
    (arrow2b (pts (xy 199.517 72.517) (xy 200.103421 73.643504)))
  )
  (gr_text "Notes:\n\nVias MUST be tented since we put them beneath some metal components" (at 121.92 122.047) (layer Cmts.User))
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 146.05 69.85) (xy 184.15 69.85) (xy 184.15 107.95) (xy 146.05 107.95)
      )
    )
  )
  (zone (net 2) (net_name +3V3) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 146.05 69.85) (xy 184.15 69.85) (xy 184.15 107.95) (xy 146.05 107.95)
      )
    )
  )
  (zone (net 78) (net_name "/Power Supply/+3.3V_REG_OUT") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing chamfer) (radius 0.1))
    (polygon
      (pts
        (xy 164.084 82.042) (xy 161.798 82.042) (xy 161.4805 82.296) (xy 159.766 82.296) (xy 159.5755 82.1055)
        (xy 158.369 82.1055) (xy 158.369 80.899) (xy 162.433 80.899) (xy 162.56 80.772) (xy 162.687 80.645)
        (xy 162.814 80.518) (xy 162.814 79.629) (xy 163.449 79.629) (xy 163.449 80.518) (xy 163.83 80.899)
        (xy 164.084 80.899)
      )
    )
  )
  (zone (net 2) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 162.306 80.5815) (xy 162.306 78.9305) (xy 160.909 78.9305) (xy 160.909 80.5815)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing chamfer) (radius 0.1))
    (polygon
      (pts
        (xy 161.163 82.8675) (xy 161.163 84.455) (xy 159.0675 84.455) (xy 158.369 83.7565) (xy 158.369 82.677)
        (xy 159.5755 82.677) (xy 159.766 82.8675)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.1524)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 164.465 93.599) (xy 165.735 93.599) (xy 165.735 95.758) (xy 164.465 95.758)
      )
    )
  )
)
