(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1~bpo9+1)
  (general
    (links 236)
    (no_connects 0)
    (area 112.4472 42.2722 181.251001 129.109001)
    (thickness 1.6)
    (drawings 239)
    (tracks 1995)
    (zones 0)
    (modules 46)
    (nets 94)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1778)
    (trace_clearance 0.1778)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.1778)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.4)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDD)
  (net 2 +3V3)
  (net 3 +5V)
  (net 4 SYS_5V)
  (net 5 PWR_BUT)
  (net 6 VDD_ADC)
  (net 7 GNDA_ADC)
  (net 8 "Net-(C201-Pad1)")
  (net 9 "Net-(C202-Pad1)")
  (net 10 "Net-(C203-Pad1)")
  (net 11 "Net-(C204-Pad1)")
  (net 12 "Net-(C205-Pad1)")
  (net 13 "Net-(D1-Pad2)")
  (net 14 "Net-(D1-Pad1)")
  (net 15 "Net-(D2-Pad2)")
  (net 16 "Net-(IC201-Pad2)")
  (net 17 IO0_BB)
  (net 18 IO1_BB)
  (net 19 IO2_BB)
  (net 20 IO3_BB)
  (net 21 IO4_BB)
  (net 22 IO5_BB)
  (net 23 IO6_BB)
  (net 24 IO7_BB)
  (net 25 IO7)
  (net 26 IO6)
  (net 27 IO5)
  (net 28 IO4)
  (net 29 IO3)
  (net 30 IO2)
  (net 31 IO1)
  (net 32 IO0)
  (net 33 "Net-(IC202-Pad2)")
  (net 34 IO8_BB)
  (net 35 IO9_BB)
  (net 36 IO10_BB)
  (net 37 IO11_BB)
  (net 38 IO12_BB)
  (net 39 IO13_BB)
  (net 40 IO14_BB)
  (net 41 IO15_BB)
  (net 42 IO15)
  (net 43 IO14)
  (net 44 IO13)
  (net 45 IO12)
  (net 46 IO11)
  (net 47 IO10)
  (net 48 IO9)
  (net 49 IO8)
  (net 50 "Net-(IC203-Pad2)")
  (net 51 IO16_BB)
  (net 52 IO17_BB)
  (net 53 IO18_BB)
  (net 54 IO19_BB)
  (net 55 IO20_BB)
  (net 56 IO21_BB)
  (net 57 IO22_BB)
  (net 58 IO23_BB)
  (net 59 IO23)
  (net 60 IO22)
  (net 61 IO21)
  (net 62 IO20)
  (net 63 IO19)
  (net 64 IO18)
  (net 65 IO17)
  (net 66 IO16)
  (net 67 "Net-(IC204-Pad2)")
  (net 68 IO24_BB)
  (net 69 IO25_BB)
  (net 70 IO26_BB)
  (net 71 IO27_BB)
  (net 72 IO28_BB)
  (net 73 IO29_BB)
  (net 74 IO30_BB)
  (net 75 IO31_BB)
  (net 76 IO31)
  (net 77 IO30)
  (net 78 IO29)
  (net 79 IO28)
  (net 80 IO27)
  (net 81 IO26)
  (net 82 IO25)
  (net 83 IO24)
  (net 84 "Net-(IC205-Pad2)")
  (net 85 IO32_BB)
  (net 86 IO33_BB)
  (net 87 IO33)
  (net 88 IO32)
  (net 89 GND_OR_5V)
  (net 90 SYS_RESETn)
  (net 91 CODING)
  (net 92 STATUS_LED)
  (net 93 PULLUP_REF)
  (net_class Default "To jest domyślna klasa połączeń."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CODING)
    (add_net GNDA_ADC)
    (add_net IO0)
    (add_net IO0_BB)
    (add_net IO1)
    (add_net IO10)
    (add_net IO10_BB)
    (add_net IO11)
    (add_net IO11_BB)
    (add_net IO12)
    (add_net IO12_BB)
    (add_net IO13)
    (add_net IO13_BB)
    (add_net IO14)
    (add_net IO14_BB)
    (add_net IO15)
    (add_net IO15_BB)
    (add_net IO16)
    (add_net IO16_BB)
    (add_net IO17)
    (add_net IO17_BB)
    (add_net IO18)
    (add_net IO18_BB)
    (add_net IO19)
    (add_net IO19_BB)
    (add_net IO1_BB)
    (add_net IO2)
    (add_net IO20)
    (add_net IO20_BB)
    (add_net IO21)
    (add_net IO21_BB)
    (add_net IO22)
    (add_net IO22_BB)
    (add_net IO23)
    (add_net IO23_BB)
    (add_net IO24)
    (add_net IO24_BB)
    (add_net IO25)
    (add_net IO25_BB)
    (add_net IO26)
    (add_net IO26_BB)
    (add_net IO27)
    (add_net IO27_BB)
    (add_net IO28)
    (add_net IO28_BB)
    (add_net IO29)
    (add_net IO29_BB)
    (add_net IO2_BB)
    (add_net IO3)
    (add_net IO30)
    (add_net IO30_BB)
    (add_net IO31)
    (add_net IO31_BB)
    (add_net IO32)
    (add_net IO32_BB)
    (add_net IO33)
    (add_net IO33_BB)
    (add_net IO3_BB)
    (add_net IO4)
    (add_net IO4_BB)
    (add_net IO5)
    (add_net IO5_BB)
    (add_net IO6)
    (add_net IO6_BB)
    (add_net IO7)
    (add_net IO7_BB)
    (add_net IO8)
    (add_net IO8_BB)
    (add_net IO9)
    (add_net IO9_BB)
    (add_net "Net-(C201-Pad1)")
    (add_net "Net-(C202-Pad1)")
    (add_net "Net-(C203-Pad1)")
    (add_net "Net-(C204-Pad1)")
    (add_net "Net-(C205-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(IC201-Pad2)")
    (add_net "Net-(IC202-Pad2)")
    (add_net "Net-(IC203-Pad2)")
    (add_net "Net-(IC204-Pad2)")
    (add_net "Net-(IC205-Pad2)")
    (add_net PULLUP_REF)
    (add_net PWR_BUT)
    (add_net STATUS_LED)
    (add_net SYS_RESETn)
    (add_net VDD_ADC)
  )
  (net_class Big ""
    (clearance 0.1778)
    (trace_width 0.3048)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Output ""
    (clearance 0.1778)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.1778)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GNDD)
    (add_net GND_OR_5V)
    (add_net SYS_5V)
  )
  (module footprint:IDC26 (layer F.Cu) (tedit 5A986CA7)
    (at 141.55 76.7 90)
    (descr "surface-mounted straight pin header, 2x13, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x13 2.54mm double row")
    (attr smd)
    (fp_text reference P101 (at 5.6 -18.5 180) (layer F.SilkS))
    (fp_text value IDC26 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.25 -15.24 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 32 IO0))
    (pad 2 smd rect (at 3.25 -15.24 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 31 IO1))
    (pad 3 smd rect (at -3.25 -12.7 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 30 IO2))
    (pad 4 smd rect (at 3.25 -12.7 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 29 IO3))
    (pad 5 smd rect (at -3.25 -10.16 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 28 IO4))
    (pad 6 smd rect (at 3.25 -10.16 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 27 IO5))
    (pad 7 smd rect (at -3.25 -7.62 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 26 IO6))
    (pad 8 smd rect (at 3.25 -7.62 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 25 IO7))
    (pad 9 smd rect (at -3.25 -5.08 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 49 IO8))
    (pad 10 smd rect (at 3.25 -5.08 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 11 smd rect (at -3.25 -2.54 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 48 IO9))
    (pad 12 smd rect (at 3.25 -2.54 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 13 smd rect (at -3.25 0 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 47 IO10))
    (pad 14 smd rect (at 3.25 0 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 15 smd rect (at -3.25 2.54 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 46 IO11))
    (pad 16 smd rect (at 3.25 2.54 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 17 smd rect (at -3.25 5.08 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 45 IO12))
    (pad 18 smd rect (at 3.25 5.08 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (pad 19 smd rect (at -3.25 7.62 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 44 IO13))
    (pad 20 smd rect (at 3.25 7.62 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (pad 21 smd rect (at -3.25 10.16 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 43 IO14))
    (pad 22 smd rect (at 3.25 10.16 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (pad 23 smd rect (at -3.25 12.7 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 42 IO15))
    (pad 24 smd rect (at 3.25 12.7 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (pad 25 smd rect (at -3.25 15.24 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 66 IO16))
    (pad 26 smd rect (at 3.25 15.24 90) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x13_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AAE8FCD)
    (at 123.25 125.25)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R211 (at 0 1.75) (layer F.SilkS))
    (fp_text value 200k (at -3.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 VDD_ADC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 91 CODING))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A5A51C9)
    (at 123.85 89.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C201 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C201-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A5A6800)
    (at 138.3 89.95 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C202 (at 0 -1.6 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at -0.05 0.05 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C202-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A5A51EA)
    (at 160.4 102 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C203 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C203-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A5A5200)
    (at 146.7 101.9 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C204 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C204-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A5A5212)
    (at 132.25 101.85 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C205 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at -0.05 0.05 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C205-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5AAE7E8A)
    (at 160.5 59.4 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0.8 -1.7 180) (layer F.SilkS))
    (fp_text value Yellow (at -1 1.7 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5AAE7E15)
    (at 160.5 51.9 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -3.1 1 180) (layer F.SilkS))
    (fp_text value Green (at -0.6 -1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module GTL2003PW:SOP65P640X110-20N (layer F.Cu) (tedit 5A5A60EE)
    (at 130.55 89.2 90)
    (descr "NXP TSSOP20 SOT360-1")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC201 (at -0.5 4.5 90) (layer F.SilkS))
    (fp_text value GTL2003PW (at -0.05 4.7 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.938 -2.925 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -2.938 -2.275 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC201-Pad2)"))
    (pad 3 smd rect (at -2.938 -1.625 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 17 IO0_BB))
    (pad 4 smd rect (at -2.938 -0.975 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 18 IO1_BB))
    (pad 5 smd rect (at -2.938 -0.325 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 19 IO2_BB))
    (pad 6 smd rect (at -2.938 0.325 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 20 IO3_BB))
    (pad 7 smd rect (at -2.938 0.975 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 21 IO4_BB))
    (pad 8 smd rect (at -2.938 1.625 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 22 IO5_BB))
    (pad 9 smd rect (at -2.938 2.275 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 23 IO6_BB))
    (pad 10 smd rect (at -2.938 2.925 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 24 IO7_BB))
    (pad 11 smd rect (at 2.938 2.925 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 25 IO7))
    (pad 12 smd rect (at 2.938 2.275 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 26 IO6))
    (pad 13 smd rect (at 2.938 1.625 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 27 IO5))
    (pad 14 smd rect (at 2.938 0.975 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 28 IO4))
    (pad 15 smd rect (at 2.938 0.325 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 29 IO3))
    (pad 16 smd rect (at 2.938 -0.325 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 30 IO2))
    (pad 17 smd rect (at 2.938 -0.975 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 31 IO1))
    (pad 18 smd rect (at 2.938 -1.625 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 32 IO0))
    (pad 19 smd rect (at 2.938 -2.275 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C201-Pad1)"))
    (pad 20 smd rect (at 2.938 -2.925 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C201-Pad1)"))
  )
  (module GTL2003PW:SOP65P640X110-20N (layer F.Cu) (tedit 5AAE95CB)
    (at 144.95 89.2 90)
    (descr "NXP TSSOP20 SOT360-1")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC202 (at -4.8 0.3 180) (layer F.SilkS))
    (fp_text value GTL2003PW (at 0 4.7 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.938 -2.925 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -2.938 -2.275 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC202-Pad2)"))
    (pad 3 smd rect (at -2.938 -1.625 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 34 IO8_BB))
    (pad 4 smd rect (at -2.938 -0.975 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 35 IO9_BB))
    (pad 5 smd rect (at -2.938 -0.325 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 36 IO10_BB))
    (pad 6 smd rect (at -2.938 0.325 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 37 IO11_BB))
    (pad 7 smd rect (at -2.938 0.975 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 38 IO12_BB))
    (pad 8 smd rect (at -2.938 1.625 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 39 IO13_BB))
    (pad 9 smd rect (at -2.938 2.275 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 40 IO14_BB))
    (pad 10 smd rect (at -2.938 2.925 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 41 IO15_BB))
    (pad 11 smd rect (at 2.938 2.925 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 42 IO15))
    (pad 12 smd rect (at 2.938 2.275 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 43 IO14))
    (pad 13 smd rect (at 2.938 1.625 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 44 IO13))
    (pad 14 smd rect (at 2.938 0.975 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 45 IO12))
    (pad 15 smd rect (at 2.938 0.325 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 46 IO11))
    (pad 16 smd rect (at 2.938 -0.325 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 47 IO10))
    (pad 17 smd rect (at 2.938 -0.975 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 48 IO9))
    (pad 18 smd rect (at 2.938 -1.625 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 49 IO8))
    (pad 19 smd rect (at 2.938 -2.275 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C202-Pad1)"))
    (pad 20 smd rect (at 2.938 -2.925 180) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C202-Pad1)"))
  )
  (module GTL2003PW:SOP65P640X110-20N (layer F.Cu) (tedit 5AAE963C)
    (at 154.1 102.5 270)
    (descr "NXP TSSOP20 SOT360-1")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC203 (at -1.25 4.35 270) (layer F.SilkS))
    (fp_text value GTL2003PW (at -0.3 4.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.938 -2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -2.938 -2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(IC203-Pad2)"))
    (pad 3 smd rect (at -2.938 -1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 51 IO16_BB))
    (pad 4 smd rect (at -2.938 -0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 52 IO17_BB))
    (pad 5 smd rect (at -2.938 -0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 53 IO18_BB))
    (pad 6 smd rect (at -2.938 0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 54 IO19_BB))
    (pad 7 smd rect (at -2.938 0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 55 IO20_BB))
    (pad 8 smd rect (at -2.938 1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 56 IO21_BB))
    (pad 9 smd rect (at -2.938 2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 57 IO22_BB))
    (pad 10 smd rect (at -2.938 2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 58 IO23_BB))
    (pad 11 smd rect (at 2.938 2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 59 IO23))
    (pad 12 smd rect (at 2.938 2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 60 IO22))
    (pad 13 smd rect (at 2.938 1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 61 IO21))
    (pad 14 smd rect (at 2.938 0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 62 IO20))
    (pad 15 smd rect (at 2.938 0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 63 IO19))
    (pad 16 smd rect (at 2.938 -0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 64 IO18))
    (pad 17 smd rect (at 2.938 -0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 65 IO17))
    (pad 18 smd rect (at 2.938 -1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 66 IO16))
    (pad 19 smd rect (at 2.938 -2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C203-Pad1)"))
    (pad 20 smd rect (at 2.938 -2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C203-Pad1)"))
  )
  (module GTL2003PW:SOP65P640X110-20N (layer F.Cu) (tedit 5A5A608E)
    (at 140.3 102.5 270)
    (descr "NXP TSSOP20 SOT360-1")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC204 (at -0.1 4.3 270) (layer F.SilkS))
    (fp_text value GTL2003PW (at -0.2 4.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.938 -2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -2.938 -2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(IC204-Pad2)"))
    (pad 3 smd rect (at -2.938 -1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 68 IO24_BB))
    (pad 4 smd rect (at -2.938 -0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 69 IO25_BB))
    (pad 5 smd rect (at -2.938 -0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 70 IO26_BB))
    (pad 6 smd rect (at -2.938 0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 71 IO27_BB))
    (pad 7 smd rect (at -2.938 0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 72 IO28_BB))
    (pad 8 smd rect (at -2.938 1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 73 IO29_BB))
    (pad 9 smd rect (at -2.938 2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 74 IO30_BB))
    (pad 10 smd rect (at -2.938 2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 75 IO31_BB))
    (pad 11 smd rect (at 2.938 2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 76 IO31))
    (pad 12 smd rect (at 2.938 2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 77 IO30))
    (pad 13 smd rect (at 2.938 1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 78 IO29))
    (pad 14 smd rect (at 2.938 0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 79 IO28))
    (pad 15 smd rect (at 2.938 0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 80 IO27))
    (pad 16 smd rect (at 2.938 -0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 81 IO26))
    (pad 17 smd rect (at 2.938 -0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 82 IO25))
    (pad 18 smd rect (at 2.938 -1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 83 IO24))
    (pad 19 smd rect (at 2.938 -2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C204-Pad1)"))
    (pad 20 smd rect (at 2.938 -2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C204-Pad1)"))
  )
  (module GTL2003PW:SOP65P640X110-20N (layer F.Cu) (tedit 5A5A6084)
    (at 126.3 102.5 270)
    (descr "NXP TSSOP20 SOT360-1")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC205 (at -0.1 4.3 270) (layer F.SilkS))
    (fp_text value GTL2003PW (at -0.25 4.85 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.938 -2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -2.938 -2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(IC205-Pad2)"))
    (pad 3 smd rect (at -2.938 -1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 85 IO32_BB))
    (pad 4 smd rect (at -2.938 -0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 86 IO33_BB))
    (pad 5 smd rect (at -2.938 -0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.938 0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.938 0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -2.938 1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -2.938 2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2.938 2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 2.938 2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.938 2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.938 1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.938 0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.938 0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.938 -0.325) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 2.938 -0.975) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 87 IO33))
    (pad 18 smd rect (at 2.938 -1.625) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 88 IO32))
    (pad 19 smd rect (at 2.938 -2.275) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C205-Pad1)"))
    (pad 20 smd rect (at 2.938 -2.925) (size 0.45 1.475) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C205-Pad1)"))
  )
  (module M20-8760342:M20-8760342 (layer F.Cu) (tedit 5A5A6899)
    (at 156 90.25 180)
    (descr M20-8760342)
    (tags Connector)
    (attr smd)
    (fp_text reference JP101 (at -4.9 0 270) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual_Double_Header (at -0.2 5.5 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.54 2.9 180) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
    (pad 2 smd rect (at -2.54 -2.9 180) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
    (pad 3 smd rect (at 0 2.9 180) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (pad 4 smd rect (at 0 -2.9 180) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 2.54 2.9 180) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 6 smd rect (at 2.54 -2.9 180) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
  )
  (module Pin_Headers:Pin_Header_Straight_2x23_Pitch2.54mm (layer F.Cu) (tedit 5A5A65DA)
    (at 116.37 62.38)
    (descr "Through hole straight pin header, 2x23, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x23 2.54mm double row")
    (fp_text reference P102 (at 1.53 58.62) (layer F.SilkS))
    (fp_text value BeagleBone_Black_Header (at -2.97 47.82 90) (layer F.Fab))
    (fp_text user %R (at 1.27 27.94 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SYS_5V))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SYS_5V))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 PWR_BUT))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 SYS_RESETn))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 IO7_BB))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 IO28_BB))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 IO10_BB))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 IO19_BB))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 IO21_BB))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 IO29_BB))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 IO13_BB))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 IO3_BB))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 IO11_BB))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 IO12_BB))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 IO17_BB))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 IO30_BB))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 IO9_BB))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 IO1_BB))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 IO31_BB))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 IO32_BB))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 IO33_BB))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 IO18_BB))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 IO20_BB))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 VDD_ADC))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GNDA_ADC))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 CODING))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 IO16_BB))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 IO5_BB))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x23_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x23_Pitch2.54mm (layer F.Cu) (tedit 5A5A65D1)
    (at 164.64 62.38)
    (descr "Through hole straight pin header, 2x23, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x23 2.54mm double row")
    (fp_text reference P103 (at 0.76 58.62) (layer F.SilkS))
    (fp_text value BeagleBone_Black_Header (at 5.56 47.82 270) (layer F.Fab))
    (fp_text user %R (at 1.27 27.94 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 IO14_BB))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 IO22_BB))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 IO24_BB))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 IO23_BB))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 IO2_BB))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 IO4_BB))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 IO0_BB))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 IO25_BB))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 IO6_BB))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 IO8_BB))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 IO26_BB))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 IO27_BB))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 IO15_BB))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 STATUS_LED))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x23_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module M20-8760342:M20-8760342 (layer F.Cu) (tedit 5AAE92DC)
    (at 129 61 90)
    (descr M20-8760342)
    (tags Connector)
    (attr smd)
    (fp_text reference P105 (at 4.5 0.25 180) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at -0.5 5.6 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.54 2.9 90) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -2.54 -2.9 90) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 5 PWR_BUT))
    (pad 3 smd rect (at 0 2.9 90) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 4 smd rect (at 0 -2.9 90) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 90 SYS_RESETn))
    (pad 5 smd rect (at 2.54 2.9 90) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 6 smd rect (at 2.54 -2.9 90) (size 1.27 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AAE9277)
    (at 155.7 59.8)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R101 (at 0.05 1.7) (layer F.SilkS))
    (fp_text value 330 (at -0.2 -1.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AAE9254)
    (at 155.7 52.1)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R102 (at 0.05 1.65) (layer F.SilkS))
    (fp_text value 330 (at 0.05 -1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A5A6818)
    (at 123.85 94.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R201 (at 0.1 1.6 90) (layer F.SilkS))
    (fp_text value 10k (at 0.2 -1.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC201-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AAE9181)
    (at 123.85 85.3 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R202 (at -0.05 1.6 270) (layer F.SilkS))
    (fp_text value 200k (at 0.2 -1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C201-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A5A6808)
    (at 138.3 94.15 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 1.6 90) (layer F.SilkS))
    (fp_text value 10k (at 0 -1.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC202-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AAE91E2)
    (at 138.4 85.35 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R204 (at 0.65 1.65 270) (layer F.SilkS))
    (fp_text value 200k (at 0.65 -1.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C202-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AAE94DC)
    (at 160.4 97.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R205 (at 0 -1.6 270) (layer F.SilkS))
    (fp_text value 10k (at 1 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(IC203-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 160.6 106.2 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R206 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 200k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C203-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A5A6859)
    (at 146.7 97.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R207 (at -0.1 1.5 270) (layer F.SilkS))
    (fp_text value 10k (at 0.1 -1.7 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(IC204-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AAE8EF4)
    (at 146.7 106.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R208 (at 0.6 1.8 90) (layer F.SilkS))
    (fp_text value 200k (at 0.6 -1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C204-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A5A6852)
    (at 132.2 97.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R209 (at 0 1.6 270) (layer F.SilkS))
    (fp_text value 10k (at 0 -1.7 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(IC205-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AAE8DEA)
    (at 132.2 106.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R210 (at 0.35 -1.7 90) (layer F.SilkS))
    (fp_text value 200k (at 0.35 1.8 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SYS_5V))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C205-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AAE8820)
    (at 123.25 121.5 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R212 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 91 CODING))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDA_ADC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:CAT_CAY16 (layer F.Cu) (tedit 5AAE87BA)
    (at 127.5 67.5 180)
    (fp_text reference RN201 (at -2.5 0.25 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 2 smd rect (at -0.4 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 3 smd rect (at 0.4 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 4 smd rect (at 1.2 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 1.2 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 IO0))
    (pad 6 smd rect (at 0.4 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 IO1))
    (pad 7 smd rect (at -0.4 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 IO2))
    (pad 8 smd rect (at -1.2 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 IO3))
  )
  (module footprint:CAT_CAY16 (layer F.Cu) (tedit 5AAE9133)
    (at 140.75 67.5 180)
    (fp_text reference RN202 (at 0 2.25 360) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 2 smd rect (at -0.4 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 3 smd rect (at 0.4 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 4 smd rect (at 1.2 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 1.2 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 IO8))
    (pad 6 smd rect (at 0.4 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 IO9))
    (pad 7 smd rect (at -0.4 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 IO10))
    (pad 8 smd rect (at -1.2 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 IO11))
  )
  (module footprint:CAT_CAY16 (layer F.Cu) (tedit 5AAE8FF1)
    (at 156.5 123.75)
    (fp_text reference RN203 (at 2.5 -0.75 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 2 smd rect (at -0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 3 smd rect (at 0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 4 smd rect (at 1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 IO16))
    (pad 6 smd rect (at 0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 IO17))
    (pad 7 smd rect (at -0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 IO18))
    (pad 8 smd rect (at -1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 IO19))
  )
  (module footprint:CAT_CAY16 (layer F.Cu) (tedit 5AAE87BD)
    (at 132.5 67.5 180)
    (fp_text reference RN204 (at -2.75 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 2 smd rect (at -0.4 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 3 smd rect (at 0.4 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 4 smd rect (at 1.2 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 1.2 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 IO4))
    (pad 6 smd rect (at 0.4 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 IO5))
    (pad 7 smd rect (at -0.4 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 IO6))
    (pad 8 smd rect (at -1.2 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 IO7))
  )
  (module footprint:CAT_CAY16 (layer F.Cu) (tedit 5AAE9131)
    (at 150.25 67.5 180)
    (fp_text reference RN205 (at 0 2.25 360) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 2 smd rect (at -0.4 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 3 smd rect (at 0.4 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 4 smd rect (at 1.2 0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 1.2 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 IO12))
    (pad 6 smd rect (at 0.4 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 IO13))
    (pad 7 smd rect (at -0.4 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 IO14))
    (pad 8 smd rect (at -1.2 -0.85 180) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 IO15))
  )
  (module footprint:CAT_CAY16 (layer F.Cu) (tedit 5AAE8F38)
    (at 149.5 123.75)
    (fp_text reference RN206 (at -2.5 -0.25 90) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 2 smd rect (at -0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 3 smd rect (at 0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 4 smd rect (at 1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 IO20))
    (pad 6 smd rect (at 0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 IO21))
    (pad 7 smd rect (at -0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 IO22))
    (pad 8 smd rect (at -1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 IO23))
  )
  (module footprint:CAT_CAY16 (layer F.Cu) (tedit 5AAE8F2B)
    (at 135 123.75)
    (fp_text reference RN207 (at 0 -2.25) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 2 smd rect (at -0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 3 smd rect (at 0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 4 smd rect (at 1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 IO28))
    (pad 6 smd rect (at 0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 IO29))
    (pad 7 smd rect (at -0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 IO30))
    (pad 8 smd rect (at -1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 IO31))
  )
  (module footprint:CAT_CAY16 (layer F.Cu) (tedit 5AAE8B8A)
    (at 142.5 123.75)
    (fp_text reference RN208 (at 0 -2.25) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 2 smd rect (at -0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 3 smd rect (at 0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 4 smd rect (at 1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 IO24))
    (pad 6 smd rect (at 0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 IO25))
    (pad 7 smd rect (at -0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 IO26))
    (pad 8 smd rect (at -1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 IO27))
  )
  (module footprint:CAT_CAY16 (layer F.Cu) (tedit 5AAE8F1C)
    (at 128.75 123.75)
    (fp_text reference RN209 (at -0.25 -2.25) (layer F.SilkS))
    (fp_text value 10k (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 2 smd rect (at -0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 3 smd rect (at 0.4 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 4 smd rect (at 1.2 0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 PULLUP_REF))
    (pad 5 smd rect (at 1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.4 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 IO32))
    (pad 8 smd rect (at -1.2 -0.85) (size 0.45 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 IO33))
  )
  (module footprint:PTS645_SMT (layer F.Cu) (tedit 5A5A6893)
    (at 120.8 50.8 90)
    (descr "PTS645(SMT)")
    (tags Switch)
    (attr smd)
    (fp_text reference SW101 (at -0.1 -4 90) (layer F.SilkS))
    (fp_text value SW_Push (at -0.1 4.5 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.975 -2.25 180) (size 1.3 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 1 smd rect (at 3.975 -2.25 180) (size 1.3 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -3.975 2.25 180) (size 1.3 1.55) (layers F.Cu F.Paste F.Mask)
      (net 5 PWR_BUT))
    (pad 2 smd rect (at 3.975 2.25 180) (size 1.3 1.55) (layers F.Cu F.Paste F.Mask)
      (net 5 PWR_BUT))
  )
  (module footprint:PTS645_SMT (layer F.Cu) (tedit 5A5A6895)
    (at 129.75 51 270)
    (descr "PTS645(SMT)")
    (tags Switch)
    (attr smd)
    (fp_text reference SW102 (at 0 -4 270) (layer F.SilkS))
    (fp_text value SW_Push (at -0.1 4.5 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.975 -2.25) (size 1.3 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 1 smd rect (at 3.975 -2.25) (size 1.3 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -3.975 2.25) (size 1.3 1.55) (layers F.Cu F.Paste F.Mask)
      (net 90 SYS_RESETn))
    (pad 2 smd rect (at 3.975 2.25) (size 1.3 1.55) (layers F.Cu F.Paste F.Mask)
      (net 90 SYS_RESETn))
  )
  (module footprint:515-1114F_2 (layer F.Cu) (tedit 5AAE927D)
    (at 162 42.7 180)
    (descr 515-1114F)
    (tags "Undefined or Miscellaneous")
    (fp_text reference Z106 (at 3.75 -13.8 450) (layer F.SilkS))
    (fp_text value Light_Pipe_2_LED (at 7.4 -11.3 270) (layer F.SilkS) hide)
    (pad 15 thru_hole circle (at -0.765 -14.2 270) (size 1.57 1.57) (drill 1.57) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at -0.765 -11.66 270) (size 1.57 1.57) (drill 1.57) (layers *.Cu *.Mask F.SilkS))
  )
  (module footprint:OSHW (layer F.Cu) (tedit 0)
    (at 158.25 66.25)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module footprint:IDC26 (layer F.Cu) (tedit 5AAE8BA7)
    (at 141.8 114.8 270)
    (descr "surface-mounted straight pin header, 2x13, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x13 2.54mm double row")
    (attr smd)
    (fp_text reference P104 (at -5.55 -18.45 360) (layer F.SilkS))
    (fp_text value IDC26 (at 0 17.57 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -3.25 -15.24 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 65 IO17))
    (pad 2 smd rect (at 3.25 -15.24 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 64 IO18))
    (pad 3 smd rect (at -3.25 -12.7 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 63 IO19))
    (pad 4 smd rect (at 3.25 -12.7 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 62 IO20))
    (pad 5 smd rect (at -3.25 -10.16 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 61 IO21))
    (pad 6 smd rect (at 3.25 -10.16 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 60 IO22))
    (pad 7 smd rect (at -3.25 -7.62 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 59 IO23))
    (pad 8 smd rect (at 3.25 -7.62 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 83 IO24))
    (pad 9 smd rect (at -3.25 -5.08 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 82 IO25))
    (pad 10 smd rect (at 3.25 -5.08 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 11 smd rect (at -3.25 -2.54 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 81 IO26))
    (pad 12 smd rect (at 3.25 -2.54 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 13 smd rect (at -3.25 0 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 80 IO27))
    (pad 14 smd rect (at 3.25 0 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 15 smd rect (at -3.25 2.54 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 79 IO28))
    (pad 16 smd rect (at 3.25 2.54 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 17 smd rect (at -3.25 5.08 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 78 IO29))
    (pad 18 smd rect (at 3.25 5.08 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (pad 19 smd rect (at -3.25 7.62 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 77 IO30))
    (pad 20 smd rect (at 3.25 7.62 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (pad 21 smd rect (at -3.25 10.16 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 76 IO31))
    (pad 22 smd rect (at 3.25 10.16 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (pad 23 smd rect (at -3.25 12.7 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 88 IO32))
    (pad 24 smd rect (at 3.25 12.7 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (pad 25 smd rect (at -3.25 15.24 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 87 IO33))
    (pad 26 smd rect (at 3.25 15.24 270) (size 4.8 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 GND_OR_5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x13_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:SOT95P240X105-3N (layer F.Cu) (tedit 5AAE7C32)
    (at 166 55.4 180)
    (descr SOT95P240X105-3N)
    (tags "Undefined or Miscellaneous")
    (attr smd)
    (fp_text reference Q101 (at -0.4 2.4 360) (layer F.SilkS))
    (fp_text value 2N7002K (at -3.2 3.05 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.016 -0.9652 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 92 STATUS_LED))
    (pad 3 smd rect (at -1.016 0.9652 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at 1.016 0 270) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad1)"))
  )
  (gr_text PWR (at 121 45) (layer F.SilkS))
  (gr_text RST (at 129.75 45) (layer F.SilkS))
  (gr_text PU (at 150.5 93) (layer F.SilkS))
  (gr_text OUT (at 150.5 87.25) (layer F.SilkS))
  (gr_text 5V (at 158.75 85) (layer F.SilkS))
  (gr_text GND (at 152.5 85) (layer F.SilkS))
  (gr_text 5V (at 158.5 95.75 90) (layer F.SilkS))
  (gr_text 3V3 (at 153.5 96.25 90) (layer F.SilkS))
  (gr_text GND (at 134 61.25 90) (layer F.SilkS))
  (gr_text PWR (at 122.75 63.5) (layer F.SilkS))
  (gr_text RST (at 122.75 61) (layer F.SilkS))
  (gr_text 5V (at 123.25 58.5) (layer F.SilkS))
  (gr_text 25 (at 156.75 83.25) (layer F.SilkS))
  (gr_text 23 (at 154.25 83.25) (layer F.SilkS))
  (gr_text 21 (at 151.75 83.25) (layer F.SilkS))
  (gr_text 19 (at 149 83.25) (layer F.SilkS))
  (gr_text 17 (at 146.5 83.25) (layer F.SilkS))
  (gr_text 15 (at 144 84) (layer F.SilkS))
  (gr_text 13 (at 141.5 84) (layer F.SilkS))
  (gr_text 11 (at 138.25 83.25) (layer F.SilkS))
  (gr_text 9 (at 136.25 83.25) (layer F.SilkS))
  (gr_text 7 (at 133.75 83.25) (layer F.SilkS))
  (gr_text 5 (at 131.25 83.25) (layer F.SilkS))
  (gr_text 3 (at 128.75 83.25) (layer F.SilkS))
  (gr_text 1 (at 126.25 83.25) (layer F.SilkS))
  (gr_text 26 (at 158 70.25) (layer F.SilkS))
  (gr_text 24 (at 154 70.25) (layer F.SilkS))
  (gr_text 22 (at 151.5 70.25) (layer F.SilkS))
  (gr_text 20 (at 149 70.25) (layer F.SilkS))
  (gr_text 18 (at 146.5 70.25) (layer F.SilkS))
  (gr_text 16 (at 144 70.25) (layer F.SilkS))
  (gr_text 14 (at 141.5 70.25) (layer F.SilkS))
  (gr_text 12 (at 139 70.25) (layer F.SilkS))
  (gr_text 10 (at 136.5 70.25) (layer F.SilkS))
  (gr_text 8 (at 133.75 70.25) (layer F.SilkS))
  (gr_text 6 (at 131.25 70.25) (layer F.SilkS))
  (gr_text 4 (at 128.75 70.25) (layer F.SilkS))
  (gr_text 2 (at 126.25 70.25) (layer F.SilkS))
  (gr_text 20 (at 154.5 121.5) (layer F.SilkS))
  (gr_text 22 (at 152 121.5) (layer F.SilkS))
  (gr_text 24 (at 149.5 121.5) (layer F.SilkS))
  (gr_text 18 (at 157 121.5) (layer F.SilkS))
  (gr_text 17 (at 157 108.25) (layer F.SilkS))
  (gr_text 19 (at 154.5 108.25) (layer F.SilkS))
  (gr_text 21 (at 152 108.25) (layer F.SilkS))
  (gr_text 23 (at 149.5 108.25) (layer F.SilkS))
  (gr_text 25 (at 146.75 108.25) (layer F.SilkS))
  (gr_text 26 (at 144.25 107.5) (layer F.SilkS))
  (gr_text 27 (at 141.75 107.5) (layer F.SilkS))
  (gr_text 28 (at 139.25 107.5) (layer F.SilkS))
  (gr_text 29 (at 136.75 108.25) (layer F.SilkS))
  (gr_text 30 (at 134 108.25) (layer F.SilkS))
  (gr_text 31 (at 131.5 108.25) (layer F.SilkS))
  (gr_text 32 (at 129 108.25) (layer F.SilkS))
  (gr_text 33 (at 126.5 108.25) (layer F.SilkS))
  (gr_text "Rev 1.1" (at 162.25 125.25 30) (layer F.SilkS))
  (gr_text "Parallel Cape by Alexander Rössler" (at 142 126.75) (layer F.SilkS))
  (gr_line (start 135.419 42.6987) (end 120.815 42.6987) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2874) (end 135.419 42.6987) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2875) (end 135.419 64.2874) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2876) (end 135.419 64.2875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2877) (end 135.419 64.2876) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2878) (end 135.419 64.2877) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2879) (end 135.419 64.2878) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.288) (end 135.419 64.2879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2881) (end 135.419 64.288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2882) (end 135.419 64.2881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2883) (end 135.419 64.2882) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2884) (end 135.419 64.2883) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2884) (end 135.419 64.2884) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.419 64.2885) (end 135.419 64.2884) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 64.2885) (end 135.419 64.2885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 64.2886) (end 135.42 64.2885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 64.2886) (end 135.42 64.2886) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 64.2887) (end 135.42 64.2886) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 64.2887) (end 135.42 64.2887) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 64.2887) (end 135.42 64.2887) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.2 64.2887) (end 135.42 64.2887) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.2 82.7887) (end 181.2 82.7887) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.2 82.7887) (end 181.2 82.7887) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.2 82.7886) (end 181.2 82.7887) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7886) (end 181.2 82.7886) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7885) (end 181.201 82.7886) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7885) (end 181.201 82.7885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7884) (end 181.201 82.7885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7884) (end 181.201 82.7884) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7883) (end 181.201 82.7884) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7882) (end 181.201 82.7883) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7881) (end 181.201 82.7882) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.788) (end 181.201 82.7881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7879) (end 181.201 82.788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7878) (end 181.201 82.7879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7877) (end 181.201 82.7878) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7876) (end 181.201 82.7877) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7875) (end 181.201 82.7876) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.201 82.7874) (end 181.201 82.7875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.201 49.6837) (end 153.201 64.2874) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.074 49.6837) (end 153.201 49.6837) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.074 116.357) (end 169.074 49.6837) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.308 120.701) (end 169.074 116.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.103 124.52) (end 168.308 120.701) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.724 127.355) (end 166.103 124.52) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.58 128.863) (end 162.724 127.355) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.375 129.056) (end 158.58 128.863) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.165 129.056) (end 156.375 129.056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.822 128.29) (end 127.165 129.056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.003 126.085) (end 122.822 128.29) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.168 122.707) (end 119.003 126.085) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.659 118.562) (end 116.168 122.707) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.466 116.357) (end 114.659 118.562) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.466 49.0475) (end 114.466 116.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.849 46.876) (end 114.466 49.0475) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.952 44.9665) (end 114.849 46.876) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.641 43.5493) (end 115.952 44.9665) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.713 42.7951) (end 117.641 43.5493) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.815 42.6987) (end 119.713 42.7951) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 42.6961) (end 135.42 42.6961) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.815 42.6961) (end 135.42 42.6961) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.815 42.6961) (end 120.815 42.6961) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.815 42.6961) (end 120.815 42.6961) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.712 42.7926) (end 120.815 42.6961) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.712 42.7926) (end 119.712 42.7926) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.712 42.7927) (end 119.712 42.7926) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.64 43.5469) (end 119.712 42.7927) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.639 43.5472) (end 117.64 43.5469) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.95 44.9647) (end 117.639 43.5472) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.95 44.9651) (end 115.95 44.9647) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.847 46.8749) (end 115.95 44.9651) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.847 46.8754) (end 114.847 46.8749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.464 49.0472) (end 114.847 46.8754) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.464 49.0473) (end 114.464 49.0472) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.464 49.0474) (end 114.464 49.0473) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.464 116.357) (end 114.464 49.0474) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.464 116.357) (end 114.464 116.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.464 116.358) (end 114.464 116.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.657 118.563) (end 114.464 116.358) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.657 118.563) (end 114.657 118.563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.657 118.563) (end 114.657 118.563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.165 122.708) (end 114.657 118.563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.166 122.708) (end 116.165 122.708) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.001 126.087) (end 116.166 122.708) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.001 126.087) (end 119.001 126.087) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.001 126.087) (end 119.001 126.087) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.821 128.293) (end 119.001 126.087) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.821 128.293) (end 122.821 128.293) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.165 129.059) (end 122.821 128.293) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.165 129.059) (end 127.165 129.059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.165 129.059) (end 127.165 129.059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.375 129.059) (end 127.165 129.059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.375 129.059) (end 156.375 129.059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.375 129.059) (end 156.375 129.059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.581 128.866) (end 156.375 129.059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.581 128.866) (end 158.581 128.866) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.581 128.866) (end 158.581 128.866) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.726 127.357) (end 158.581 128.866) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.726 127.357) (end 162.726 127.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.105 124.522) (end 162.726 127.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.105 124.522) (end 166.105 124.522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.105 124.521) (end 166.105 124.522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.31 120.702) (end 166.105 124.521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.31 120.701) (end 168.31 120.702) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 116.358) (end 168.31 120.701) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 116.358) (end 169.076 116.358) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 116.357) (end 169.076 116.358) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6824) (end 169.076 116.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6823) (end 169.076 49.6824) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6822) (end 169.076 49.6823) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6821) (end 169.076 49.6822) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.682) (end 169.076 49.6821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6819) (end 169.076 49.682) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6818) (end 169.076 49.6819) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6817) (end 169.076 49.6818) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6816) (end 169.076 49.6817) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6815) (end 169.076 49.6816) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6814) (end 169.076 49.6815) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6814) (end 169.076 49.6814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6813) (end 169.076 49.6814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6813) (end 169.076 49.6813) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.076 49.6812) (end 169.076 49.6813) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.075 49.6812) (end 169.076 49.6812) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.075 49.6811) (end 169.075 49.6812) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.075 49.6811) (end 169.075 49.6811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.075 49.6811) (end 169.075 49.6811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.2 49.6811) (end 169.075 49.6811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.2 49.6811) (end 153.2 49.6811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.2 49.6811) (end 153.2 49.6811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.2 49.6812) (end 153.2 49.6811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.2 49.6812) (end 153.2 49.6812) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.2 49.6813) (end 153.2 49.6812) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6813) (end 153.2 49.6813) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6814) (end 153.199 49.6813) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6814) (end 153.199 49.6814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6815) (end 153.199 49.6814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6816) (end 153.199 49.6815) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6817) (end 153.199 49.6816) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6818) (end 153.199 49.6817) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6819) (end 153.199 49.6818) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.682) (end 153.199 49.6819) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6821) (end 153.199 49.682) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6822) (end 153.199 49.6821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6823) (end 153.199 49.6822) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 49.6824) (end 153.199 49.6823) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.199 64.2861) (end 153.199 49.6824) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 64.2861) (end 153.199 64.2861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6974) (end 135.421 64.2861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6973) (end 135.421 42.6974) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6972) (end 135.421 42.6973) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6971) (end 135.421 42.6972) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.697) (end 135.421 42.6971) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6969) (end 135.421 42.697) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6968) (end 135.421 42.6969) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6967) (end 135.421 42.6968) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6966) (end 135.421 42.6967) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6965) (end 135.421 42.6966) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6964) (end 135.421 42.6965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6964) (end 135.421 42.6964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6963) (end 135.421 42.6964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6963) (end 135.421 42.6963) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.421 42.6962) (end 135.421 42.6963) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 42.6962) (end 135.421 42.6962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 42.6961) (end 135.42 42.6962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.42 42.6961) (end 135.42 42.6961) (layer Edge.Cuts) (width 0.1))
  (gr_text P8 (at 166 59.2) (layer F.SilkS))
  (gr_text P9 (at 117.7 59) (layer F.SilkS))
  (zone (net 1) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.1 64.6) (xy 153.5 64.6) (xy 153.5 50) (xy 168.7 50) (xy 168.7 116.4)
        (xy 168 120.4) (xy 166 124.2) (xy 162.6 127) (xy 158.6 128.6) (xy 156.4 128.8)
        (xy 127.2 128.8) (xy 123 128) (xy 119.2 125.8) (xy 116.4 122.6) (xy 115 118.6)
        (xy 114.8 116.4) (xy 114.8 49) (xy 115.2 47) (xy 116.2 45.2) (xy 117.8 43.8)
        (xy 119.8 43) (xy 135.1 43)
      )
    )
  )
  (zone (net 1) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.1 64.6) (xy 153.5 64.6) (xy 153.5 50) (xy 168.7 50) (xy 168.7 116.4)
        (xy 168 120.4) (xy 166 124.2) (xy 162.6 127) (xy 158.6 128.6) (xy 156.4 128.8)
        (xy 127.2 128.8) (xy 123 128) (xy 119.2 125.8) (xy 116.4 122.6) (xy 115 118.6)
        (xy 114.8 116.4) (xy 114.8 49) (xy 115.2 47) (xy 116.2 45.2) (xy 117.8 43.8)
        (xy 119.8 43) (xy 135.1 43)
      )
    )
  )
)
