(kicad_pcb (version 4) (host pcbnew 4.0.4-1.fc25-product)
  (general
    (links 5)
    (no_connects 0)
    (area 179.629999 88.819666 200.227001 119.714333)
    (thickness 1.6)
    (drawings 16)
    (tracks 11)
    (zones 0)
    (modules 3)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 186.11 112.58)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P4-Pad1)")
  (net 2 "Net-(P4-Pad2)")
  (net 3 "Net-(P5-Pad1)")
  (net 4 "Net-(P5-Pad2)")
  (net 5 "Net-(P5-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
  )
  (module sparkfun:SF-ROTARY-ENCODER (layer F.Cu) (tedit 58917B67)
    (at 189.992 104.14)
    (fp_text reference ROT1 (at 0 9.5) (layer F.SilkS) hide)
    (fp_text value ROTARY-ENCODER (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.5 -7) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P4-Pad2)"))
    (pad 2 thru_hole circle (at -2.5 7.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P5-Pad1)"))
    (pad 3 thru_hole circle (at 0 7.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P5-Pad2)"))
    (pad 4 thru_hole circle (at 2.5 7.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P5-Pad3)"))
    (pad 5 thru_hole circle (at 2.5 -7) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P4-Pad1)"))
    (pad "" thru_hole circle (at 5.6 0) (size 3 3) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -5.6 0) (size 3 3) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 587E811E)
    (at 189.992 93.853 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P4-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 587E8123)
    (at 187.452 114.681 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P5-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text ^GND (at 191.27 113.1) (layer F.Mask))
  (gr_text ^GND (at 191.27 113.1) (layer F.Cu))
  (gr_text B (at 194.25 111.63) (layer F.Cu))
  (gr_text B (at 194.25 111.63) (layer F.Mask))
  (gr_text "A\n" (at 185.71 111.63) (layer F.Mask))
  (gr_text "A\n" (at 185.71 111.63) (layer F.Cu))
  (gr_text "https://github.com/pdp7\nrotary-encoder-breakout\n" (at 189.992 99.822) (layer B.SilkS))
  (gr_text "SparkFun COM-09117\n318-ENC130175F-12PS" (at 190.119 108.458) (layer B.SilkS))
  (gr_line (start 179.705 116.84) (end 179.705 91.313) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.152 116.84) (end 179.705 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.152 91.313) (end 200.152 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.705 91.313) (end 200.152 91.313) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "SparkFun COM-09117\n" (at 198.755 103.886 90) (layer F.Mask))
  (gr_text "SparkFun COM-09117\n" (at 198.755 103.886 90) (layer F.Cu))
  (gr_text "pdp7/rotary-encoder-breakout\n" (at 180.848 104.394 90) (layer F.Mask))
  (gr_text "pdp7/rotary-encoder-breakout\n" (at 180.848 104.394 90) (layer F.Cu))
)
