<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="19.05" x2="39.04" y2="19.05" width="0" layer="20"/>
<wire x1="39.04" y1="19.05" x2="39.04" y2="58.41" width="0" layer="20"/>
<wire x1="39.04" y1="58.41" x2="0" y2="58.41" width="0" layer="20"/>
<wire x1="0" y1="58.41" x2="0" y2="19.05" width="0" layer="20"/>
<hole x="36.83" y="55.88" drill="0.35"/>
<hole x="36.83" y="21.59" drill="0.35"/>
<hole x="2.54" y="21.59" drill="0.35"/>
<hole x="2.54" y="55.88" drill="0.35"/>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-3">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 3 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC18U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="con-amp-mt">
<description>&lt;b&gt;AMP Connectors, Type MT&lt;/b&gt;&lt;p&gt;
include  Type MT6; con-amp-mt6.lbr&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="L10P">
<description>&lt;b&gt;AMP MT CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitor-wima" package="C2.5-3" value="10uF"/>
<element name="IC1" library="ic-package" package="DIL16" value="SM5021"/>
<element name="JP1" library="jumper" package="JP1" value="JP1"/>
<element name="JP2" library="jumper" package="JP1" value="JP2"/>
<element name="LED1" library="led" package="LD260" value="LED1"/>
<element name="Q1" library="crystal" package="HC18U-V" value="455kHz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="4.7"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K"/>
<element name="T1" library="transistor" package="TO92" value="2N3904"/>
<element name="T2" library="transistor" package="TO92" value="2N3904"/>
<element name="LED2" library="led" package="LD260" value="IR LED"/>
<element name="SV2" library="con-amp-mt" package="L10P" value="Connector">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="14"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="15"/>
<contactref element="T2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="T2" pad="3"/>
<contactref element="R2" pad="P$2"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="T2" pad="1"/>
<contactref element="T1" pad="1"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="3"/>
<contactref element="SV2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="4"/>
<contactref element="SV2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="5"/>
<contactref element="SV2" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="11"/>
<contactref element="SV2" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="10"/>
<contactref element="SV2" pad="7"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="9"/>
<contactref element="SV2" pad="8"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="6"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="7"/>
<contactref element="SV2" pad="5"/>
</signal>
<signal name="3.3V">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="IC1" pad="16"/>
<contactref element="SV2" pad="9"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="T1" pad="3"/>
<contactref element="IC1" pad="8"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="LED1" pad="K"/>
<contactref element="SV2" pad="10"/>
</signal>
<signal name="N$17">
<contactref element="JP2" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R1" pad="P$1"/>
<contactref element="LED2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
