(kicad_pcb (version 20170123) (host pcbnew "(2017-06-19 revision 6733101c6)-makepkg")
  (general
    (links 191)
    (no_connects 0)
    (area 105.49 40.64 157.985001 91.9408)
    (thickness 1.6)
    (drawings 19)
    (tracks 1003)
    (zones 0)
    (modules 81)
    (nets 85)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.2)
    (pad_size 1.778 1.778)
    (pad_drill 0.99822)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad46)")
  (net 2 "Net-(IC1-Pad45)")
  (net 3 "Net-(IC1-Pad35)")
  (net 4 "Net-(IC1-Pad21)")
  (net 5 "Net-(IC1-Pad20)")
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(U1-Pad4)")
  (net 11 "Net-(MS1-Pad1)")
  (net 12 "Net-(MS1-Pad3)")
  (net 13 "Net-(MS1-Pad5)")
  (net 14 "Net-(MS1-Pad6)")
  (net 15 "Net-(MS1-Pad7)")
  (net 16 "Net-(MS1-Pad8)")
  (net 17 "Net-(MS1-Pad9)")
  (net 18 "Net-(MS1-Pad10)")
  (net 19 "Net-(MS1-Pad14)")
  (net 20 "Net-(MS1-Pad15)")
  (net 21 "Net-(MS1-Pad16)")
  (net 22 "Net-(MS1-Pad19)")
  (net 23 "Net-(MS1-Pad20)")
  (net 24 "Net-(MS1-Pad23)")
  (net 25 "Net-(MS1-Pad24)")
  (net 26 "Net-(MS1-Pad25)")
  (net 27 "Net-(MS1-Pad27)")
  (net 28 "Net-(MS1-Pad28)")
  (net 29 UB)
  (net 30 UC)
  (net 31 UA)
  (net 32 "Net-(C17-Pad1)")
  (net 33 "Net-(C19-Pad1)")
  (net 34 "Net-(C21-Pad2)")
  (net 35 "Net-(C20-Pad2)")
  (net 36 "Net-(C15-Pad2)")
  (net 37 "Net-(C13-Pad2)")
  (net 38 "Net-(J9-Pad1)")
  (net 39 MOSI)
  (net 40 MISO)
  (net 41 SCLK)
  (net 42 CS)
  (net 43 CF1)
  (net 44 CF4)
  (net 45 CF2)
  (net 46 CF3)
  (net 47 I1P_IN)
  (net 48 I1P)
  (net 49 GND)
  (net 50 I2P_IN)
  (net 51 I1N)
  (net 52 I1N_IN)
  (net 53 I3N_IN)
  (net 54 I3P_IN)
  (net 55 I2N_IN)
  (net 56 I3N)
  (net 57 IP_IN)
  (net 58 IN_IN)
  (net 59 I2P)
  (net 60 I2N)
  (net 61 IP)
  (net 62 IN)
  (net 63 I3P)
  (net 64 DMA)
  (net 65 PM1)
  (net 66 PM0)
  (net 67 IRQ1)
  (net 68 IRQ2)
  (net 69 WARN)
  (net 70 ZX2)
  (net 71 ZX1)
  (net 72 ZX0)
  (net 73 V3P)
  (net 74 V2P)
  (net 75 V1P)
  (net 76 "Net-(D5-Pad2)")
  (net 77 "Net-(JP1-Pad1)")
  (net 78 USB)
  (net 79 "Net-(J9-Pad3)")
  (net 80 "Net-(J10-Pad1)")
  (net 81 "Net-(J10-Pad2)")
  (net 82 /Featherwing/VOUT)
  (net 83 /Featherwing/VIN)
  (net 84 VDD)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CF1)
    (add_net CF2)
    (add_net CF3)
    (add_net CF4)
    (add_net CS)
    (add_net DMA)
    (add_net I1N)
    (add_net I1N_IN)
    (add_net I1P)
    (add_net I1P_IN)
    (add_net I2N)
    (add_net I2N_IN)
    (add_net I2P)
    (add_net I2P_IN)
    (add_net I3N)
    (add_net I3N_IN)
    (add_net I3P)
    (add_net I3P_IN)
    (add_net IN)
    (add_net IN_IN)
    (add_net IP)
    (add_net IP_IN)
    (add_net IRQ1)
    (add_net IRQ2)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad35)")
    (add_net "Net-(IC1-Pad45)")
    (add_net "Net-(IC1-Pad46)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(J9-Pad3)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(MS1-Pad1)")
    (add_net "Net-(MS1-Pad10)")
    (add_net "Net-(MS1-Pad14)")
    (add_net "Net-(MS1-Pad15)")
    (add_net "Net-(MS1-Pad16)")
    (add_net "Net-(MS1-Pad19)")
    (add_net "Net-(MS1-Pad20)")
    (add_net "Net-(MS1-Pad23)")
    (add_net "Net-(MS1-Pad24)")
    (add_net "Net-(MS1-Pad25)")
    (add_net "Net-(MS1-Pad27)")
    (add_net "Net-(MS1-Pad28)")
    (add_net "Net-(MS1-Pad3)")
    (add_net "Net-(MS1-Pad5)")
    (add_net "Net-(MS1-Pad6)")
    (add_net "Net-(MS1-Pad7)")
    (add_net "Net-(MS1-Pad8)")
    (add_net "Net-(MS1-Pad9)")
    (add_net "Net-(U1-Pad4)")
    (add_net PM0)
    (add_net PM1)
    (add_net SCLK)
    (add_net V1P)
    (add_net V2P)
    (add_net V3P)
    (add_net WARN)
    (add_net ZX0)
    (add_net ZX1)
    (add_net ZX2)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Featherwing/VIN)
    (add_net /Featherwing/VOUT)
    (add_net GND)
    (add_net UA)
    (add_net UB)
    (add_net UC)
    (add_net USB)
    (add_net VDD)
  )
  (module Connectors_Phoenix:PhoenixContact_MC-G_04x3.50mm_Angled locked (layer F.Cu) (tedit 59566E61)
    (at 115.316 46.736 270)
    (descr "Generic Phoenix Contact connector footprint for series: MC-G; number of pins: 04; pin pitch: 3.50mm; Angled || order number: 1844236 8A 160V")
    (tags "phoenix_contact connector MC_01x04_G_3.5mm")
    (fp_text reference J4 (at -3.81 3.048) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.25 9 270) (layer F.Fab))
    (fp_text user %R (at 5.25 3 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 10.5 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 UA))
    (pad 3 thru_hole oval (at 7 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 UB))
    (pad 2 thru_hole oval (at 3.5 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 30 UC))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MC-G_04x3.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_SH_BM04B-SRSS-TB_04x1.00mm_Straight (layer F.Cu) (tedit 56B07435)
    (at 110.992 65.7785 180)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J1 (at -1.5 -3.5 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 3.5 180) (layer F.Fab))
    (pad "" smd rect (at 2.8 -1.2625 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -2.8 -1.2625 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 43 CF1))
    (pad 3 smd rect (at 0.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 45 CF2))
    (pad 2 smd rect (at -0.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 46 CF3))
    (pad 1 smd rect (at -1.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 44 CF4))
    (model ${KIPRJMOD}/JST.3dshapes/BM04B-SRSS-TB.STEP
      (at (xyz 0 0.05905511811023623 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_JST:JST_SH_BM06B-SRSS-TB_06x1.00mm_Straight (layer F.Cu) (tedit 56B07435)
    (at 120.279 65.7935 180)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J8 (at 0.645 -3.5 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 3.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 64 DMA))
    (pad 2 smd rect (at -1.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 65 PM1))
    (pad 3 smd rect (at -0.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 66 PM0))
    (pad 4 smd rect (at 0.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 67 IRQ1))
    (pad 5 smd rect (at 1.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 68 IRQ2))
    (pad 6 smd rect (at 2.5 1.2625 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 69 WARN))
    (pad "" smd rect (at -3.8 -1.2625 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.8 -1.2625 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (model ${KIPRJMOD}/JST.3dshapes/BM06B-SRSS-TB.STEP
      (at (xyz 0 0.05905511811023623 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_JST:JST_SH_BM06B-SRSS-TB_06x1.00mm_Straight (layer F.Cu) (tedit 56B07435)
    (at 138.694 43.6805)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J3 (at 3.546 3.5635) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 3.5) (layer F.Fab))
    (pad "" smd rect (at 3.8 -1.2625) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.8 -1.2625) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.5 1.2625) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 5 smd rect (at 1.5 1.2625) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 42 CS))
    (pad 4 smd rect (at 0.5 1.2625) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 41 SCLK))
    (pad 3 smd rect (at -0.5 1.2625) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 40 MISO))
    (pad 2 smd rect (at -1.5 1.2625) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 39 MOSI))
    (pad 1 smd rect (at -2.5 1.2625) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (model ${KIPRJMOD}/JST.3dshapes/BM06B-SRSS-TB.STEP
      (at (xyz 0 0.05905511811023623 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_JST:JST_SH_BM03B-SRSS-TB_03x1.00mm_Straight (layer F.Cu) (tedit 56B07435)
    (at 129.018 43.6805)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J11 (at -1.51 3.5635) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 3.5) (layer F.Fab))
    (pad "" smd rect (at 2.3 -1.2625) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -2.3 -1.2625) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1 1.2625) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 72 ZX0))
    (pad 2 smd rect (at 0 1.2625) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 71 ZX1))
    (pad 1 smd rect (at -1 1.2625) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 70 ZX2))
    (model ${KIPRJMOD}/JST.3dshapes/BM03B-SRSS-TB.STEP
      (at (xyz 0 0.05905511811023623 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 135.144 62.992)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at -2.302 0.508 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 132.35 51.054)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0.492 2.032) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA locked (layer F.Cu) (tedit 586432E5)
    (at 112.236 84.328 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D7 (at 4.032 0 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.6 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 83 /Featherwing/VIN))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 31 UA))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA locked (layer F.Cu) (tedit 586432E5)
    (at 112.268 80.01 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D8 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.6 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 83 /Featherwing/VIN))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 29 UB))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA locked (layer F.Cu) (tedit 586432E5)
    (at 112.268 75.692 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D9 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.6 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 83 /Featherwing/VIN))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 30 UC))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ATM90E26_from_eagle:SEEED-CONNECTOR--2016_HW4-SMD-2.0-90D locked (layer F.Cu) (tedit 200000)
    (at 148.336 80.01 270)
    (attr smd)
    (fp_text reference J10 (at 7.366 -3.81) (layer F.SilkS))
    (fp_text value GROVE-SMD-90D (at 0.127 -4.8895 270) (layer F.SilkS))
    (pad SS2 smd rect (at 5.3975 -7.39902) (size 2.99974 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad SS1 smd rect (at -5.40004 -7.39902) (size 2.99974 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 4 smd rect (at 2.99974 0.09906) (size 2.73812 1.00838) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 3 smd rect (at 0.99822 0.09906) (size 2.73812 1.00838) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (pad 2 smd rect (at -0.99822 0.09906) (size 2.73812 1.00838) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(J10-Pad2)"))
    (pad 1 smd rect (at -2.99974 0.09906) (size 2.73812 1.00838) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(J10-Pad1)"))
    (model "${KIPRJMOD}/SeeedStudio.3dshapes/Grove Connecteur.wrl"
      (at (xyz 0 0.3937007874015748 -0.03937007874015748))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:CP_Elec_5x5.8 locked (layer F.Cu) (tedit 58AA8B00)
    (at 143.002 79.248 270)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.8")
    (attr smd)
    (fp_text reference C23 (at -4.572 0) (layer F.SilkS))
    (fp_text value 100u/16V (at 0 -3.92 270) (layer F.Fab))
    (fp_text user + (at -1.38 -0.06 270) (layer F.Fab))
    (fp_text user + (at -3.38 2.35 270) (layer F.SilkS))
    (fp_text user %R (at 0 3.92 270) (layer F.Fab))
    (pad 1 smd rect (at -2.2 0 90) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 82 /Featherwing/VOUT))
    (pad 2 smd rect (at 2.2 0 90) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_5x5.8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x10 locked (layer F.Cu) (tedit 58AA9153)
    (at 121.412 80.01 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C25 (at -6.096 0 180) (layer F.SilkS))
    (fp_text value 220u/50V (at 0 -5.45 90) (layer F.Fab))
    (fp_text user + (at -2.31 -0.08 90) (layer F.Fab))
    (fp_text user + (at -4.78 3.9 90) (layer F.SilkS))
    (fp_text user %R (at 0 5.45 90) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 83 /Featherwing/VIN))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 locked (layer F.Cu) (tedit 597D6277)
    (at 143.002 85.344)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at -0.254 -1.27) (layer F.SilkS))
    (fp_text value 1u/16V (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 82 /Featherwing/VOUT))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 locked (layer F.Cu) (tedit 58AA844E)
    (at 117.856 72.644 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 1u/50V (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 83 /Featherwing/VIN))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 locked (layer F.Cu) (tedit 586134A1)
    (at 138.176 87.63 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP1 (at 0 2.794) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at -1.8 0) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 82 /Featherwing/VOUT))
  )
  (module Connectors:GS3 (layer B.Cu) (tedit 58613494)
    (at 120.142 44.704)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J7 (at -1.7 0 -90) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 -90) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 65 PM1))
    (pad 3 smd rect (at 0 -1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 84 VDD))
  )
  (module Connectors:GS3 (layer B.Cu) (tedit 58613494)
    (at 127.762 44.704)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J2 (at -1.7 0 -90) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 -90) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 64 DMA))
    (pad 3 smd rect (at 0 -1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 84 VDD))
  )
  (module Connectors:GS3 locked (layer B.Cu) (tedit 58613494)
    (at 123.952 44.704)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J6 (at -1.7 0 -90) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 -90) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 66 PM0))
    (pad 3 smd rect (at 0 -1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 84 VDD))
  )
  (module Molex_RJ45:RJ45_8 locked (layer F.Cu) (tedit 58C81A5F)
    (at 143.256 61.629 90)
    (tags RJ45)
    (fp_text reference J5 (at 4.7 11.18 90) (layer F.SilkS))
    (fp_text value RJ45 (at 4.59 6.25 90) (layer F.Fab))
    (pad 9 thru_hole circle (at -3.65 9.4 90) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 9 thru_hole circle (at 12.54 9.4 90) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad Hole np_thru_hole circle (at 10.38 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad "" np_thru_hole circle (at -1.49 6.35 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 I1P_IN))
    (pad 2 thru_hole circle (at 1.27 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 I1N_IN))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 I2P_IN))
    (pad 4 thru_hole circle (at 3.81 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 I2N_IN))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 I3P_IN))
    (pad 6 thru_hole circle (at 6.35 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 I3N_IN))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 57 IP_IN))
    (pad 8 thru_hole circle (at 8.89 -2.54 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 IN_IN))
    (model :Git3D:Connectors_Molex.3dshapes/Molex_955402881.stp
      (at (xyz 0.1771653543307087 -0.5590551181102362 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
    (model ${KIPRJMOD}/Molex_RJ45.3dshapes/Molex_955402881.stp
      (at (xyz 0.1771653543307087 -0.5590551181102362 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Whatnick_logo:Whatnick_logo locked (layer B.Cu) (tedit 0)
    (at 122.174 78.994 270)
    (fp_text reference LOGO2 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 138.176 55.372)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -3.556 0.254 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 63 I3P))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 54 I3P_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer F.Cu) (tedit 58E0A85E)
    (at 136.906 49.276 180)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R27 (at 0 -2.6 180) (layer F.SilkS))
    (fp_text value SMD-RES-ARRAY (at 0 2.6 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (pad 3 smd rect (at -0.85 0.4 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (pad 1 smd rect (at -0.85 -1.2 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (pad 4 smd rect (at -0.85 1.2 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (pad 8 smd rect (at 0.85 -1.2 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 CS))
    (pad 7 smd rect (at 0.85 -0.4 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 SCLK))
    (pad 6 smd rect (at 0.85 0.4 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 MISO))
    (pad 5 smd rect (at 0.85 1.2 180) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 MOSI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS3 locked (layer B.Cu) (tedit 58613494)
    (at 139.954 73.152 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J9 (at -1.7 0 180) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J9-Pad1)"))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 42 CS))
    (pad 3 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(J9-Pad3)"))
  )
  (module Diodes_SMD:D_SOD-123 locked (layer F.Cu) (tedit 58645DC7)
    (at 142.748 72.898)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D6 (at 3.556 0) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 78 USB))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 82 /Featherwing/VOUT))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 locked (layer F.Cu) (tedit 57FE93A5)
    (at 146.812 87.63 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering locked (layer F.Cu) (tedit 58E0A804)
    (at 142.494 87.63)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at -1.778 -2.286 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 114.808 79.248 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference LOGO1 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OPEN_HARDWARE_1 (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 locked (layer F.Cu) (tedit 58E0A85E)
    (at 119.634 61.214 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R28 (at 0 -2.6 270) (layer F.SilkS))
    (fp_text value SMD-RES-ARRAY (at 0 2.6 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 CF3))
    (pad 3 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 CF2))
    (pad 1 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 44 CF4))
    (pad 4 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 CF1))
    (pad 8 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 7 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 6 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 5 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ATM90E26_from_eagle:ADAFRUIT_FEATHERWING locked (layer F.Cu) (tedit 59467C6D)
    (at 106.985 91.4908)
    (attr virtual)
    (fp_text reference MS1 (at 19.05 -7.62) (layer F.SilkS) hide)
    (fp_text value ADAFRUIT_FEATHERWING (at 22.86 -5.08) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 6.35 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 11 "Net-(MS1-Pad1)"))
    (pad 2 thru_hole circle (at 8.89 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 84 VDD))
    (pad 3 thru_hole circle (at 11.43 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 12 "Net-(MS1-Pad3)"))
    (pad 4 thru_hole circle (at 13.97 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 5 thru_hole circle (at 16.51 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 13 "Net-(MS1-Pad5)"))
    (pad 6 thru_hole circle (at 19.05 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 14 "Net-(MS1-Pad6)"))
    (pad 7 thru_hole circle (at 21.59 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 15 "Net-(MS1-Pad7)"))
    (pad 8 thru_hole circle (at 24.13 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 16 "Net-(MS1-Pad8)"))
    (pad 9 thru_hole circle (at 26.67 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 17 "Net-(MS1-Pad9)"))
    (pad 10 thru_hole circle (at 29.21 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 18 "Net-(MS1-Pad10)"))
    (pad 11 thru_hole circle (at 31.75 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 41 SCLK))
    (pad 12 thru_hole circle (at 34.29 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 39 MOSI))
    (pad 13 thru_hole circle (at 36.83 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 40 MISO))
    (pad 14 thru_hole circle (at 39.37 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 19 "Net-(MS1-Pad14)"))
    (pad 15 thru_hole circle (at 41.91 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 20 "Net-(MS1-Pad15)"))
    (pad 16 thru_hole circle (at 44.45 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 21 "Net-(MS1-Pad16)"))
    (pad 17 thru_hole circle (at 44.45 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 81 "Net-(J10-Pad2)"))
    (pad 18 thru_hole circle (at 41.91 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 80 "Net-(J10-Pad1)"))
    (pad 19 thru_hole circle (at 39.37 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 22 "Net-(MS1-Pad19)"))
    (pad 20 thru_hole circle (at 36.83 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 23 "Net-(MS1-Pad20)"))
    (pad 21 thru_hole circle (at 34.29 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 79 "Net-(J9-Pad3)"))
    (pad 22 thru_hole circle (at 31.75 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 38 "Net-(J9-Pad1)"))
    (pad 23 thru_hole circle (at 29.21 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 24 "Net-(MS1-Pad23)"))
    (pad 24 thru_hole circle (at 26.67 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 25 "Net-(MS1-Pad24)"))
    (pad 25 thru_hole circle (at 24.13 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 26 "Net-(MS1-Pad25)"))
    (pad 26 thru_hole circle (at 21.59 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 78 USB))
    (pad 27 thru_hole circle (at 19.05 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 27 "Net-(MS1-Pad27)"))
    (pad 28 thru_hole circle (at 16.51 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 28 "Net-(MS1-Pad28)"))
    (pad "" thru_hole circle (at 2.54 -20.32) (size 3.81 3.81) (drill 2.49936) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole circle (at 2.54 -2.54) (size 3.81 3.81) (drill 2.49936) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" np_thru_hole circle (at 48.26 -20.32) (size 2.49936 2.49936) (drill 2.49936) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 48.26 -2.54) (size 2.49936 2.49936) (drill 2.49936) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 120.396 50.534 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0.266 -4.572 270) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 75 V1P))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 139.7 48.514 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -2.286 0 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 61 IP))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 132.092 49.022)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 -1.5) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 118.745 44.057 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -0.139 3.429 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 136.652 60.186 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 135.128 65.024)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 2.286 0.508 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 130.556 66.536 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0.52 1.524 270) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 118.745 50.685 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0.139 3.429 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C21-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 138.176 62.992 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0.508 -4.826 90) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 51 I1N))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 136.652 56.146 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 139.7 65.278 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.286 -0.254 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 48 I1P))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 135.89 55.626 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -2.54 90) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 63 I3P))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 135.89 52.07 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.254 -4.064 90) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 56 I3N))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 locked (layer B.Cu) (tedit 58AA844E)
    (at 120.396 57.289 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0.115 -4.572 270) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 73 V3P))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 locked (layer B.Cu) (tedit 58AA844E)
    (at 120.396 53.836 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -4.572 270) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 74 V2P))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 135.89 62.23 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -0.254 -3.81 90) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 59 I2P))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 135.89 58.674 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -0.254 -4.064 90) (layer B.SilkS))
    (fp_text value C_Small (at 9.652 -4.318 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 60 I2N))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 118.745 47.51 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 0.266 3.429 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C20-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 138.176 50.8 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 1.524 5.08 270) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 62 IN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_2520-4pin_2.5x2.0mm (layer F.Cu) (tedit 58CD2E9C)
    (at 119.634 54.356 180)
    (descr "SMD Crystal SERIES SMD2520/4 http://www.newxtal.com/UploadFiles/Images/2012-11-12-09-29-09-776.pdf, 2.5x2.0mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 -2.2 180) (layer F.SilkS))
    (fp_text value Crystal_GND24 (at 0 2.2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.875 0.7 180) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad20)"))
    (pad 2 smd rect (at 0.875 0.7 180) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 3 smd rect (at 0.875 -0.7 180) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad21)"))
    (pad 4 smd rect (at -0.875 -0.7 180) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_2520-4pin_2.5x2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 138.176 60.452)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at -3.81 -1.524 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 I2P))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 I2P_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 138.176 58.674)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at -5.08 0.254 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 60 I2N))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 55 I2N_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 140.716 50.292)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 1.524 1.778 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 62 IN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 IN_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 locked (layer B.Cu) (tedit 58E0A804)
    (at 118.618 50.534 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at -0.266 5.08 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 UC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 75 V1P))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 locked (layer B.Cu) (tedit 597D6AF0)
    (at 122.174 50.534 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 0.266 -4.064 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 75 V1P))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 120.523 44.081 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0.115 -2.921 270) (layer F.SilkS))
    (fp_text value R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C15-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 120.523 47.486 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at -0.242 -2.921 270) (layer F.SilkS))
    (fp_text value R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C20-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 132.588 66.56 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at -0.75 1.778 90) (layer F.SilkS))
    (fp_text value R (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 locked (layer B.Cu) (tedit 58E0A804)
    (at 146.57 54.356)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 5.322 -0.254 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 IN_IN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 143.51 50.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 -1.524 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 61 IP))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 IP_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 120.523 50.788 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at -0.242 -2.921 270) (layer F.SilkS))
    (fp_text value R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C21-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 149.594 54.356)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 3.568 -0.254 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 IP_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 locked (layer B.Cu) (tedit 58E0A804)
    (at 118.618 57.15 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -0.254 5.08 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 31 UA))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 73 V3P))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 146.57 58.166)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 5.322 0 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 55 I2N_IN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 locked (layer B.Cu) (tedit 58E0A804)
    (at 122.174 57.265 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0.139 -4.064 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 73 V3P))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 locked (layer B.Cu) (tedit 58E0A804)
    (at 118.618 53.836 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 5.08 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 29 UB))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 74 V2P))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 locked (layer B.Cu) (tedit 597D6A45)
    (at 122.174 53.836 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -4.064 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 74 V2P))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 149.594 58.166)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 3.568 0 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 I2P_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 138.176 53.594)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -3.81 -1.27 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 56 I3N))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 53 I3N_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ROF-78E:SMD-4 locked (layer F.Cu) (tedit 0)
    (at 126.492 85.344)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U1 (at 1.27 2.032) (layer F.SilkS))
    (fp_text value ROF-78E (at 6.096 -2.032) (layer F.SilkS))
    (pad 4 smd rect (at 1 -1) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad4)") (solder_mask_margin 0.2))
    (pad 3 smd rect (at 11.5 -1) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 82 /Featherwing/VOUT) (solder_mask_margin 0.2))
    (pad 2 smd rect (at 11.5 -11.5) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 49 GND) (solder_mask_margin 0.2))
    (pad 1 smd rect (at 1 -11.5) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 83 /Featherwing/VIN) (solder_mask_margin 0.2))
    (model ${KIPRJMOD}/RECOM_ROF-78E.3dshapes/RECOM_ROF-78E.step
      (at (xyz 0.2480314960629921 0.2480314960629921 0))
      (scale (xyz 1 0.95 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 locked (layer F.Cu) (tedit 57FE93A5)
    (at 113.538 60.452)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 3.556 0.254 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 locked (layer F.Cu) (tedit 57FE93A5)
    (at 109.982 60.452 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -5.842 -0.254 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 locked (layer F.Cu) (tedit 57FE93A5)
    (at 109.982 62.23 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -5.842 -0.254 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 locked (layer F.Cu) (tedit 57FE93A5)
    (at 113.538 62.103)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 3.556 0.381 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 149.618 59.944)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 3.544 0.254 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 I1P_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 locked (layer B.Cu) (tedit 58E0A804)
    (at 146.57 59.944)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 5.322 0.254 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 52 I1N_IN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 149.618 56.134)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 3.544 0 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 54 I3P_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 146.57 56.134)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 5.322 0 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 53 I3N_IN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 143.002 64.008)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.286 0) (layer B.SilkS))
    (fp_text value R (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 I1P))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 I1P_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 140.208 62.738 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0.254 -5.588 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 51 I1N))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 52 I1N_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-48_7x7mm_Pitch0.5mm locked (layer F.Cu) (tedit 58CC9A48)
    (at 128.811 58.4428 225)
    (descr "48 LEAD TQFP 7x7mm (see MICREL TQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference IC1 (at -4.30331 4.70919 225) (layer F.SilkS))
    (fp_text value ATM90E36_ATM90E36 (at 0 6 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (pad 2 smd rect (at -4.35 -2.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 3 smd rect (at -4.35 -1.749999 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 I1P))
    (pad 4 smd rect (at -4.35 -1.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 I1N))
    (pad 5 smd rect (at -4.35 -0.750001 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 I2P))
    (pad 6 smd rect (at -4.35 -0.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 I2N))
    (pad 7 smd rect (at -4.35 0.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 I3P))
    (pad 8 smd rect (at -4.35 0.750001 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 I3N))
    (pad 9 smd rect (at -4.35 1.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 IP))
    (pad 10 smd rect (at -4.35 1.749999 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 IN))
    (pad 11 smd rect (at -4.35 2.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C13-Pad2)"))
    (pad 12 smd rect (at -4.35 2.75 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 13 smd rect (at -2.75 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 75 V1P))
    (pad 14 smd rect (at -2.25 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C15-Pad2)"))
    (pad 15 smd rect (at -1.749999 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 V2P))
    (pad 16 smd rect (at -1.25 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C20-Pad2)"))
    (pad 17 smd rect (at -0.750001 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 73 V3P))
    (pad 18 smd rect (at -0.25 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C21-Pad2)"))
    (pad 19 smd rect (at 0.25 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 20 smd rect (at 0.750001 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 1.25 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad21)"))
    (pad 22 smd rect (at 1.749999 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 ZX0))
    (pad 23 smd rect (at 2.25 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 71 ZX1))
    (pad 24 smd rect (at 2.75 4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 70 ZX2))
    (pad 25 smd rect (at 4.35 2.75 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 CF1))
    (pad 26 smd rect (at 4.35 2.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 CF2))
    (pad 27 smd rect (at 4.35 1.749999 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 CF3))
    (pad 28 smd rect (at 4.35 1.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 CF4))
    (pad 29 smd rect (at 4.35 0.750001 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 WARN))
    (pad 30 smd rect (at 4.35 0.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 IRQ2))
    (pad 31 smd rect (at 4.35 -0.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 IRQ1))
    (pad 32 smd rect (at 4.35 -0.750001 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 33 smd rect (at 4.35 -1.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 PM0))
    (pad 34 smd rect (at 4.35 -1.749999 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 PM1))
    (pad 35 smd rect (at 4.35 -2.25 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad35)"))
    (pad 36 smd rect (at 4.35 -2.75 225) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 DMA))
    (pad 37 smd rect (at 2.75 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 CS))
    (pad 38 smd rect (at 2.25 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 SCLK))
    (pad 39 smd rect (at 1.749999 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 MISO))
    (pad 40 smd rect (at 1.25 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 MOSI))
    (pad 41 smd rect (at 0.750001 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C19-Pad1)"))
    (pad 42 smd rect (at 0.25 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C17-Pad1)"))
    (pad 43 smd rect (at -0.25 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C17-Pad1)"))
    (pad 44 smd rect (at -0.750001 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 45 smd rect (at -1.25 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad45)"))
    (pad 46 smd rect (at -1.749999 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(IC1-Pad46)"))
    (pad 47 smd rect (at -2.25 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 48 smd rect (at -2.75 -4.35 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 84 VDD))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text CF (at 115.062 67.056 90) (layer F.SilkS))
  (gr_text SIG (at 125.73 67.056 90) (layer F.SilkS))
  (gr_text ZX (at 124.968 42.418 90) (layer F.SilkS))
  (gr_text SPI (at 133.35 42.418 90) (layer F.SilkS))
  (gr_text DMA (at 127.762 47.752) (layer B.SilkS))
  (gr_text PM1 (at 123.952 47.752) (layer B.SilkS))
  (gr_text PM0 (at 120.142 47.752) (layer B.SilkS))
  (gr_text CS (at 139.954 75.184) (layer B.SilkS))
  (gr_text "ATM90E3X Featherwing\nv1.0 30/07/2017\nDesign by: Tisham Dhar\nhttp://whatnick.com\n(CS pins - 9 or 10)" (at 140.462 81.534) (layer B.SilkS))
  (gr_arc (start 154.832756 88.859078) (end 157.654978 88.859078) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 109.6772 88.859078) (end 106.854978 88.859078) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 154.832756 43.703522) (end 157.654978 43.703522) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 109.6772 43.703522) (end 109.6772 40.8813) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 106.854978 88.859078) (end 106.854978 43.703522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.6772 40.8813) (end 109.6772 40.8813) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.654978 43.703522) (end 157.654978 88.859078) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154.832756 91.6813) (end 109.6772 91.6813) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.6772 40.8813) (end 154.832756 40.8813) (layer Edge.Cuts) (width 0.1))
  (zone (net 49) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.68 40.64) (xy 157.48 40.64) (xy 157.48 91.44) (xy 106.68 91.44)
      )
    )
  )
)
