(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 76)
    (zones 0)
    (modules 5)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (trace_clearance 0.0508)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.0508)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
  )
  (module Connector_JST:JST_SUR_SM06B-SURS-TF_1x06-1MP_P0.80mm_Horizontal (layer F.Cu) (tedit 5B78AD88)
    (at 144.78 83.82 270)
    (descr "JST SUR series connector, SM06B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SUR top entry")
    (attr smd)
    (fp_text reference J1 (at 0 0 90) (layer F.SilkS))
    (fp_text value SM06B (at 0.508 -3.302 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2 -1.15 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd roundrect (at -1.2 -1.15 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd roundrect (at -0.4 -1.15 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd roundrect (at 0.4 -1.15 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd roundrect (at 1.2 -1.15 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd roundrect (at 2 -1.15 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad6)"))
    (pad MP smd roundrect (at -3.3 0.8 270) (size 1.2 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 3.3 0.8 270) (size 1.2 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SUR_SM06B-SURS-TF_1x06-1MP_P0.80mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SUR_SM02B-SURS-TF_1x02-1MP_P0.80mm_Horizontal (layer F.Cu) (tedit 5B78AD88)
    (at 144.78 92.71 270)
    (descr "JST SUR series connector, SM02B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SUR top entry")
    (attr smd)
    (fp_text reference J2 (at 0 0 90) (layer F.SilkS))
    (fp_text value SM02B (at -0.508 -3.302 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.4 -1.15 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd roundrect (at 0.4 -1.15 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad2)"))
    (pad MP smd roundrect (at -1.7 0.8 270) (size 1.2 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 1.7 0.8 270) (size 1.2 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SUR_SM02B-SURS-TF_1x02-1MP_P0.80mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 152.4 81.28)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 2.286 6.35 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
  )
  (module Connector_JST:JST_SUR_SM03B-SURS-TF_1x03-1MP_P0.80mm_Horizontal (layer B.Cu) (tedit 5B78AD88)
    (at 144.78 91.44 90)
    (descr "JST SUR series connector, SM03B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SUR top entry")
    (attr smd)
    (fp_text reference J4 (at 0 0 90) (layer B.SilkS))
    (fp_text value SM03B (at -0.508 3.302 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.8 1.15 90) (size 0.5 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd roundrect (at 0 1.15 90) (size 0.5 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd roundrect (at 0.8 1.15 90) (size 0.5 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad3)"))
    (pad MP smd roundrect (at -2.1 -0.8 90) (size 1.2 1.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 2.1 -0.8 90) (size 1.2 1.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SUR_SM03B-SURS-TF_1x03-1MP_P0.80mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SUR_SM04B-SURS-TF_1x04-1MP_P0.80mm_Horizontal (layer B.Cu) (tedit 5B78AD88)
    (at 144.78 83.82 90)
    (descr "JST SUR series connector, SM04B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SUR top entry")
    (attr smd)
    (fp_text reference J5 (at 0 0 90) (layer B.SilkS))
    (fp_text value SM04B (at -0.254 3.302 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.2 1.15 90) (size 0.5 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd roundrect (at -0.4 1.15 90) (size 0.5 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd roundrect (at 0.4 1.15 90) (size 0.5 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd roundrect (at 1.2 1.15 90) (size 0.5 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad4)"))
    (pad MP smd roundrect (at -2.5 -0.8 90) (size 1.2 1.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 2.5 -0.8 90) (size 1.2 1.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SUR_SM04B-SURS-TF_1x04-1MP_P0.80mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "JST SUR Breakout" (at 148.844 96.774) (layer F.SilkS))
  (gr_text "1 2 3 4 5 6" (at 154.94 87.63 90) (layer B.SilkS))
  (gr_text "JST SUR Breakout" (at 148.844 96.52) (layer B.SilkS))
  (gr_line (start 139.7 81.28) (end 139.7 93.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 76.2) (end 144.78 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.48 93.98) (end 157.48 81.28) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.78 99.06) (end 152.4 99.06) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 144.78 93.98) (end 139.7 93.98) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 144.78 81.28) (end 144.78 76.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 152.4 81.28) (end 157.48 81.28) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 152.4 93.98) (end 152.4 99.06) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "6 5 4 3 2 1" (at 154.94 87.63 90) (layer F.SilkS))
)
