(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 23)
    (no_connects 0)
    (area 126.51 57.509999 166.505001 86.435001)
    (thickness 1.6)
    (drawings 33)
    (tracks 65)
    (zones 0)
    (modules 15)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 Sense)
  (net 3 Switched)
  (net 4 "Net-(P1-Pad1)")
  (net 5 GND)
  (net 6 AlwaysOn)
  (net 7 "Net-(P4-Pad1)")
  (net 8 "Net-(P5-Pad1)")
  (net 9 "Net-(P5-Pad2)")
  (net 10 MOSFET)
  (net 11 LED)
  (net 12 "Net-(R1-Pad2)")
  (net 13 "Net-(R2-Pad2)")
  (net 14 "Net-(U1-Pad1)")
  (net 15 Shutdown)
  (net 16 "Net-(U1-Pad9)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net AlwaysOn)
    (add_net LED)
    (add_net MOSFET)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad9)")
    (add_net Sense)
    (add_net Shutdown)
    (add_net Switched)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1.016)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
  )
  (module Connect:PINHEAD1-3 (layer F.Cu) (tedit 5ADEA4B9)
    (at 132.715 81.915 270)
    (attr virtual)
    (fp_text reference P1 (at -1.27 4.445 270) (layer F.SilkS))
    (fp_text value "Power input" (at -17.145 4.445 270) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 2 Sense))
  )
  (module Connect:PINHEAD1-2 (layer F.Cu) (tedit 5ADEA4D5)
    (at 132.715 67.945 270)
    (attr virtual)
    (fp_text reference P2 (at 8.89 4.445 270) (layer F.SilkS))
    (fp_text value "Switched Output" (at 1.27 4.445 270) (layer F.Fab))
    (pad 1 thru_hole oval (at -1.27 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 3 Switched))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5ADEA4C2)
    (at 153.67 84.455 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -3.81 26.035 270) (layer F.SilkS))
    (fp_text value "Always On Switch" (at -10.16 26.035 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 AlwaysOn))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5ADEA4BE)
    (at 143.51 84.455 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -1.905 15.875 270) (layer F.SilkS))
    (fp_text value "Status LED" (at -12.7 15.875 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5ADEA665)
    (at 163.83 84.455 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -1.905 35.56 270) (layer F.SilkS))
    (fp_text value "Request Shutdown" (at -15.875 35.56 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P5-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 5ADEA4C8)
    (at 134.62 73.66 180)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference Q1 (at -1.27 10.16 180) (layer F.SilkS))
    (fp_text value FQP27P06 (at -1.27 10.795 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 Switched))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 MOSFET))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer B.Cu) (tedit 5ADEA870)
    (at 161.925 76.2)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -27.305 -12.7) (layer B.Fab))
    (fp_text value 1k (at -3.175 0) (layer B.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 15 Shutdown))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer B.Cu) (tedit 5ADEA4C5)
    (at 146.685 75.565)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -8.89 -12.065) (layer B.Fab))
    (fp_text value 10k (at -3.81 0) (layer B.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 Sense))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer B.Cu) (tedit 5ADEA4C4)
    (at 151.765 75.565)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -15.875 -12.7) (layer B.Fab))
    (fp_text value 4.7k (at 3.81 0) (layer B.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:R_1206_MTS (layer B.Cu) (tedit 5ADEA8D4)
    (at 147.32 84.455 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 11.43 20.955 180) (layer B.Fab))
    (fp_text value 1k (at 0 1.905 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 LED))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(P4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:DigiSpark (layer F.Cu) (tedit 5ADEA4C0)
    (at 149.225 73.66)
    (fp_text reference U1 (at -16.51 -10.795) (layer F.SilkS))
    (fp_text value DigiSpark (at -13.335 -12.065) (layer F.Fab))
    (fp_text user D5 (at 7.62 2.54 90) (layer F.SilkS))
    (fp_text user D4 (at 5.08 2.54 90) (layer F.SilkS))
    (fp_text user D3 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text user D2 (at 0 2.54 90) (layer F.SilkS))
    (fp_text user D1 (at -2.54 2.54 90) (layer F.SilkS))
    (fp_text user D0 (at -5.08 2.54 90) (layer F.SilkS))
    (fp_text user Vin (at -5.08 -2.54) (layer F.SilkS))
    (fp_text user GND (at -5.08 -5.08) (layer F.SilkS))
    (fp_text user +5V (at -5.08 -7.62) (layer F.SilkS))
    (pad 1 thru_hole oval (at -7.62 -7.62) (size 1.778 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at -7.62 -5.08) (size 1.778 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 3 thru_hole oval (at -7.62 -2.54) (size 1.778 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad1)"))
    (pad 4 thru_hole oval (at -5.08 5.08) (size 1.524 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 MOSFET))
    (pad 5 thru_hole oval (at -2.54 5.08) (size 1.524 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 LED))
    (pad 6 thru_hole oval (at 0 5.08) (size 1.524 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R2-Pad2)"))
    (pad 7 thru_hole oval (at 2.54 5.08) (size 1.524 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 AlwaysOn))
    (pad 8 thru_hole oval (at 5.08 5.08) (size 1.524 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 Shutdown))
    (pad 9 thru_hole oval (at 7.62 5.08) (size 1.524 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad9)"))
  )
  (module Housings_DIP:DIP-4_W7.62mm_LongPads (layer F.Cu) (tedit 5ADEA8D6)
    (at 163.83 72.39 270)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at -9.525 29.21 270) (layer F.SilkS))
    (fp_text value LTV-817 (at 0.635 35.56 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 3 thru_hole oval (at 7.62 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P5-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-4_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:DO-214BA (layer B.Cu) (tedit 5ADEA4A5)
    (at 146.685 71.12)
    (descr "Microsemi LSM115J")
    (tags "DO-214BA diode")
    (attr smd)
    (fp_text reference D1 (at -10.795 -8.89) (layer B.SilkS))
    (fp_text value 1N5719 (at -11.43 -8.89) (layer B.Fab))
    (pad 2 smd rect (at 1.7 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 Sense))
    (pad 1 smd rect (at -1.7 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad1)"))
  )
  (module Diodes_SMD:DO-214BA (layer B.Cu) (tedit 5ADEA4A7)
    (at 146.685 66.675)
    (descr "Microsemi LSM115J")
    (tags "DO-214BA diode")
    (attr smd)
    (fp_text reference D2 (at -9.525 -5.08) (layer B.SilkS))
    (fp_text value 1N5719 (at -10.16 -4.445) (layer B.Fab))
    (pad 2 smd rect (at 1.7 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 Switched))
    (pad 1 smd rect (at -1.7 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5ADEA8D2)
    (at 162.56 67.945)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at -24.765 -5.08) (layer F.SilkS))
    (fp_text value MountingHole_3mm (at -26.035 -5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (gr_text 2018-04-23 (at 146.685 71.755) (layer F.SilkS))
  (gr_text "Be good humans." (at 154.305 81.28) (layer B.SilkS))
  (gr_text O (at 135.89 78.105) (layer B.Mask))
  (gr_text o (at 136.525 81.28) (layer B.Mask))
  (gr_text o (at 137.795 79.375) (layer B.Mask))
  (gr_text <>< (at 136.525 83.82) (layer B.Mask))
  (gr_text ><> (at 138.43 82.55) (layer B.Mask))
  (gr_text "CC NC-BY-SA" (at 146.685 69.85) (layer F.SilkS))
  (gr_text @SmittyHalibut (at 146.685 67.945) (layer F.SilkS))
  (gr_text "Car Power v1.0a" (at 146.685 66.04) (layer F.SilkS))
  (gr_text + (at 163.83 82.55) (layer F.SilkS))
  (gr_text - (at 161.29 82.55) (layer F.SilkS))
  (gr_text + (at 153.67 82.55) (layer F.SilkS))
  (gr_text - (at 151.13 82.55) (layer F.SilkS))
  (gr_text + (at 143.51 82.55) (layer F.SilkS))
  (gr_text - (at 140.97 82.55) (layer F.SilkS))
  (gr_line (start 129.54 85.09) (end 129.54 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 85.09) (end 166.37 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 1N5817 (at 149.86 71.12) (layer B.SilkS))
  (gr_text 1N5817 (at 149.86 66.675) (layer B.SilkS))
  (gr_text FQP27P06 (at 134.62 77.47) (layer F.SilkS))
  (gr_text Swchd (at 135.89 66.675) (layer F.SilkS))
  (gr_text Gnd (at 135.89 69.215) (layer F.SilkS))
  (gr_text Input (at 135.89 84.455) (layer F.SilkS))
  (gr_text Gnd (at 135.89 81.915) (layer F.SilkS))
  (gr_text Batt (at 135.89 79.375) (layer F.SilkS))
  (gr_text Shutdown (at 162.56 81.915) (layer F.SilkS))
  (gr_text "Always On" (at 152.4 81.28) (layer F.SilkS))
  (gr_text LED (at 142.24 81.28) (layer F.SilkS))
  (gr_line (start 129.54 85.09) (end 129.54 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 86.36) (end 129.54 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 64.77) (end 166.37 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 64.77) (end 166.37 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.54 64.77) (xy 166.37 64.77) (xy 166.37 86.36) (xy 129.54 86.36)
      )
    )
  )
)
