(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J2-Pad3)")
  (net 8 "Net-(J2-Pad4)")
  (net 9 "Net-(J3-Pad1)")
  (net 10 "Net-(J3-Pad2)")
  (net 11 "Net-(J3-Pad3)")
  (net 12 "Net-(J3-Pad4)")
  (net 13 "unconnected-(U2-Pad4)")
  (net 14 "unconnected-(U2-Pad12)")
  (net 15 "unconnected-(U2-Pad13)")
  (net 16 "unconnected-(U2-Pad14)")
  (net 17 "unconnected-(U2-Pad15)")
  (net 18 "unconnected-(U2-Pad16)")
  (net 19 "unconnected-(U3-Pad2)")
  (net 20 "unconnected-(U3-Pad5)")
  (net 21 "unconnected-(U3-Pad7)")
  (footprint "SHT45-AD1B-R2:SHT4X" (layer "F.Cu")
    (tedit 63BE628E)
    (at 107.15 100.5)
    (descr "Consumer SHT4x Digital and Analog")
    (property "Sheetfile" "AirspeedProbe_Feb23_a.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -0.4 -1.45) (layer "F.SilkS"))
    (fp_text value "SHT45-AD1B-R2" (at 1.875 1.665) (layer "F.Fab"))
    (pad "1" smd rect (at -0.7 -0.4) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(J2-Pad3)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "2" smd rect (at -0.7 0.4) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J2-Pad4)") (pinfunction "SCL") (pintype "input"))
    (pad "3" smd rect (at 0.7 0.4) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(J2-Pad2)") (pinfunction "VDD") (pintype "power_in"))
    (pad "4" smd rect (at 0.7 -0.4) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J2-Pad1)") (pinfunction "VSS") (pintype "power_in"))
    (model "${KICAD_USER_3DMODELS}/SHT45-AD1B-R2.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.3 96.86 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "AirspeedProbe_Feb23_a.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.3 104.16 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "AirspeedProbe_Feb23_a.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -0.01 -1.95 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DPS310:XDCR_DPS310" (layer "F.Cu")
    (tedit 63BE7807)
    (at 95.5 100.5 180)
    (property "AVAILABILITY" "Unavailable")
    (property "DESCRIPTION" "Supply voltage range 1.7V to 3.6V | Operation range 300hPa 1200hPa | Sensors precision 0.005hPa | Relative accuracy 0.06hPa | Pressure temperature sensitivity of 0.5Pa/K | Temperature accuracy 0.5C")
    (property "MF" "Infineon")
    (property "MP" "DPS310XTSA1")
    (property "PACKAGE" "LGA-8 Infineon")
    (property "PRICE" "None")
    (property "Sheetfile" "AirspeedProbe_Feb23_a.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 1.1 -2.2) (layer "F.SilkS"))
    (fp_text value "DPS310" (at 2.4704 2.1064) (layer "F.Fab"))
    (pad "1" smd rect (at 0.725 -0.975 180) (size 0.35 0.35) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(J3-Pad1)") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at 0.725 -0.325 180) (size 0.35 0.35) (layers "F.Cu" "F.Mask")
      (net 19 "unconnected-(U3-Pad2)") (pinfunction "CSB") (pintype "input"))
    (pad "3" smd rect (at 0.725 0.325 180) (size 0.35 0.35) (layers "F.Cu" "F.Mask")
      (net 11 "Net-(J3-Pad3)") (pinfunction "SDI") (pintype "bidirectional"))
    (pad "4" smd rect (at 0.725 0.975 180) (size 0.35 0.35) (layers "F.Cu" "F.Mask")
      (net 12 "Net-(J3-Pad4)") (pinfunction "SCK") (pintype "input"))
    (pad "5" smd rect (at -0.725 0.975 180) (size 0.35 0.35) (layers "F.Cu" "F.Mask")
      (net 20 "unconnected-(U3-Pad5)") (pinfunction "SDO") (pintype "output"))
    (pad "6" smd rect (at -0.725 0.325 180) (size 0.35 0.35) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(J3-Pad2)") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "7" smd rect (at -0.725 -0.325 180) (size 0.35 0.35) (layers "F.Cu" "F.Mask")
      (net 21 "unconnected-(U3-Pad7)") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect (at -0.725 -0.975 180) (size 0.35 0.35) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(J3-Pad2)") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD_USER_3DMODELS}/DPS310.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 124.3 100.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "AirspeedProbe_Feb23_a.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 1.95 90) (layer "F.SilkS"))
    (fp_text value "0.1" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SPD31:SDP3x_corrected" (layer "F.Cu")
    (tedit 0)
    (at 119.98 100.49 90)
    (property "AVAILABILITY" "")
    (property "DESCRIPTION" "")
    (property "MF" "")
    (property "MP" "")
    (property "PACKAGE" "")
    (property "PRICE" "")
    (property "Sheetfile" "AirspeedProbe_Feb23_a.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 4.79 -0.03 unlocked) (layer "F.SilkS"))
    (fp_text value "SDP31-500PA" (at -0.01 6.77 90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 2.825 1 90) (size 0.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 2 "Net-(C1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at 2.825 0 90) (size 0.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 2 "Net-(C1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at 2.825 -1 90) (size 0.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 2 "Net-(C1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at 2 -2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 13 "unconnected-(U2-Pad4)") (pinfunction "IRQ") (pintype "input"))
    (pad "5" smd roundrect (at 1 -2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 4 "Net-(J1-Pad4)") (pinfunction "SCL") (pintype "input"))
    (pad "6" smd roundrect (at 0 -2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 2 "Net-(C1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd roundrect (at -1 -2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 1 "Net-(C1-Pad1)") (pinfunction "VDD") (pintype "power_in"))
    (pad "8" smd roundrect (at -2 -2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 3 "Net-(J1-Pad3)") (pinfunction "SDA") (pintype "input"))
    (pad "9" smd roundrect (at -2.825 -1 90) (size 0.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 2 "Net-(C1-Pad2)") (pinfunction "ADDR") (pintype "input"))
    (pad "10" smd roundrect (at -2.825 0 90) (size 0.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 2 "Net-(C1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd roundrect (at -2.825 1 90) (size 0.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "12" smd roundrect (at -2 2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 14 "unconnected-(U2-Pad12)") (pinfunction "NC") (pintype "no_connect"))
    (pad "13" smd roundrect (at -1 2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 15 "unconnected-(U2-Pad13)") (pinfunction "NC") (pintype "no_connect"))
    (pad "14" smd roundrect (at 0 2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 16 "unconnected-(U2-Pad14)") (pinfunction "NC") (pintype "no_connect"))
    (pad "15" smd roundrect (at 1 2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 17 "unconnected-(U2-Pad15)") (pinfunction "NC") (pintype "no_connect"))
    (pad "16" smd roundrect (at 2 2.075 90) (size 0.4 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 18 "unconnected-(U2-Pad16)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD_USER_3DMODELS}/SDP31.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 114.55 102.405 180)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (property "Sheetfile" "AirspeedProbe_Feb23_a.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -1.95) (layer "F.SilkS") hide)
    (fp_text value " " (at 0 9.35) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.905 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 111.75 98.595)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (property "Sheetfile" "AirspeedProbe_Feb23_a.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -1.745) (layer "F.SilkS"))
    (fp_text value "Connector" (at 0 5.505) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 103.95 102.405 180)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (property "Sheetfile" "AirspeedProbe_Feb23_a.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -1.95) (layer "F.SilkS"))
    (fp_text value "Connector" (at 0 5.505) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 112.48 97.58) (end 112.48 99.98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 112.48 100.98) (end 113.8 100.98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.04 106.4) (end 116.04 103.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 114.3 103.5) (end 113.8 102.99) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.25 97.98) (end 110.25 97.58) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 105.23 100.515) (end 105.48 100.515) (layer "Edge.Cuts") (width 0.1) (fill solid))
  (gr_line (start 104.685 98.015) (end 104.685 100.015) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 119.98 100.49) (end 119.98 100.49) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_line (start 113.8 97.99) (end 113.8 99.98) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 122.13 104.14) (end 122.13 104.14) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_line (start 113.8 97.99) (end 114.3 97.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105.78 102.98) (end 105.78 101.015) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.04 106.4) (end 125.44 106.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.04 97.5) (end 114.3 97.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 104.685 103.015) (end 104.185 103.505) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 113.8 102.99) (end 113.8 100.98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 112.48 103.38) (end 112.48 100.98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.04 103.5) (end 114.3 103.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 104.185 103.505) (end 93.505 103.505) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.04 94.6) (end 116.04 97.5) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 117.83 104.14) (end 118.18 104.14) (layer "Edge.Cuts") (width 0.1) (fill solid))
  (gr_line (start 110.25 102.98) (end 105.78 102.98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 125.44 94.6) (end 116.04 94.6) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 104.685 101.015) (end 105.78 101.015) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 117.83 96.84) (end 118.18 96.84) (layer "Edge.Cuts") (width 0.1) (fill solid))
  (gr_line (start 105.78 97.98) (end 105.78 100.015) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 113.14 100.48) (end 113.39 100.48) (layer "Edge.Cuts") (width 0.1) (fill solid))
  (gr_line (start 104.685 100.015) (end 105.78 100.015) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.25 103.38) (end 112.48 103.38) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.25 97.98) (end 105.78 97.98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.25 102.98) (end 110.25 103.38) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 93.505 97.505) (end 104.185 97.505) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 112.48 99.98) (end 113.8 99.98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 104.685 103.015) (end 104.685 101.015) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 125.44 106.4) (end 125.44 94.6) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 122.13 104.14) (end 122.48 104.14) (layer "Edge.Cuts") (width 0.1) (fill solid))
  (gr_line (start 93.505 97.505) (end 93.505 103.505) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.25 97.58) (end 112.48 97.58) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 104.185 97.505) (end 104.685 98.015) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 119.98 100.49) (end 120.28 100.49) (layer "Edge.Cuts") (width 0.1) (fill solid))
  (gr_text "L" (at 119.15 102.15) (layer "User.1"))
  (gr_text "H" (at 119.15 98.9) (layer "User.1"))
)
