(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "/Users/ramona/Documents/POVideo/povideo-gerbers/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "LED_DATA")
	(net 3 "+3.3V")
	(net 4 "Net-(R3-Pad1)")
	(net 5 "Net-(R4-Pad1)")
	(net 6 "COL1")
	(net 7 "Net-(D14-A)")
	(net 8 "COL2")
	(net 9 "Net-(D15-A)")
	(net 10 "Net-(D16-A)")
	(net 11 "COL3")
	(net 12 "Net-(D17-A)")
	(net 13 "Net-(D18-A)")
	(net 14 "Net-(D19-A)")
	(net 15 "COL4")
	(net 16 "Net-(D20-A)")
	(net 17 "Net-(D21-A)")
	(net 18 "COL5")
	(net 19 "Net-(D22-A)")
	(net 20 "Net-(D23-A)")
	(net 21 "Net-(D24-A)")
	(net 22 "Net-(D25-A)")
	(net 23 "Net-(D26-A)")
	(net 24 "Net-(D27-A)")
	(net 25 "Net-(D28-A)")
	(net 26 "Net-(D29-A)")
	(net 27 "Net-(D30-A)")
	(net 28 "Net-(D31-A)")
	(net 29 "MOSI")
	(net 30 "CS")
	(net 31 "SCK")
	(net 32 "Net-(J2-Pin_5)")
	(net 33 "unconnected-(J2-Pin_2-Pad2)")
	(net 34 "Net-(J2-Pin_1)")
	(net 35 "unconnected-(J2-Pin_4-Pad4)")
	(net 36 "unconnected-(J3-Pin_4-Pad4)")
	(net 37 "unconnected-(J3-Pin_2-Pad2)")
	(net 38 "SYNC")
	(net 39 "POT A")
	(net 40 "POT B")
	(net 41 "ROW1")
	(net 42 "ROW2")
	(net 43 "ROW3")
	(net 44 "ROW4")
	(net 45 "unconnected-(U1-MISO{slash}GPIO20-Pad13)")
	(net 46 "unconnected-(U1-RESET-Pad1)")
	(net 47 "unconnected-(U1-3.3V-Pad3)")
	(net 48 "unconnected-(U1-A3{slash}GPIO29-Pad8)")
	(net 49 "unconnected-(U1-A2{slash}GPIO28-Pad7)")
	(net 50 "unconnected-(U1-VBat-Pad28)")
	(net 51 "unconnected-(U1-D24{slash}GPIO24-Pad9)")
	(net 52 "unconnected-(U1-Vbus-Pad26)")
	(net 53 "unconnected-(U1-TX{slash}GPIO0-Pad15)")
	(net 54 "unconnected-(J1-Pin_2-Pad2)")
	(net 55 "unconnected-(J1-Pin_8-Pad8)")
	(net 56 "unconnected-(J1-Pin_7-Pad7)")
	(net 57 "unconnected-(J1-Pin_9-Pad9)")
	(net 58 "unconnected-(SW19-A-Pad1)")
	(net 59 "Net-(SW19-B)")
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 180.1 90.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D24"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "COL3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(D24-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 195.1 86.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D21"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "COL5")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D21-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 175 112.3 90)
		(property "Reference" "SW3"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 41 "ROW1")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 41 "ROW1")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 10 "Net-(D16-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 10 "Net-(D16-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 172.6 94.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D28"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "COL2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(D28-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:Adafruit Potentiometer"
		(layer "F.Cu")
		(at 186 112.3 180)
		(descr "10k linear pot PID 4133")
		(property "Reference" "RV1"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_Potentiometer"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at -2.5 6.5 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net 3 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 0 6.5 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net 4 "Net-(R3-Pad1)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 2.5 6.5 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at -4 0 180)
			(size 3 3)
			(drill 2.1)
			(layers "*.Cu" "*.Mask" "Dwgs.User")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
		)
		(pad "5" thru_hole roundrect
			(at 4 0 180)
			(size 3 3)
			(drill 2.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 172.6 82.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D15"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "COL2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D15-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 175 124.8 90)
		(property "Reference" "SW6"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 14 "Net-(D19-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 14 "Net-(D19-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 195.1 90.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D26"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "COL5")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(D26-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 164 112.3 90)
		(property "Reference" "SW2"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 41 "ROW1")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 41 "ROW1")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 9 "Net-(D15-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 9 "Net-(D15-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 186 137.3 90)
		(property "Reference" "SW12"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 22 "Net-(D25-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 22 "Net-(D25-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 153 124.8 90)
		(property "Reference" "SW4"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 12 "Net-(D17-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 12 "Net-(D17-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 175 149.8 90)
		(property "Reference" "SW16"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 26 "Net-(D29-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 26 "Net-(D29-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 192.73 82.25)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -0.02 -1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "15uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "POT A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 187.6 94.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D30"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "COL4")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(D30-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 172.6 86.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D18"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "COL2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D18-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 153 149.8 90)
		(property "Reference" "SW14"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 24 "Net-(D27-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 24 "Net-(D27-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 154.76 63 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "SYNC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(J2-Pin_5)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 186 124.8 90)
		(property "Reference" "SW7"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 16 "Net-(D20-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 16 "Net-(D20-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 164 124.8 90)
		(property "Reference" "SW5"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 13 "Net-(D18-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 13 "Net-(D18-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 153 112.3 90)
		(property "Reference" "SW1"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 41 "ROW1")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 41 "ROW1")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 7 "Net-(D14-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 7 "Net-(D14-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 153 137.3 90)
		(property "Reference" "SW9"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 19 "Net-(D22-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 19 "Net-(D22-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:Adafruit Potentiometer"
		(layer "F.Cu")
		(at 197 112.3 180)
		(descr "10k linear pot PID 4133")
		(property "Reference" "RV2"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_Potentiometer"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at -2.5 6.5 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net 3 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 0 6.5 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net 5 "Net-(R4-Pad1)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at 2.5 6.5 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at -4 0 180)
			(size 3 3)
			(drill 2.1)
			(layers "*.Cu" "*.Mask" "Dwgs.User")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
		)
		(pad "5" thru_hole roundrect
			(at 4 0 180)
			(size 3 3)
			(drill 2.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 197 149.8 90)
		(property "Reference" "SW18"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 28 "Net-(D31-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 28 "Net-(D31-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 197 137.3 90)
		(property "Reference" "SW13"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 23 "Net-(D26-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 23 "Net-(D26-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 189.99 82.25)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(R3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "POT A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 165.1 94.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D27"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "COL1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(D27-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 186 149.8 90)
		(property "Reference" "SW17"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 27 "Net-(D30-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 27 "Net-(D30-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 164.85 57.5 90)
		(descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x09 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x05_Socket"
			(at 0 22.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x09, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(J1-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "SCK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.15 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "MOSI")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "CS")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(J1-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(J1-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(J1-Pin_9-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 180.1 82.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D16"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "COL3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D16-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 197.98 82.25)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "15uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "POT B")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 187.6 86.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D20"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "COL4")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D20-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 175 137.3 90)
		(property "Reference" "SW11"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 21 "Net-(D24-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 21 "Net-(D24-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 187.6 90.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D25"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "COL4")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(D25-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 172.6 90.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D23"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "COL2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(D23-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 180.1 94.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D29"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "COL3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(D29-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 165.1 86.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D17"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "COL1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D17-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 157.51 63 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "SYNC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 165.1 82.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D14"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "COL1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D14-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 195.1 94.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D31"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "COL5")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(D31-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 164 137.3 90)
		(property "Reference" "SW10"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 43 "ROW3")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 20 "Net-(D23-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 20 "Net-(D23-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 195.51 82.25)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(R4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "POT B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 197 124.8 90)
		(property "Reference" "SW8"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "ROW2")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 17 "Net-(D21-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 17 "Net-(D21-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 165.1 90.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D22"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "COL1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(D22-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:TL3301 6mm tactile switch"
		(layer "F.Cu")
		(at 164 149.8 90)
		(property "Reference" "SW15"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd roundrect
			(at 4.55 2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 44 "ROW4")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 25 "Net-(D28-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.55 -2.25 90)
			(size 2.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 25 "Net-(D28-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 180.1 86.5)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D19"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_45deg"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, rotated by 45°"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "COL3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D19-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ramona Library:Right Angle Slide Switch"
		(layer "B.Cu")
		(at 149.55 100.25 -90)
		(property "Reference" "SW19"
			(at 0 3.55 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "SW_SPST"
			(at -2.5 4 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 270)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(SW19-A-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(SW19-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.5 0 270)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:5 pin headphone jack"
		(layer "B.Cu")
		(at 201.75 68 -90)
		(property "Reference" "J3"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x05_Socket"
			(at 0 -1 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -5 2.5 270)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.5 2.5 270)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(J3-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 -2.5 270)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.5 2.5 270)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(J3-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 5 2.5 270)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J2-Pin_1)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Ramona Library:5 pin headphone jack"
		(layer "B.Cu")
		(at 148.25 68 90)
		(property "Reference" "J2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x05_Socket"
			(at 0 -1 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -5 2.5 90)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.5 2.5 90)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(J2-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 -2.5 90)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.5 2.5 90)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(J2-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 5 2.5 90)
			(size 2.1 2.1)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Module:Adafruit_Feather"
		(layer "B.Cu")
		(at 155.4 78 -90)
		(descr "Common footprint for the Adafruit Feather series of boards, https://learn.adafruit.com/adafruit-feather/feather-specification")
		(tags "Adafruit Feather")
		(property "Reference" "U1"
			(at 10.16 7.62 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Adafruit-Feather-RP2040"
			(at -2.25 -21.85 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "POVideo V2.kicad_sch")
		(clearance 0.2)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 -19.05 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 46 "unconnected-(U1-RESET-Pad1)")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3.3V")
			(pinfunction "3.3V")
			(pintype "power_out")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(U1-3.3V-Pad3)")
			(pinfunction "3.3V")
			(pintype "power_out")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "POT A")
			(pinfunction "A0/GPIO26")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "POT B")
			(pinfunction "A1/GPIO27")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(U1-A2{slash}GPIO28-Pad7)")
			(pinfunction "A2/GPIO28")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(U1-A3{slash}GPIO29-Pad8)")
			(pinfunction "A3/GPIO29")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at 0 -20.32 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(U1-D24{slash}GPIO24-Pad9)")
			(pinfunction "D24/GPIO24")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at 0 -22.86 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "SYNC")
			(pinfunction "D25/GPIO25")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at 0 -25.4 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "SCK")
			(pinfunction "SCK/GPIO18")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole oval
			(at 0 -27.94 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "MOSI")
			(pinfunction "MOSI/GPIO19")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole oval
			(at 0 -30.48 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(U1-MISO{slash}GPIO20-Pad13)")
			(pinfunction "MISO/GPIO20")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole oval
			(at 0 -33.02 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "CS")
			(pinfunction "RX/CS/GPIO1")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole oval
			(at 0 -35.56 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(U1-TX{slash}GPIO0-Pad15)")
			(pinfunction "TX/GPIO0")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole oval
			(at 0 -38.1 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "LED_DATA")
			(pinfunction "D4/GPIO6")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole oval
			(at 20.32 -38.1 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "COL5")
			(pinfunction "SDA/GPIO2")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole oval
			(at 20.32 -35.56 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "COL4")
			(pinfunction "SCL/GPIO3")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole oval
			(at 20.32 -33.02 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "COL3")
			(pinfunction "D5/GPIO7")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole oval
			(at 20.32 -30.48 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "COL2")
			(pinfunction "D6/GPIO8")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole oval
			(at 20.32 -27.94 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "COL1")
			(pinfunction "D9/GPIO9")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 20.32 -25.4 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "ROW4")
			(pinfunction "D10/GPIO10")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole oval
			(at 20.32 -22.86 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "ROW3")
			(pinfunction "D11/GPIO11")
			(pintype "bidirectional")
		)
		(pad "24" thru_hole oval
			(at 20.32 -20.32 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "ROW2")
			(pinfunction "D12/GPIO12")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole oval
			(at 20.32 -17.78 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "ROW1")
			(pinfunction "D13/GPIO13")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole oval
			(at 20.32 -15.24 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(U1-Vbus-Pad26)")
			(pinfunction "Vbus")
			(pintype "power_out")
		)
		(pad "27" thru_hole oval
			(at 20.32 -12.7 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(SW19-B)")
			(pinfunction "ENABLE")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 20.32 -10.16 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(U1-VBat-Pad28)")
			(pinfunction "VBat")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/Adafruit_Feather.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 188.5 41.5)
		(mid 191.5 44.5)
		(end 188.5 47.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 161.5 47.5)
		(mid 158.5 44.5)
		(end 161.5 41.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 205 158)
		(mid 204.414214 159.414214)
		(end 203 160)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 143.25 57.5)
		(mid 143.982233 55.732233)
		(end 145.75 55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 147 160)
		(mid 145.585786 159.414214)
		(end 145 158)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.5 55)
		(end 145.75 55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.5 55)
		(end 204.25 55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 161.5 53)
		(mid 153 44.5)
		(end 161.5 36)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.5 55)
		(end 167.5 55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.5 36)
		(end 161.5 36)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 182.5 53)
		(mid 183.5 54)
		(end 182.5 55)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 188.5 36)
		(mid 197 44.5)
		(end 188.5 53)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 164.5 53)
		(mid 165.5 54)
		(end 164.5 55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147 160)
		(end 203 160)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.5 53)
		(end 167.5 53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205 111)
		(end 205.029751 110.875287)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 164.5 53)
		(end 161.5 53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 206.75 57.5)
		(end 206.75 108.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.5 47.5)
		(end 188.5 47.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.5 53)
		(end 188.5 53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145 111)
		(end 144.959431 110.871707)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172 41.5)
		(end 161.5 41.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 167.5 55)
		(mid 166.5 54)
		(end 167.5 53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145 112.5)
		(end 145 111)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.25 57.5)
		(end 143.25 108.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 204.25 55)
		(mid 206.017767 55.732233)
		(end 206.75 57.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145 158)
		(end 145 112.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.5 55)
		(mid 184.5 54)
		(end 185.5 53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 178 41.5)
		(end 188.5 41.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205 112.5)
		(end 205 111)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.959431 110.871708)
		(mid 143.721895 109.961776)
		(end 143.25 108.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172 41.5)
		(mid 175 38.5)
		(end 178 41.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205 158)
		(end 205 112.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 206.75 108.5)
		(mid 206.274769 109.966394)
		(end 205.02975 110.875287)
		(layer "Edge.Cuts")
	)
	(gr_text "1"
		(at 152.25 143 0)
		(layer "F.SilkS")
	)
	(gr_text "B"
		(at 196.25 118.25 0)
		(layer "F.SilkS")
	)
	(gr_text "3\n"
		(at 174.25 143 0)
		(layer "F.SilkS")
	)
	(gr_text "#PO10DIY by RMNA"
		(at 162 51.25 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 185.25 143 0)
		(layer "F.SilkS")
	)
	(gr_text "!"
		(at 152.5 130.5 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 185.25 155.5 0)
		(layer "F.SilkS")
	)
	(gr_text "A"
		(at 185.25 118.25 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 163.25 143 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 163.25 155.5 0)
		(layer "F.SilkS")
	)
	(gr_text "!!!"
		(at 173.9 130.5 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 174.25 155.5 0)
		(layer "F.SilkS")
	)
	(gr_text "FX"
		(at 195.5 130.25 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 152.25 155.5 0)
		(layer "F.SilkS")
	)
	(gr_text "!!"
		(at 163.25 130.5 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 143.25 55) (xy 143.25 160) (xy 206.75 160) (xy 206.75 55)
			)
		)
	)
	(embedded_fonts no)
)
