<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>GND</text>
<text>Vcc</text>
<text>H</text>
<text>L</text>
<text>IN</text>
<text>GND</text>
<text>IN</text>
<text>L</text>
<text>H</text>
<text>Vcc</text>
<text>Darker</text>
<text>Darker</text>
<wire x1="0.375" y1="0" x2="0.375" y2="5.6" width="0" layer="20"/>
<wire x1="0.375" y1="5.6" x2="0" y2="5.6" width="0" layer="20"/>
<wire x1="0" y1="5.6" x2="0" y2="14.4" width="0" layer="20"/>
<wire x1="0" y1="14.4" x2="0.375" y2="14.4" width="0" layer="20"/>
<wire x1="0.375" y1="14.4" x2="0.375" y2="20" width="0" layer="20"/>
<wire x1="0.375" y1="20" x2="9.625" y2="20" width="0" layer="20"/>
<wire x1="9.625" y1="20" x2="9.625" y2="14.4" width="0" layer="20"/>
<wire x1="9.625" y1="14.4" x2="10" y2="14.4" width="0" layer="20"/>
<wire x1="10" y1="14.4" x2="10" y2="5.6" width="0" layer="20"/>
<wire x1="10" y1="5.6" x2="9.625" y2="5.6" width="0" layer="20"/>
<wire x1="9.625" y1="5.6" x2="9.625" y2="0" width="0" layer="20"/>
<wire x1="9.625" y1="0" x2="0.375" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="BUK9Y107-80E">
<packages>
<package name="SO8">
</package>
</packages>
</library>
<library name="CoinKit">
<packages>
<package name="FINGERS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$15" library="BUK9Y107-80E" package="SO8" value="BUK9Y1O7-80E">
<attribute name="VGS" value="+/-10Constant, +/-15 pulsed"/>
<attribute name="PTOT" value="37W"/>
<attribute name="ID" value="11.8A"/>
<attribute name="IMAX" value="47A (pulsed)"/>
<attribute name="QGD" value="2.5nC"/>
<attribute name="VDS" value="80V"/>
</element>
<element name="U$16" library="BUK9Y107-80E" package="SO8" value="BUK9Y1O7-80E">
<attribute name="VGS" value="+/-10Constant, +/-15 pulsed"/>
<attribute name="PTOT" value="37W"/>
<attribute name="ID" value="11.8A"/>
<attribute name="IMAX" value="47A (pulsed)"/>
<attribute name="QGD" value="2.5nC"/>
<attribute name="VDS" value="80V"/>
</element>
<element name="U$2" library="BUK9Y107-80E" package="SO8" value="BUK9Y1O7-80E">
<attribute name="VGS" value="+/-10Constant, +/-15 pulsed"/>
<attribute name="PTOT" value="37W"/>
<attribute name="ID" value="11.8A"/>
<attribute name="IMAX" value="47A (pulsed)"/>
<attribute name="QGD" value="2.5nC"/>
<attribute name="VDS" value="80V"/>
</element>
<element name="U$3" library="BUK9Y107-80E" package="SO8" value="BUK9Y1O7-80E">
<attribute name="VGS" value="+/-10Constant, +/-15 pulsed"/>
<attribute name="PTOT" value="37W"/>
<attribute name="ID" value="11.8A"/>
<attribute name="IMAX" value="47A (pulsed)"/>
<attribute name="QGD" value="2.5nC"/>
<attribute name="VDS" value="80V"/>
</element>
<element name="U$33" library="CoinKit" package="FINGERS" value="PCI-10"/>
<element name="U$34" library="CoinKit" package="FINGERS" value="PCI-10"/>
</elements>
<signals>
<signal name="HIGH2">
<contactref element="U$2" pad="GATE"/>
<contactref element="U$34" pad="6A"/>
</signal>
<signal name="HIGH1">
<contactref element="U$15" pad="GATE"/>
<contactref element="U$34" pad="6B"/>
</signal>
<signal name="GND">
<contactref element="U$34" pad="1A"/>
<contactref element="U$34" pad="3A"/>
<contactref element="U$34" pad="2A"/>
<contactref element="U$3" pad="SOURCE1"/>
<contactref element="U$3" pad="SOURCE2"/>
<contactref element="U$3" pad="SOURCE3"/>
</signal>
<signal name="LOW1">
<contactref element="U$16" pad="GATE"/>
<contactref element="U$34" pad="5B"/>
</signal>
<signal name="LOW2">
<contactref element="U$3" pad="GATE"/>
<contactref element="U$34" pad="5A"/>
</signal>
<signal name="LOAD2">
<contactref element="U$2" pad="SOURCE1"/>
<contactref element="U$2" pad="SOURCE2"/>
<contactref element="U$2" pad="SOURCE3"/>
<contactref element="U$3" pad="DRAIN"/>
<contactref element="U$3" pad="DRAIN2"/>
<contactref element="U$33" pad="1A"/>
<contactref element="U$34" pad="4A"/>
<contactref element="U$33" pad="2A"/>
<contactref element="U$33" pad="3A"/>
<contactref element="U$33" pad="4A"/>
<contactref element="U$33" pad="5A"/>
<contactref element="U$33" pad="6A"/>
<contactref element="U$33" pad="7A"/>
<contactref element="U$33" pad="8A"/>
<contactref element="U$33" pad="9A"/>
</signal>
<signal name="LOAD1">
<contactref element="U$15" pad="SOURCE1"/>
<contactref element="U$15" pad="SOURCE2"/>
<contactref element="U$15" pad="SOURCE3"/>
<contactref element="U$16" pad="DRAIN"/>
<contactref element="U$16" pad="DRAIN2"/>
<contactref element="U$33" pad="1B"/>
<contactref element="U$34" pad="4B"/>
<contactref element="U$33" pad="2B"/>
<contactref element="U$33" pad="3B"/>
<contactref element="U$33" pad="4B"/>
<contactref element="U$33" pad="5B"/>
<contactref element="U$33" pad="6B"/>
<contactref element="U$33" pad="7B"/>
<contactref element="U$33" pad="8B"/>
<contactref element="U$33" pad="9B"/>
</signal>
<signal name="VCC">
<contactref element="U$15" pad="DRAIN"/>
<contactref element="U$15" pad="DRAIN2"/>
<contactref element="U$34" pad="9B"/>
<contactref element="U$34" pad="8B"/>
<contactref element="U$34" pad="7B"/>
</signal>
<signal name="VCC2">
<contactref element="U$2" pad="DRAIN"/>
<contactref element="U$2" pad="DRAIN2"/>
<contactref element="U$34" pad="9A"/>
<contactref element="U$34" pad="8A"/>
<contactref element="U$34" pad="7A"/>
</signal>
<signal name="GND2">
<contactref element="U$34" pad="3B"/>
<contactref element="U$34" pad="2B"/>
<contactref element="U$34" pad="1B"/>
<contactref element="U$16" pad="SOURCE1"/>
<contactref element="U$16" pad="SOURCE2"/>
<contactref element="U$16" pad="SOURCE3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
