(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/Battery unit8/V_batt+12V")
  (net 2 "GND")
  (net 3 "/Battery unit/V_batt-")
  (net 4 "/Battery unit/V_batt+12V")
  (net 5 "/Battery unit1/V_batt-")
  (net 6 "/Battery unit2/V_batt-")
  (net 7 "/Battery unit3/V_batt-")
  (net 8 "Net-(JP201-Pad3)")
  (net 9 "Net-(R201-Pad2)")
  (net 10 "Net-(JP301-Pad3)")
  (net 11 "Net-(R301-Pad2)")
  (net 12 "Net-(JP401-Pad3)")
  (net 13 "Net-(R401-Pad2)")
  (net 14 "Net-(JP501-Pad3)")
  (net 15 "Net-(R501-Pad2)")
  (net 16 "unconnected-(U201-PadMH1)")
  (net 17 "unconnected-(U301-PadMH1)")
  (net 18 "unconnected-(U401-PadMH1)")
  (net 19 "unconnected-(U501-PadMH1)")
  (net 20 "Net-(JP601-Pad3)")
  (net 21 "Net-(R601-Pad2)")
  (net 22 "unconnected-(U601-PadMH1)")
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.025 42.545 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit8")
    (attr smd)
    (fp_text reference "R601" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "120k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 20 "Net-(JP601-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 21 "Net-(R601-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 72.75 106.045 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit2")
    (attr smd)
    (fp_text reference "R401" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "120k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 12 "Net-(JP401-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 13 "Net-(R401-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 127.635 149.86 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "Bias-Battery-Holder.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H101" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 90.175 36.195 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Bias-Battery-Holder.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J103" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Chain Out" (at 2.54 1.27 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/Battery unit8/V_batt+12V") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 72.75 116.825 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit2")
    (attr through_hole)
    (fp_text reference "JP401" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Bypass" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/Battery unit2/V_batt-") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/Battery unit1/V_batt-") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(JP401-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 73.025 53.96 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit8")
    (attr through_hole)
    (fp_text reference "JP601" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Bypass" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/Battery unit/V_batt+12V") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/Battery unit8/V_batt+12V") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(JP601-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "23A_Battery_Holder:Keystone-1018" (layer "F.Cu")
    (tedit 0)
    (at 102.51 51.435)
    (descr "1018-3")
    (tags "Undefined or Miscellaneous")
    (property "Description" "KEYSTONE - 1018 - BATTERY HOLDER, 2/3A CELL, SURFACE MT")
    (property "Height" "15.23")
    (property "Manufacturer_Name" "Keystone Electronics")
    (property "Manufacturer_Part_Number" "1018")
    (property "Mouser Part Number" "534-1018")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/1018?qs=%2F%252BPMR94VuMZseySUioSuqQ%3D%3D")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit8")
    (attr through_hole)
    (fp_text reference "U601" (at 0 -0.22) (layer "F.SilkS"))
    (fp_text value "Keystone-1018-SMD" (at 0 -0.22) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -0.22) (layer "F.Fab"))
    (pad "1" smd rect (at -22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(R601-Pad2)") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/Battery unit/V_batt+12V") (pinfunction "-") (pintype "passive"))
    (pad "MH1" thru_hole circle (at -18.83 -8.1) (size 2.97 2.97) (drill 1.98) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U601-PadMH1)") (pinfunction "MH1") (pintype "passive+no_connect"))
    (model "C:\\Users\\luitz\\OneDrive-luitz\\OneDrive\\Documents\\KiCAD\\LibraryLoader\\SamacSys_Parts.3dshapes\\1018.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132203-12_Horizontal" (layer "F.Cu")
    (tedit 5CF42CD6)
    (at 100.965 35.69)
    (descr "https://www.amphenolrf.com/media/downloads/1769/132203-12.pdf")
    (tags "SMA THT Female Jack Horizontal")
    (property "Sheetfile" "Bias-Battery-Holder.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J102" (at -5.2 0 90) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "/Battery unit8/V_batt+12V") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132203-12_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "23A_Battery_Holder:Keystone-1018" (layer "F.Cu")
    (tedit 0)
    (at 102.595 93.345)
    (descr "1018-3")
    (tags "Undefined or Miscellaneous")
    (property "Description" "KEYSTONE - 1018 - BATTERY HOLDER, 2/3A CELL, SURFACE MT")
    (property "Height" "15.23")
    (property "Manufacturer_Name" "Keystone Electronics")
    (property "Manufacturer_Part_Number" "1018")
    (property "Mouser Part Number" "534-1018")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/1018?qs=%2F%252BPMR94VuMZseySUioSuqQ%3D%3D")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit1")
    (attr through_hole)
    (fp_text reference "U301" (at 0 -0.22) (layer "F.SilkS"))
    (fp_text value "Keystone-1018-SMD" (at 0 -0.22) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -0.22) (layer "F.Fab"))
    (pad "1" smd rect (at -22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(R301-Pad2)") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/Battery unit1/V_batt-") (pinfunction "-") (pintype "passive"))
    (pad "MH1" thru_hole circle (at -18.83 -8.1) (size 2.97 2.97) (drill 1.98) (layers *.Cu *.Mask)
      (net 17 "unconnected-(U301-PadMH1)") (pinfunction "MH1") (pintype "passive+no_connect"))
    (model "C:\\Users\\luitz\\OneDrive-luitz\\OneDrive\\Documents\\KiCAD\\LibraryLoader\\SamacSys_Parts.3dshapes\\1018.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "23A_Battery_Holder:Keystone-1018" (layer "F.Cu")
    (tedit 0)
    (at 102.595 72.39)
    (descr "1018-3")
    (tags "Undefined or Miscellaneous")
    (property "Description" "KEYSTONE - 1018 - BATTERY HOLDER, 2/3A CELL, SURFACE MT")
    (property "Height" "15.23")
    (property "Manufacturer_Name" "Keystone Electronics")
    (property "Manufacturer_Part_Number" "1018")
    (property "Mouser Part Number" "534-1018")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/1018?qs=%2F%252BPMR94VuMZseySUioSuqQ%3D%3D")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit")
    (attr through_hole)
    (fp_text reference "U201" (at 0 -0.22) (layer "F.SilkS"))
    (fp_text value "Keystone-1018-SMD" (at 0 -0.22) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -0.22) (layer "F.Fab"))
    (pad "1" smd rect (at -22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(R201-Pad2)") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/Battery unit/V_batt-") (pinfunction "-") (pintype "passive"))
    (pad "MH1" thru_hole circle (at -18.83 -8.1) (size 2.97 2.97) (drill 1.98) (layers *.Cu *.Mask)
      (net 16 "unconnected-(U201-PadMH1)") (pinfunction "MH1") (pintype "passive+no_connect"))
    (model "C:\\Users\\luitz\\OneDrive-luitz\\OneDrive\\Documents\\KiCAD\\LibraryLoader\\SamacSys_Parts.3dshapes\\1018.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 73.025 34.29)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "Bias-Battery-Holder.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H104" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 109.22 34.285)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Bias-Battery-Holder.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J101" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "V_Test" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/Battery unit8/V_batt+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 72.75 95.87 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit1")
    (attr through_hole)
    (fp_text reference "JP301" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Bypass" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/Battery unit1/V_batt-") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/Battery unit/V_batt-") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(JP301-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 73.025 149.86)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "Bias-Battery-Holder.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H103" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 72.75 127 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit3")
    (attr smd)
    (fp_text reference "R501" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "120k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 14 "Net-(JP501-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 15 "Net-(R501-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 73.025 76.185 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit")
    (attr through_hole)
    (fp_text reference "JP201" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Bypass" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/Battery unit/V_batt-") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/Battery unit/V_batt+12V") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(JP201-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "23A_Battery_Holder:Keystone-1018" (layer "F.Cu")
    (tedit 0)
    (at 102.595 114.3)
    (descr "1018-3")
    (tags "Undefined or Miscellaneous")
    (property "Description" "KEYSTONE - 1018 - BATTERY HOLDER, 2/3A CELL, SURFACE MT")
    (property "Height" "15.23")
    (property "Manufacturer_Name" "Keystone Electronics")
    (property "Manufacturer_Part_Number" "1018")
    (property "Mouser Part Number" "534-1018")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/1018?qs=%2F%252BPMR94VuMZseySUioSuqQ%3D%3D")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit2")
    (attr through_hole)
    (fp_text reference "U401" (at 0 -0.22) (layer "F.SilkS"))
    (fp_text value "Keystone-1018-SMD" (at 0 -0.22) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -0.22) (layer "F.Fab"))
    (pad "1" smd rect (at -22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(R401-Pad2)") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/Battery unit2/V_batt-") (pinfunction "-") (pintype "passive"))
    (pad "MH1" thru_hole circle (at -18.83 -8.1) (size 2.97 2.97) (drill 1.98) (layers *.Cu *.Mask)
      (net 18 "unconnected-(U401-PadMH1)") (pinfunction "MH1") (pintype "passive+no_connect"))
    (model "C:\\Users\\luitz\\OneDrive-luitz\\OneDrive\\Documents\\KiCAD\\LibraryLoader\\SamacSys_Parts.3dshapes\\1018.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 72.75 85.09 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit1")
    (attr smd)
    (fp_text reference "R301" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "120k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 10 "Net-(JP301-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 11 "Net-(R301-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "23A_Battery_Holder:Keystone-1018" (layer "F.Cu")
    (tedit 0)
    (at 102.51 135.255)
    (descr "1018-3")
    (tags "Undefined or Miscellaneous")
    (property "Description" "KEYSTONE - 1018 - BATTERY HOLDER, 2/3A CELL, SURFACE MT")
    (property "Height" "15.23")
    (property "Manufacturer_Name" "Keystone Electronics")
    (property "Manufacturer_Part_Number" "1018")
    (property "Mouser Part Number" "534-1018")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/1018?qs=%2F%252BPMR94VuMZseySUioSuqQ%3D%3D")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit3")
    (attr through_hole)
    (fp_text reference "U501" (at 0 -0.22) (layer "F.SilkS"))
    (fp_text value "Keystone-1018-SMD" (at 0 -0.22) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -0.22) (layer "F.Fab"))
    (pad "1" smd rect (at -22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(R501-Pad2)") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 22.5 0 90) (size 6.35 7.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/Battery unit3/V_batt-") (pinfunction "-") (pintype "passive"))
    (pad "MH1" thru_hole circle (at -18.83 -8.1) (size 2.97 2.97) (drill 1.98) (layers *.Cu *.Mask)
      (net 19 "unconnected-(U501-PadMH1)") (pinfunction "MH1") (pintype "passive+no_connect"))
    (model "C:\\Users\\luitz\\OneDrive-luitz\\OneDrive\\Documents\\KiCAD\\LibraryLoader\\SamacSys_Parts.3dshapes\\1018.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.025 64.77 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit")
    (attr smd)
    (fp_text reference "R201" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "120k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 8 "Net-(JP201-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 9 "Net-(R201-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 72.75 137.145 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "battery_unit.kicad_sch")
    (property "Sheetname" "Battery unit3")
    (attr through_hole)
    (fp_text reference "JP501" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Bypass" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/Battery unit3/V_batt-") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/Battery unit2/V_batt-") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(JP501-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 88.265 148.59 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Bias-Battery-Holder.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J104" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Chain In" (at 2.54 1.27 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/Battery unit3/V_batt-") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 127.635 34.29 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "Bias-Battery-Holder.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H102" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_rect (start 69.85 30.353) (end 130.81 153.035) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "<" (at 250.825 98.425 180) (layer "B.SilkS"))
  (gr_text "<" (at 250.825 14.605 180) (layer "B.SilkS"))
  (gr_text "<" (at 250.825 55.88 180) (layer "B.SilkS"))
  (gr_text "<" (at 250.825 77.47 180) (layer "B.SilkS"))
  (gr_text "Battery Board for Bias Voltage\n23A-size Batteries with safety resistors\nSL 12/2022" (at 115.57 48.26) (layer "B.SilkS"))
  (gr_text "<" (at 250.825 35.56 180) (layer "B.SilkS"))
  (gr_text "-" (at 88.265 151.13) (layer "F.SilkS"))
  (gr_text "Battery Probe" (at 116.84 34.29) (layer "F.SilkS"))
  (gr_text "GND" (at 113.03 38.1) (layer "F.SilkS"))
  (gr_text "-" (at 90.17 33.655) (layer "F.SilkS"))
  (gr_text "Chain In\nClose when not chaining" (at 93.218 150.114) (layer "F.SilkS"))
  (gr_text "Chain Out" (at 88.9 39.37) (layer "F.SilkS"))
  (gr_text ">" (at 70.485 71.12) (layer "F.SilkS"))
  (gr_text "+" (at 86.995 33.655) (layer "F.SilkS"))
  (gr_text "> : Battery on\n" (at 115.57 147.32) (layer "F.SilkS"))
  (gr_text "+" (at 90.805 151.13) (layer "F.SilkS"))
  (gr_text ">" (at 70.485 48.895) (layer "F.SilkS"))
  (gr_text "12-60V/I_max 0.1mA " (at 119.38 40.64) (layer "F.SilkS"))
  (gr_text ">" (at 70.485 132.08) (layer "F.SilkS"))
  (gr_text ">" (at 70.485 111.76) (layer "F.SilkS"))
)
