<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>CAN L</text>
<text>CAN H</text>
<text>1uF</text>
<text>1uF</text>
<text>120ohm</text>
<text>0.1uF</text>
<wire x1="6.599096875" y1="67.300034375" x2="48.1984" y2="67.300346875" width="0" layer="20"/>
<wire x1="48.1984" y1="67.300346875" x2="48.20235625" y2="54.198084375" width="0" layer="20"/>
<wire x1="48.20235625" y1="54.198084375" x2="6.59880625" y2="54.200159375" width="0" layer="20"/>
<wire x1="6.59880625" y1="54.200159375" x2="6.599096875" y2="67.300034375" width="0" layer="20"/>
</plain>
<libraries>
<library name="con-jst">
<description>&lt;b&gt;J.S.T. Connectors&lt;/b&gt;&lt;p&gt;
J.S.T Mfg Co.,Ltd.&lt;p&gt;
http://www.jst-mfg.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B4B-ZR">
<description>&lt;b&gt;ZH CONNECTOR&lt;/b&gt;  Top entry type, 1.5 mm, 4 pin 1 row&lt;p&gt;
Source: http://www.jst.com .. eZH.pdf</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="8S1">
<description>&lt;b&gt;8S1&lt;/b&gt; 8-lead (0.150" Wide Body)&lt;p&gt;
Plastic Gull Wing Small Outline (JEDEC SOIC)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT89-R">
<description>&lt;b&gt;SOT89 Reflow soldering&lt;/b&gt; Philips SC01_Mounting_1996.pdf</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP06SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ref-packages">
<description>&lt;b&gt;Reference Package&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$13" library="con-jst" package="B4B-ZR" value="">
<attribute name="VALUE"/>
</element>
<element name="E$16" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$22" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$28" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$29" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$30" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$31" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$32" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$33" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$34" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$36" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$39" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$40" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$41" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$42" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$43" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$44" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$45" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$46" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$47" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$48" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$49" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$50" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$51" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$54" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$55" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$56" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$57" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$58" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$59" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$60" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$61" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$64" library="testpad" package="TP06SQ" value="">
<attribute name="VALUE"/>
</element>
<element name="E$65" library="diode" package="SOT89-R" value="">
<attribute name="VALUE"/>
</element>
<element name="E$66" library="atmel" package="8S1" value="">
<attribute name="VALUE"/>
</element>
<element name="E$67" library="ref-packages" package="R0805" value="">
<attribute name="VALUE"/>
</element>
<element name="E$68" library="ref-packages" package="R0805" value="">
<attribute name="VALUE"/>
</element>
<element name="E$69" library="ref-packages" package="R0805" value="">
<attribute name="VALUE"/>
</element>
<element name="E$71" library="ref-packages" package="R0805" value="">
<attribute name="VALUE"/>
</element>
<element name="E$110" library="ref-packages" package="R0805" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$15">
</signal>
<signal name="S$18">
</signal>
<signal name="S$33">
</signal>
<signal name="S$20">
</signal>
<signal name="S$19">
</signal>
<signal name="S$22">
</signal>
<signal name="S$23">
</signal>
<signal name="S$38">
</signal>
<signal name="S$1">
</signal>
<signal name="S$2">
</signal>
<signal name="S$5">
</signal>
<signal name="S$9">
</signal>
<signal name="S$10">
</signal>
<signal name="S$12">
</signal>
<signal name="S$14">
</signal>
<signal name="S$16">
</signal>
<signal name="S$17">
</signal>
<signal name="S$21">
</signal>
</signals>
</board>
</drawing>
</eagle>
