(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 238)
    (no_connects 0)
    (area 87.500001 49.15 184.285715 165.450001)
    (thickness 1.6)
    (drawings 68)
    (tracks 1506)
    (zones 0)
    (modules 62)
    (nets 79)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.008)
    (zone_45_only yes)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.5)
    (via_drill 0.32)
    (via_min_size 0.019685)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.007874)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.25)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x030f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D4-Pad2)")
  (net 8 "Net-(D4-Pad1)")
  (net 9 +3V3)
  (net 10 /BLU3)
  (net 11 /BLU4)
  (net 12 /BLU5)
  (net 13 /BLU6)
  (net 14 /BLU7)
  (net 15 /BTN3)
  (net 16 /BTN4)
  (net 17 /BTN1)
  (net 18 /BL)
  (net 19 /CLOCK)
  (net 20 /DEN)
  (net 21 /AUDIO)
  (net 22 /BTN2)
  (net 23 "Net-(BT1-Pad1)")
  (net 24 "Net-(C2-Pad1)")
  (net 25 "Net-(C2-Pad2)")
  (net 26 "Net-(C3-Pad1)")
  (net 27 "Net-(C3-Pad2)")
  (net 28 +5V)
  (net 29 VBOOST)
  (net 30 "Net-(D5-Pad1)")
  (net 31 "Net-(D6-Pad2)")
  (net 32 "Net-(D7-Pad2)")
  (net 33 "Net-(D10-Pad1)")
  (net 34 "Net-(D8-Pad2)")
  (net 35 "Net-(D9-Pad2)")
  (net 36 "Net-(D10-Pad2)")
  (net 37 "Net-(D11-Pad1)")
  (net 38 "Net-(D11-Pad2)")
  (net 39 "Net-(D12-Pad2)")
  (net 40 "Net-(D13-Pad2)")
  (net 41 "Net-(L1-Pad2)")
  (net 42 /VSYNC)
  (net 43 /HSYNC)
  (net 44 /GRE4)
  (net 45 /GRE5)
  (net 46 /GRE7)
  (net 47 /RST)
  (net 48 /RED5)
  (net 49 /RED6)
  (net 50 /RED7)
  (net 51 /MISO)
  (net 52 /GRE2)
  (net 53 /GRE3)
  (net 54 /GRE6)
  (net 55 /RED3)
  (net 56 /RED4)
  (net 57 "Net-(Q1-Pad3)")
  (net 58 "Net-(R10-Pad2)")
  (net 59 "Net-(R11-Pad1)")
  (net 60 "Net-(R13-Pad1)")
  (net 61 "Net-(R14-Pad2)")
  (net 62 "Net-(SP1-Pad1)")
  (net 63 "Net-(SP1-Pad2)")
  (net 64 "Net-(U2-Pad2)")
  (net 65 VBAT)
  (net 66 "Net-(U1-Pad20)")
  (net 67 "Net-(U1-Pad39)")
  (net 68 "Net-(U1-Pad35)")
  (net 69 "Net-(U1-Pad32)")
  (net 70 "Net-(U1-Pad45)")
  (net 71 "Net-(U1-Pad44)")
  (net 72 "Net-(U1-Pad46)")
  (net 73 "Net-(U1-Pad47)")
  (net 74 /LED4)
  (net 75 /LED3)
  (net 76 /LED2)
  (net 77 /LED1)
  (net 78 "Net-(D14-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.32)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /AUDIO)
    (add_net /BL)
    (add_net /BLU3)
    (add_net /BLU4)
    (add_net /BLU5)
    (add_net /BLU6)
    (add_net /BLU7)
    (add_net /BTN1)
    (add_net /BTN2)
    (add_net /BTN3)
    (add_net /BTN4)
    (add_net /CLOCK)
    (add_net /DEN)
    (add_net /GRE2)
    (add_net /GRE3)
    (add_net /GRE4)
    (add_net /GRE5)
    (add_net /GRE6)
    (add_net /GRE7)
    (add_net /HSYNC)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /LED3)
    (add_net /LED4)
    (add_net /MISO)
    (add_net /RED3)
    (add_net /RED4)
    (add_net /RED5)
    (add_net /RED6)
    (add_net /RED7)
    (add_net /RST)
    (add_net /VSYNC)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U2-Pad2)")
    (add_net VBAT)
  )
  (net_class "Low power" ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.5)
    (via_drill 0.32)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net "Net-(SP1-Pad1)")
    (add_net "Net-(SP1-Pad2)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.9)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VBOOST)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 579D04BF)
    (at 114.808 71.882 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -0.942 -1.868 360) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 28 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gamegirl-v02:raspberry-zero (layer B.Cu) (tedit 578DA8F5)
    (at 137.8 145 180)
    (descr 34)
    (fp_text reference P1 (at 0 -7.25 180) (layer B.SilkS) hide)
    (fp_text value PI-ZERO (at 0.5 -4 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at -22.86 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 28 +5V))
    (pad 1 smd rect (at -22.86 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 3 smd rect (at -20.32 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 42 /VSYNC))
    (pad 5 smd rect (at -17.78 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 43 /HSYNC))
    (pad 7 smd rect (at -15.24 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 10 /BLU3))
    (pad 9 smd rect (at -12.7 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at -10.16 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 46 /GRE7))
    (pad 13 smd rect (at -7.62 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 47 /RST))
    (pad 15 smd rect (at -5.08 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 48 /RED5))
    (pad 17 smd rect (at -2.54 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 19 smd rect (at 0 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 17 /BTN1))
    (pad 21 smd rect (at 2.54 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 51 /MISO))
    (pad 23 smd rect (at 5.08 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 15 /BTN3))
    (pad 25 smd rect (at 7.62 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 27 smd rect (at 10.16 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 19 /CLOCK))
    (pad 29 smd rect (at 12.7 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 11 /BLU4))
    (pad 31 smd rect (at 15.24 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 12 /BLU5))
    (pad 33 smd rect (at 17.78 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 53 /GRE3))
    (pad 35 smd rect (at 20.32 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 21 /AUDIO))
    (pad 37 smd rect (at 22.86 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 22 /BTN2))
    (pad 39 smd rect (at 25.4 10.16 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -20.32 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 28 +5V))
    (pad 6 smd rect (at -17.78 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -15.24 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 44 /GRE4))
    (pad 10 smd rect (at -12.7 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 45 /GRE5))
    (pad 12 smd rect (at -10.16 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 18 /BL))
    (pad 14 smd rect (at -7.62 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -5.08 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 49 /RED6))
    (pad 18 smd rect (at -2.54 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 50 /RED7))
    (pad 20 smd rect (at 0 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 2.54 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 16 /BTN4))
    (pad 24 smd rect (at 5.08 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 14 /BLU7))
    (pad 26 smd rect (at 7.62 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 13 /BLU6))
    (pad 28 smd rect (at 10.16 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 20 /DEN))
    (pad 30 smd rect (at 12.7 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 32 smd rect (at 15.24 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 52 /GRE2))
    (pad 36 smd rect (at 20.32 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 54 /GRE6))
    (pad 34 smd rect (at 17.78 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 38 smd rect (at 22.86 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 55 /RED3))
    (pad 40 smd rect (at 25.4 12.7 180) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 56 /RED4))
    (model /mnt/gruscht/projects/piboy-zero/baseboard.kicad/components.pretty/3d-models/raspberry_pi_zero.x3d
      (at (xyz 0.05 0 0.04))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gamegirl-v02:rubber_pad (layer F.Cu) (tedit 578C7434)
    (at 155 136.5 45)
    (fp_text reference SW10 (at -3.040559 0.070711 135) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3 45) (layer F.Fab))
    (pad 1 smd rect (at -2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 1 smd rect (at -0.25 -2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 2 smd rect (at 2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 0.25 -1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 2 smd rect (at 0.25 -0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -0.25 0 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 2 smd rect (at 0.25 0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -0.25 1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 2 smd rect (at 0.25 1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -0.25 2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
  )
  (module gamegirl-v02:rubber_pad (layer F.Cu) (tedit 578C73E0)
    (at 118 121.5 45)
    (fp_text reference SW2 (at 3.181981 0.070711 135) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3 45) (layer F.Fab))
    (pad 1 smd rect (at -2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 1 smd rect (at -0.25 -2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.25 -1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 0.25 -0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.25 0 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 0.25 0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.25 1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 0.25 1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.25 2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
  )
  (module gamegirl-v02:Potentiometer_3386P (layer F.Cu) (tedit 579D053B)
    (at 128 157.8)
    (descr "Potentiometer, Trimmer, Spectrol Type 36X, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer, Trimmer, Spectrol Type 36X, Econtrim, Rev A, 02 Aug 2010,")
    (fp_text reference RV1 (at 0.5 -8.3) (layer F.SilkS))
    (fp_text value POT (at 0 -3.556) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 2.54 -2.54) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(C3-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 -2.54) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 578C70FF)
    (at 118.2 103.75 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -3.4 0 270) (layer B.SilkS))
    (fp_text value 330 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 77 /LED1))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 578C70FD)
    (at 116.1 103.75 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.4 0 270) (layer B.SilkS))
    (fp_text value 330 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 76 /LED2))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 578C70F4)
    (at 114 103.75 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -3.4 -0.2 270) (layer B.SilkS))
    (fp_text value 330 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 75 /LED3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57982BBC)
    (at 123 147.6 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.1 0 180) (layer F.SilkS))
    (fp_text value 680 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /AUDIO))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 579D04E8)
    (at 111.25 71.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at -0.25 2.5 360) (layer B.SilkS))
    (fp_text value 2k (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gamegirl-v02:rubber_pad (layer F.Cu) (tedit 578C73DD)
    (at 110.5 129 45)
    (fp_text reference SW1 (at -3.252691 0.141421 135) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3 45) (layer F.Fab))
    (pad 1 smd rect (at -2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 1 smd rect (at -0.25 -2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.25 -1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 0.25 -0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.25 0 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 0.25 0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.25 1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 0.25 1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.25 2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
  )
  (module gamegirl-v02:rubber_pad (layer F.Cu) (tedit 578C73DA)
    (at 118 136.5 45)
    (fp_text reference SW3 (at -3.11127 0.565685 135) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3 45) (layer F.Fab))
    (pad 1 smd rect (at -2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 1 smd rect (at -0.25 -2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 2 smd rect (at 2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.25 -1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 2 smd rect (at 0.25 -0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.25 0 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 2 smd rect (at 0.25 0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.25 1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 2 smd rect (at 0.25 1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.25 2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
  )
  (module gamegirl-v02:rubber_pad (layer F.Cu) (tedit 578C7430)
    (at 162.5 129 45)
    (fp_text reference SW11 (at 3.181981 0.070711 135) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3 45) (layer F.Fab))
    (pad 1 smd rect (at -2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 1 smd rect (at -0.25 -2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D12-Pad2)"))
    (pad 2 smd rect (at 0.25 -1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 0.25 -0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -0.25 0 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 0.25 0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -0.25 1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 0.25 1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -0.25 2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
  )
  (module gamegirl-v02:rubber_pad (layer F.Cu) (tedit 578C73D4)
    (at 125.5 129 45)
    (fp_text reference SW4 (at 3.323402 0.353553 135) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3 45) (layer F.Fab))
    (pad 1 smd rect (at -2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 1 smd rect (at -0.25 -2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 2 smd rect (at 2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.25 -1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 2 smd rect (at 0.25 -0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.25 0 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 2 smd rect (at 0.25 0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.25 1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 2 smd rect (at 0.25 1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.25 2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
  )
  (module gamegirl-v02:ER-CON50HT-1 (layer B.Cu) (tedit 578C7628)
    (at 127.25 98.75 90)
    (fp_text reference U1 (at 11.95 1.6 90) (layer B.SilkS))
    (fp_text value ER-TFT024-3 (at 12 2.9 90) (layer B.Fab))
    (fp_text user 1 (at -3.45 -1.45 360) (layer B.SilkS))
    (pad 1 smd rect (at 0 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 28 +5V))
    (pad 2 smd rect (at 0.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 77 /LED1))
    (pad "" smd rect (at -1.54 -2.325 90) (size 2 3) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 1.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 75 /LED3))
    (pad 3 smd rect (at 1 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 76 /LED2))
    (pad 5 smd rect (at 2 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 74 /LED4))
    (pad 7 smd rect (at 3 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 6 smd rect (at 2.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 3.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 10 smd rect (at 4.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 47 /RST))
    (pad 9 smd rect (at 4 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 14 smd rect (at 6.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 20 /DEN))
    (pad 15 smd rect (at 7 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 50 /RED7))
    (pad 16 smd rect (at 7.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 49 /RED6))
    (pad 17 smd rect (at 8 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 48 /RED5))
    (pad 19 smd rect (at 9 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 55 /RED3))
    (pad 18 smd rect (at 8.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 56 /RED4))
    (pad 20 smd rect (at 9.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(U1-Pad20)"))
    (pad 13 smd rect (at 6 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 /CLOCK))
    (pad 12 smd rect (at 5.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 43 /HSYNC))
    (pad 11 smd rect (at 5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 42 /VSYNC))
    (pad 38 smd rect (at 18.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 40 smd rect (at 19.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 39 smd rect (at 19 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(U1-Pad39)"))
    (pad 36 smd rect (at 17.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 /BTN4))
    (pad 37 smd rect (at 18 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 15 /BTN3))
    (pad 35 smd rect (at 17 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(U1-Pad35)"))
    (pad 21 smd rect (at 10 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 /GRE7))
    (pad 23 smd rect (at 11 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 45 /GRE5))
    (pad 22 smd rect (at 10.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 54 /GRE6))
    (pad 26 smd rect (at 12.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 52 /GRE2))
    (pad 28 smd rect (at 13.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 13 /BLU6))
    (pad 27 smd rect (at 13 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /BLU7))
    (pad 24 smd rect (at 11.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 44 /GRE4))
    (pad 25 smd rect (at 12 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 53 /GRE3))
    (pad 30 smd rect (at 14.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 /BLU4))
    (pad 32 smd rect (at 15.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(U1-Pad32)"))
    (pad 29 smd rect (at 14 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 12 /BLU5))
    (pad 31 smd rect (at 15 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 /BLU3))
    (pad 34 smd rect (at 16.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 /BTN1))
    (pad 33 smd rect (at 16 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 51 /MISO))
    (pad 43 smd rect (at 21 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 41 smd rect (at 20 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 42 smd rect (at 20.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 45 smd rect (at 22 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(U1-Pad45)"))
    (pad 44 smd rect (at 21.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(U1-Pad44)"))
    (pad 46 smd rect (at 22.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(U1-Pad46)"))
    (pad 50 smd rect (at 24.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 47 smd rect (at 23 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(U1-Pad47)"))
    (pad 49 smd rect (at 24 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 48 smd rect (at 23.5 0 90) (size 0.3 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad "" smd rect (at 26.04 -2.325 90) (size 2 3) (layers B.Cu B.Paste B.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57982BC0)
    (at 125.2 147.6 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.1 0.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 111.54 109.402 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2 90) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 120.176 109.402 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 2 90) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /BTN2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 151.666 109.752 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 2 90) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 160.556 109.752 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 2 90) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579D0511)
    (at 135.4 158.2 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.1 -1.05 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57982B99)
    (at 140.4 151.4)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 57982C34)
    (at 121.55 69.45 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -0.2 1.55 450) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 57982BE9)
    (at 113.95 86.55 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -3.3 0.05 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 29 VBOOST))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 578BAE3C)
    (at 108.55 88.75 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0.091 1.832 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 28 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57982C48)
    (at 120.8 61.2)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D5 (at -0.05 1.8 180) (layer F.SilkS))
    (fp_text value LED_Orange (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 +5V))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578ABC16)
    (at 120.176 113.72 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D6-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578ABC18)
    (at 122.462 113.72 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D7 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D7-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578ABC1C)
    (at 149.38 114.07 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D8 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D8-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578ABC21)
    (at 151.666 114.07 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D9 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D9-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578BBDB2)
    (at 153.952 114.07 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D10 (at 2.88 0.152 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D10-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578BBDB5)
    (at 158.27 114.07 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D11 (at 2.88 0.07 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D11-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578BBDB8)
    (at 160.556 114.07 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D12 (at 2.88 -0.044 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D12-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578BBDBA)
    (at 162.842 114.07 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D13 (at 2.88 0.042 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D13-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57982BEF)
    (at 114.05 84.35)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at 3.2 -0.1) (layer B.SilkS))
    (fp_text value 10uH (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 29 VBOOST))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(L1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57982C30)
    (at 121.55 64.65 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0.35 1.55 270) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57982B60)
    (at 107.2 104.6 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -0.05 -1.9 360) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 /BL))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57982B87)
    (at 135.6 151.4)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57982BF5)
    (at 108.45 92.55)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0.05 1.7) (layer B.SilkS))
    (fp_text value 976k (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 28 +5V))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R14-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57982BF8)
    (at 113.55 92.55)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at -0.05 1.7) (layer B.SilkS))
    (fp_text value 309k (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R14-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 579D0515)
    (at 138.6 155.2)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0.4 2.55 180) (layer F.SilkS))
    (fp_text value PAM8302A (at 0 2.6) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at -2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C3-Pad1)"))
    (pad 5 smd rect (at 2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(SP1-Pad2)"))
    (pad 6 smd rect (at 2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 7 smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(SP1-Pad1)"))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578ABC0A)
    (at 109.254 113.72 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578ABC0D)
    (at 111.54 113.72 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578ABC0F)
    (at 113.826 113.72 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 578ABC13)
    (at 117.89 113.72 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.055 0 270) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579D050B)
    (at 134.2 154.8 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0.2 1.7 450) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 578C711A)
    (at 111.9 103.75 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -3.4 0 450) (layer B.SilkS))
    (fp_text value 330 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 74 /LED4))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 579D04F5)
    (at 107.3 101.9 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.4 0.95 180) (layer B.SilkS))
    (fp_text value Q_PMOS_GSD (at 0 -3.81 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.50114 90) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 18 /BL))
    (pad 2 smd rect (at 0.95 -1.50114 90) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.50114 90) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(Q1-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_SH_BM02B-SRSS-TB_02x1.00mm_Straight (layer B.Cu) (tedit 578C6E35)
    (at 125.25 68.25 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference BT1 (at -0.158 3.368 90) (layer B.SilkS))
    (fp_text value Battery (at 0 -3.5 90) (layer B.Fab))
    (pad 2 smd rect (at -0.5 -1.2625 90) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.5 -1.2625 90) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (pad "" smd rect (at -1.8 1.2625 90) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 1.8 1.2625 90) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
  )
  (module Buttons_Switches_SMD:SW_SPDT_PCM12 (layer B.Cu) (tedit 57982C54)
    (at 114.25 62.25)
    (descr "Ultraminiature Surface Mount Slide Switch")
    (attr smd)
    (fp_text reference SW13 (at -5 0 90) (layer B.SilkS))
    (fp_text value Switch_SPDT_x2 (at 0 -0.325) (layer B.Fab))
    (pad "" np_thru_hole circle (at -1.5 -0.325) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.5 -0.325) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -2.25 1.425) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 65 VBAT))
    (pad 2 smd rect (at 0.75 1.425) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (pad 3 smd rect (at 2.25 1.425) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 29 VBOOST))
    (pad "" smd rect (at -3.65 -1.425) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 3.65 -1.425) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 3.65 0.775) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at -3.65 0.775) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer B.Cu) (tedit 579D04E1)
    (at 114.046 68.834 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -0.084 -2.454 360) (layer B.SilkS))
    (fp_text value MCP73831/2 (at -0.05 -2.35 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(R10-Pad2)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 65 VBAT))
    (pad 4 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 28 +5V))
    (pad 5 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R11-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer B.Cu) (tedit 579D04D4)
    (at 113.2 89.15 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U4 (at -2.8 -0.1 180) (layer B.SilkS))
    (fp_text value MCP1640B/D (at 0 -2.9 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(L1-Pad2)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 29 VBOOST))
    (pad 4 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R14-Pad2)"))
    (pad 6 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 29 VBOOST))
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 28 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gamegirl-v02:Speaker-Pinout (layer F.Cu) (tedit 578C6F75)
    (at 143.6 156.2 270)
    (attr virtual)
    (fp_text reference SP1 (at 0 -2.4 270) (layer F.SilkS))
    (fp_text value SPEAKER (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd oval (at -1.27 0 270) (size 1.50622 3.01498) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(SP1-Pad1)"))
    (pad 2 smd oval (at 1.27 0 270) (size 1.50622 3.01498) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(SP1-Pad2)"))
  )
  (module gamegirl-v02:rubber_pad (layer F.Cu) (tedit 578C7436)
    (at 147.5 129 45)
    (fp_text reference SW9 (at -3.252691 0 135) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3 45) (layer F.Fab))
    (pad 1 smd rect (at -2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 1 smd rect (at -0.25 -2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 2 smd rect (at 2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 0.25 -1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 2 smd rect (at 0.25 -0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -0.25 0 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 2 smd rect (at 0.25 0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -0.25 1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 2 smd rect (at 0.25 1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -0.25 2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
  )
  (module gamegirl-v02:rubber_pad (layer F.Cu) (tedit 578C742D)
    (at 155 121.5 45)
    (fp_text reference SW12 (at 3.11127 -0.282843 135) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3 45) (layer F.Fab))
    (pad 1 smd rect (at -2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 1 smd rect (at -0.25 -2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 2 0 45) (size 0.25 4.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D13-Pad2)"))
    (pad 2 smd rect (at 0.25 -1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 0.25 -0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -0.25 0 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 0.25 0.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -0.25 1 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 0.25 1.5 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -0.25 2 135) (size 0.25 3.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BTN3))
  )
  (module gamegirl-v02:rubber_pad (layer B.Cu) (tedit 578C73F3)
    (at 130.75 120)
    (fp_text reference SW5 (at 0 3) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0 3) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 0.25 4.25) (layers B.Cu B.Paste B.Mask)
      (net 15 /BTN3))
    (pad 1 smd rect (at -0.25 2 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 2 0) (size 0.25 4.25) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 0.25 1.5 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.25 1 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 0.25 0.5 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.25 0 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 0.25 -0.5 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 15 /BTN3))
    (pad 2 smd rect (at 0.25 -1.5 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.25 -2 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 15 /BTN3))
  )
  (module gamegirl-v02:rubber_pad (layer B.Cu) (tedit 578C740A)
    (at 141.25 120)
    (fp_text reference SW8 (at 0 3.25) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0 3) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 0.25 4.25) (layers B.Cu B.Paste B.Mask)
      (net 22 /BTN2))
    (pad 1 smd rect (at -0.25 2 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 2 0) (size 0.25 4.25) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 0.25 1.5 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -0.25 1 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 0.25 0.5 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -0.25 0 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 0.25 -0.5 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -0.25 -1 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 22 /BTN2))
    (pad 2 smd rect (at 0.25 -1.5 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -0.25 -2 270) (size 0.25 3.75) (layers B.Cu B.Paste B.Mask)
      (net 22 /BTN2))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 578D8EA6)
    (at 113.03 65.786)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.302 0 180) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 65 VBAT))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gamegirl-v02:SW_DOME_4x4.6_SMD (layer F.Cu) (tedit 57982B93)
    (at 131.3 146)
    (fp_text reference SW6 (at -0.05 -3) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -2.7) (layer F.Fab))
    (pad 1 smd rect (at -2.3 -1.7) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /BTN4))
    (pad 2 smd rect (at -2.3 1.7) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D7-Pad2)"))
    (pad 3 smd rect (at 2.3 -1.7) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.3 1.7) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
  )
  (module gamegirl-v02:SW_DOME_4x4.6_SMD (layer F.Cu) (tedit 57982B8F)
    (at 141.3 146)
    (fp_text reference SW7 (at -0.05 -3) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -2.7) (layer F.Fab))
    (pad 1 smd rect (at -2.3 -1.7) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /BTN1))
    (pad 2 smd rect (at -2.3 1.7) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D8-Pad2)"))
    (pad 3 smd rect (at 2.3 -1.7) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.3 1.7) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 124.7 61.2 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D14 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value LED_Green (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 +5V))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(D14-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57981E9D)
    (at 125.25 61.25)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 1.75) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(D14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "16mm Speaker" (at 155.25 151) (layer F.SilkS))
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 136.5 53.15) (layer Dwgs.User))
    (feature1 (pts (xy 165.5 62) (xy 165.5 51.8)))
    (feature2 (pts (xy 107.5 62) (xy 107.5 51.8)))
    (crossbar (pts (xy 107.5 54.5) (xy 165.5 54.5)))
    (arrow1a (pts (xy 165.5 54.5) (xy 164.373496 55.086421)))
    (arrow1b (pts (xy 165.5 54.5) (xy 164.373496 53.913579)))
    (arrow2a (pts (xy 107.5 54.5) (xy 108.626504 55.086421)))
    (arrow2b (pts (xy 107.5 54.5) (xy 108.626504 53.913579)))
  )
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 94.15 91 90) (layer Dwgs.User))
    (feature1 (pts (xy 105 62) (xy 92.8 62)))
    (feature2 (pts (xy 105 120) (xy 92.8 120)))
    (crossbar (pts (xy 95.5 120) (xy 95.5 62)))
    (arrow1a (pts (xy 95.5 62) (xy 96.086421 63.126504)))
    (arrow1b (pts (xy 95.5 62) (xy 94.913579 63.126504)))
    (arrow2a (pts (xy 95.5 120) (xy 96.086421 118.873496)))
    (arrow2b (pts (xy 95.5 120) (xy 94.913579 118.873496)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 167.25 162.85) (layer Dwgs.User))
    (feature1 (pts (xy 165.5 156.5) (xy 165.5 164.2)))
    (feature2 (pts (xy 169 156.5) (xy 169 164.2)))
    (crossbar (pts (xy 169 161.5) (xy 165.5 161.5)))
    (arrow1a (pts (xy 165.5 161.5) (xy 166.626504 160.913579)))
    (arrow1b (pts (xy 165.5 161.5) (xy 166.626504 162.086421)))
    (arrow2a (pts (xy 169 161.5) (xy 167.873496 160.913579)))
    (arrow2b (pts (xy 169 161.5) (xy 167.873496 162.086421)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 178.35 158.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 165.5 156.5) (xy 179.7 156.5)))
    (feature2 (pts (xy 165.5 160) (xy 179.7 160)))
    (crossbar (pts (xy 177 160) (xy 177 156.5)))
    (arrow1a (pts (xy 177 156.5) (xy 177.586421 157.626504)))
    (arrow1b (pts (xy 177 156.5) (xy 176.413579 157.626504)))
    (arrow2a (pts (xy 177 160) (xy 177.586421 158.873496)))
    (arrow2b (pts (xy 177 160) (xy 176.413579 158.873496)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 167.25 116.4) (layer Dwgs.User))
    (feature1 (pts (xy 169 120) (xy 169 115.05)))
    (feature2 (pts (xy 165.5 120) (xy 165.5 115.05)))
    (crossbar (pts (xy 165.5 117.75) (xy 169 117.75)))
    (arrow1a (pts (xy 169 117.75) (xy 167.873496 118.336421)))
    (arrow1b (pts (xy 169 117.75) (xy 167.873496 117.163579)))
    (arrow2a (pts (xy 165.5 117.75) (xy 166.626504 118.336421)))
    (arrow2b (pts (xy 165.5 117.75) (xy 166.626504 117.163579)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 105.75 116.9) (layer Dwgs.User))
    (feature1 (pts (xy 104 120) (xy 104 115.55)))
    (feature2 (pts (xy 107.5 120) (xy 107.5 115.55)))
    (crossbar (pts (xy 107.5 118.25) (xy 104 118.25)))
    (arrow1a (pts (xy 104 118.25) (xy 105.126504 117.663579)))
    (arrow1b (pts (xy 104 118.25) (xy 105.126504 118.836421)))
    (arrow2a (pts (xy 107.5 118.25) (xy 106.373496 117.663579)))
    (arrow2b (pts (xy 107.5 118.25) (xy 106.373496 118.836421)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 167.25 55.9) (layer Dwgs.User))
    (feature1 (pts (xy 165.5 60) (xy 165.5 54.55)))
    (feature2 (pts (xy 169 60) (xy 169 54.55)))
    (crossbar (pts (xy 169 57.25) (xy 165.5 57.25)))
    (arrow1a (pts (xy 165.5 57.25) (xy 166.626504 56.663579)))
    (arrow1b (pts (xy 165.5 57.25) (xy 166.626504 57.836421)))
    (arrow2a (pts (xy 169 57.25) (xy 167.873496 56.663579)))
    (arrow2b (pts (xy 169 57.25) (xy 167.873496 57.836421)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 105.75 56.65) (layer Dwgs.User))
    (feature1 (pts (xy 107.5 61.5) (xy 107.5 55.3)))
    (feature2 (pts (xy 104 61.5) (xy 104 55.3)))
    (crossbar (pts (xy 104 58) (xy 107.5 58)))
    (arrow1a (pts (xy 107.5 58) (xy 106.373496 58.586421)))
    (arrow1b (pts (xy 107.5 58) (xy 106.373496 57.413579)))
    (arrow2a (pts (xy 104 58) (xy 105.126504 58.586421)))
    (arrow2b (pts (xy 104 58) (xy 105.126504 57.413579)))
  )
  (dimension 40 (width 0.3) (layer Dwgs.User)
    (gr_text "40.000 mm" (at 94.4 140 270) (layer Dwgs.User))
    (feature1 (pts (xy 108 160) (xy 93.05 160)))
    (feature2 (pts (xy 108 120) (xy 93.05 120)))
    (crossbar (pts (xy 95.75 120) (xy 95.75 160)))
    (arrow1a (pts (xy 95.75 160) (xy 95.163579 158.873496)))
    (arrow1b (pts (xy 95.75 160) (xy 96.336421 158.873496)))
    (arrow2a (pts (xy 95.75 120) (xy 95.163579 121.126504)))
    (arrow2b (pts (xy 95.75 120) (xy 96.336421 121.126504)))
  )
  (dimension 40 (width 0.3) (layer Dwgs.User)
    (gr_text "40.000 mm" (at 172.1 140 270) (layer Dwgs.User))
    (feature1 (pts (xy 169 160) (xy 173.45 160)))
    (feature2 (pts (xy 169 120) (xy 173.45 120)))
    (crossbar (pts (xy 170.75 120) (xy 170.75 160)))
    (arrow1a (pts (xy 170.75 160) (xy 170.163579 158.873496)))
    (arrow1b (pts (xy 170.75 160) (xy 171.336421 158.873496)))
    (arrow2a (pts (xy 170.75 120) (xy 170.163579 121.126504)))
    (arrow2b (pts (xy 170.75 120) (xy 171.336421 121.126504)))
  )
  (dimension 2 (width 0.3) (layer Dwgs.User)
    (gr_text "2.000 mm" (at 177.1 61 270) (layer Dwgs.User))
    (feature1 (pts (xy 165 62) (xy 178.45 62)))
    (feature2 (pts (xy 165 60) (xy 178.45 60)))
    (crossbar (pts (xy 175.75 60) (xy 175.75 62)))
    (arrow1a (pts (xy 175.75 62) (xy 175.163579 60.873496)))
    (arrow1b (pts (xy 175.75 62) (xy 176.336421 60.873496)))
    (arrow2a (pts (xy 175.75 60) (xy 175.163579 61.126504)))
    (arrow2b (pts (xy 175.75 60) (xy 176.336421 61.126504)))
  )
  (dimension 2 (width 0.3) (layer Dwgs.User)
    (gr_text "2.000 mm" (at 97.9 61 270) (layer Dwgs.User))
    (feature1 (pts (xy 108 62) (xy 96.55 62)))
    (feature2 (pts (xy 108 60) (xy 96.55 60)))
    (crossbar (pts (xy 99.25 60) (xy 99.25 62)))
    (arrow1a (pts (xy 99.25 62) (xy 98.663579 60.873496)))
    (arrow1b (pts (xy 99.25 62) (xy 99.836421 60.873496)))
    (arrow2a (pts (xy 99.25 60) (xy 98.663579 61.126504)))
    (arrow2b (pts (xy 99.25 60) (xy 99.836421 61.126504)))
  )
  (dimension 32 (width 0.3) (layer Dwgs.User)
    (gr_text "32.000 mm" (at 120 125.4) (layer Dwgs.User))
    (feature1 (pts (xy 136 129) (xy 136 124.05)))
    (feature2 (pts (xy 104 129) (xy 104 124.05)))
    (crossbar (pts (xy 104 126.75) (xy 136 126.75)))
    (arrow1a (pts (xy 136 126.75) (xy 134.873496 127.336421)))
    (arrow1b (pts (xy 136 126.75) (xy 134.873496 126.163579)))
    (arrow2a (pts (xy 104 126.75) (xy 105.126504 127.336421)))
    (arrow2b (pts (xy 104 126.75) (xy 105.126504 126.163579)))
  )
  (dimension 14 (width 0.3) (layer Dwgs.User)
    (gr_text "14.000 mm" (at 111 143.1) (layer Dwgs.User))
    (feature1 (pts (xy 118 133.25) (xy 118 144.45)))
    (feature2 (pts (xy 104 133.25) (xy 104 144.45)))
    (crossbar (pts (xy 104 141.75) (xy 118 141.75)))
    (arrow1a (pts (xy 118 141.75) (xy 116.873496 142.336421)))
    (arrow1b (pts (xy 118 141.75) (xy 116.873496 141.163579)))
    (arrow2a (pts (xy 104 141.75) (xy 105.126504 142.336421)))
    (arrow2b (pts (xy 104 141.75) (xy 105.126504 141.163579)))
  )
  (dimension 14 (width 0.3) (layer Dwgs.User)
    (gr_text "14.000 mm" (at 162 143.85) (layer Dwgs.User))
    (feature1 (pts (xy 155 129) (xy 155 145.2)))
    (feature2 (pts (xy 169 129) (xy 169 145.2)))
    (crossbar (pts (xy 169 142.5) (xy 155 142.5)))
    (arrow1a (pts (xy 155 142.5) (xy 156.126504 141.913579)))
    (arrow1b (pts (xy 155 142.5) (xy 156.126504 143.086421)))
    (arrow2a (pts (xy 169 142.5) (xy 167.873496 141.913579)))
    (arrow2b (pts (xy 169 142.5) (xy 167.873496 143.086421)))
  )
  (dimension 31 (width 0.3) (layer Dwgs.User)
    (gr_text "31.000 mm" (at 100.9 144.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 117.5 160) (xy 99.55 160)))
    (feature2 (pts (xy 117.5 129) (xy 99.55 129)))
    (crossbar (pts (xy 102.25 129) (xy 102.25 160)))
    (arrow1a (pts (xy 102.25 160) (xy 101.663579 158.873496)))
    (arrow1b (pts (xy 102.25 160) (xy 102.836421 158.873496)))
    (arrow2a (pts (xy 102.25 129) (xy 101.663579 130.126504)))
    (arrow2b (pts (xy 102.25 129) (xy 102.836421 130.126504)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 98.4 158.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 108 156.5) (xy 97.05 156.5)))
    (feature2 (pts (xy 108 160) (xy 97.05 160)))
    (crossbar (pts (xy 99.75 160) (xy 99.75 156.5)))
    (arrow1a (pts (xy 99.75 156.5) (xy 100.336421 157.626504)))
    (arrow1b (pts (xy 99.75 156.5) (xy 99.163579 157.626504)))
    (arrow2a (pts (xy 99.75 160) (xy 100.336421 158.873496)))
    (arrow2b (pts (xy 99.75 160) (xy 99.163579 158.873496)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 105.75 164.1) (layer Dwgs.User))
    (feature1 (pts (xy 107.5 156.25) (xy 107.5 165.45)))
    (feature2 (pts (xy 104 156.25) (xy 104 165.45)))
    (crossbar (pts (xy 104 162.75) (xy 107.5 162.75)))
    (arrow1a (pts (xy 107.5 162.75) (xy 106.373496 163.336421)))
    (arrow1b (pts (xy 107.5 162.75) (xy 106.373496 162.163579)))
    (arrow2a (pts (xy 104 162.75) (xy 105.126504 163.336421)))
    (arrow2b (pts (xy 104 162.75) (xy 105.126504 162.163579)))
  )
  (gr_circle (center 165.5 62) (end 165.5 61) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119 100) (end 121 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119 73) (end 121 73) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121 100) (end 121 73) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 100.000312 (width 0.3) (layer Dwgs.User)
    (gr_text "100.000 mm" (at 175.973686 109.972878 270.1432392) (layer Dwgs.User))
    (feature1 (pts (xy 165 60) (xy 177.198682 59.969503)))
    (feature2 (pts (xy 165.25 160) (xy 177.448682 159.969503)))
    (crossbar (pts (xy 174.74869 159.976253) (xy 174.49869 59.976253)))
    (arrow1a (pts (xy 174.49869 59.976253) (xy 175.087925 61.101287)))
    (arrow1b (pts (xy 174.49869 59.976253) (xy 173.915087 61.104219)))
    (arrow2a (pts (xy 174.74869 159.976253) (xy 175.332293 158.848287)))
    (arrow2b (pts (xy 174.74869 159.976253) (xy 174.159455 158.851219)))
  )
  (gr_line (start 119 73) (end 119 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "16MM Speaker" (at 156.5 151.25) (layer Dwgs.User))
  (gr_circle (center 136 124) (end 136 125) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 107.5 120) (end 107.5 119) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 165.5 120) (end 165.5 119) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 107.5 62) (end 107.5 61) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 165.5 156.5) (end 165.5 158) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 107.5 156.5) (end 107.5 155) (layer Edge.Cuts) (width 0.15))
  (dimension 65 (width 0.3) (layer Dwgs.User)
    (gr_text "65.000 mm" (at 136.5 50.65) (layer Dwgs.User))
    (feature1 (pts (xy 169 69) (xy 169 49.3)))
    (feature2 (pts (xy 104 69) (xy 104 49.3)))
    (crossbar (pts (xy 104 52) (xy 169 52)))
    (arrow1a (pts (xy 169 52) (xy 167.873496 52.586421)))
    (arrow1b (pts (xy 169 52) (xy 167.873496 51.413579)))
    (arrow2a (pts (xy 104 52) (xy 105.126504 52.586421)))
    (arrow2b (pts (xy 104 52) (xy 105.126504 51.413579)))
  )
  (gr_line (start 104 156.5) (end 104 156.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.5 160) (end 107.5 160) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.25 60) (end 107.75 60) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.25 63.75) (end 165.25 60) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104 63.25) (end 104 156.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 107.5 63.5) (end 104 63.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 107.5 156.5) (end 107.5 160) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.5 156.5) (end 169 156.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169 63.75) (end 169 156.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 28) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.75 72) (xy 118 72) (xy 118 83) (xy 111.5 83) (xy 111.5 84.5)
        (xy 110.5 85.5) (xy 110.5 87.75) (xy 111.5 88.75) (xy 112.55 88.75) (xy 112.55 89.55)
        (xy 111.17 89.55) (xy 111.15 89.583333) (xy 111.15 91.55) (xy 108.75 91.55) (xy 108.75 99.8)
        (xy 106.15 99.8) (xy 106.15 89.75) (xy 108 89.75) (xy 108.5 89.25) (xy 108.5 87.5)
        (xy 109.5 86.25) (xy 109.5 82) (xy 114.75 75.25) (xy 114.75 69.5) (xy 118.75 69.5)
        (xy 118.75 72)
      )
    )
  )
  (zone (net 61) (net_name "Net-(R14-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.55 89.75) (xy 112.55 90.95) (xy 113.35 91.75) (xy 113.35 93.55) (xy 109.15 93.55)
        (xy 109.15 91.95) (xy 111.55 91.95) (xy 111.55 89.75)
      )
    )
  )
  (zone (net 29) (net_name VBOOST) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.75 90.35) (xy 114.95 91.55) (xy 116.95 91.55) (xy 116.95 90.15) (xy 115.35 90.15)
        (xy 114.95 89.75) (xy 113.75 89.75)
      )
    )
  )
  (zone (net 28) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 69) (xy 114.75 75) (xy 118 75) (xy 118 72) (xy 118.75 72)
        (xy 118.75 69) (xy 117.75 69)
      )
    )
  )
  (zone (net 59) (net_name "Net-(R11-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.5 69.25) (xy 110.25 69.25) (xy 110.25 71.25) (xy 112.25 71.25) (xy 112.75 70.75)
        (xy 113.5 70.75)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.25 65) (xy 112.5 65) (xy 112.75 65.25) (xy 112.75 66.5) (xy 112.5 66.75)
        (xy 112.5 68.5) (xy 113.75 68.5) (xy 113.75 67) (xy 114.5 67) (xy 114.5 68.5)
        (xy 118.75 68.5) (xy 118.75 69.25) (xy 114.5 69.25) (xy 114.5 75.25) (xy 109.25 82)
        (xy 109.25 86.25) (xy 108.25 87.5) (xy 108.25 89.25) (xy 108 89.5) (xy 105.9 89.5)
        (xy 106 98.15) (xy 106 99.75) (xy 104.5 99.75) (xy 104.5 64) (xy 111.25 64)
        (xy 111.25 65)
      )
    )
    (polygon
      (pts        (xy 110 69) (xy 110 71.5) (xy 112.333333 71.5) (xy 112.55 71.45) (xy 113 71)
        (xy 113.75 71) (xy 113.75 69.25) (xy 114.25 69.25) (xy 114 69) (xy 110 69)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.5 88.75) (xy 116.5 88.75) (xy 116.75 88.5) (xy 118 88.5) (xy 118 99.75)
        (xy 109 99.75) (xy 109 93.75) (xy 113.75 93.75) (xy 113.75 91.75) (xy 113 91)
        (xy 113 87.5) (xy 112.25 87.5) (xy 111.5 86.75) (xy 111.5 86.25) (xy 112 85.75)
        (xy 113.5 85.75) (xy 113.5 88.75)
      )
    )
    (polygon
      (pts        (xy 113.5 89.5) (xy 113.5 90.5) (xy 114.75 91.75) (xy 117.25 91.75) (xy 117.25 90)
        (xy 115.5 90) (xy 115 89.5) (xy 113.5 89.5)
      )
    )
  )
  (zone (net 29) (net_name VBOOST) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.25 85) (xy 115 85.75) (xy 116 85.75) (xy 116.25 86) (xy 116.25 87.5)
        (xy 116 87.75) (xy 115 87.75) (xy 115 87.5) (xy 113.75 87.5) (xy 113.75 85.75)
        (xy 114 86.1) (xy 114 86) (xy 113.5 85.5) (xy 112 85.5) (xy 111.25 86.25)
        (xy 111.25 86.75) (xy 112.25 87.75) (xy 112.75 87.75) (xy 112.75 88.5) (xy 111.5 88.5)
        (xy 110.75 87.75) (xy 110.75 85.5) (xy 111.75 84.5) (xy 111.75 83.25) (xy 114.25 83.25)
        (xy 114.25 85)
      )
    )
  )
  (zone (net 41) (net_name "Net-(L1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118 88.25) (xy 116.75 88.25) (xy 116.5 88.5) (xy 113.75 88.5) (xy 113.75 87.75)
        (xy 114.75 87.75) (xy 114.75 88) (xy 116 88) (xy 116.5 87.5) (xy 116.5 85.75)
        (xy 116.25 85.5) (xy 115 85.5) (xy 114.5 85) (xy 114.5 83.25) (xy 118 83.25)
        (xy 118 88.25)
      )
    )
  )
  (zone (net 65) (net_name VBAT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 68.25) (xy 118.75 68.25) (xy 118.75 64.75) (xy 114.5 64.75) (xy 114.25 64.5)
        (xy 114.25 62.75) (xy 111.5 62.75) (xy 111.5 64.75) (xy 112.75 64.75) (xy 113 65.25)
        (xy 113 66.75) (xy 114.75 66.75)
      )
    )
  )
  (zone (net 65) (net_name VBAT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.008))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.25 64.75) (xy 118.75 64.75) (xy 118.75 68.25) (xy 114.75 68.25) (xy 114.75 66.75)
        (xy 114.5 66.5) (xy 112.75 66.5) (xy 112.75 64.75) (xy 111.5 64.75) (xy 111.5 62.75)
        (xy 114.25 62.75) (xy 114.25 64.75)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.008))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.5 64) (xy 104.5 99.75) (xy 118 99.75) (xy 118 75.25) (xy 114.5 75.25)
        (xy 114.5 67) (xy 112.5 67) (xy 112.5 65) (xy 111.25 65) (xy 111.25 64)
      )
    )
  )
)
