(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 9)
    (no_connects 0)
    (area 126.924999 93.904999 152.475001 104.215001)
    (thickness 1.6)
    (drawings 12)
    (tracks 26)
    (zones 0)
    (modules 4)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 595AEA5C)
    (at 136.0932 99.06 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 150 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 595AEA59)
    (at 141.752898 99.154448 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at 0 -4.5 180) (layer F.SilkS) hide)
    (fp_text value Q_NMOS_GDSD (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module edge-pcb:edge-pcb (layer F.Cu) (tedit 595AEA34)
    (at 127 99.06 270)
    (fp_text reference J1 (at 0 1.27 270) (layer F.SilkS) hide)
    (fp_text value edge-pcb (at 0 2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.81 -3.75 270) (size 1.65 7.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.81 -3.75 270) (size 1.65 7.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.27 -3.75 270) (size 1.65 7.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -1.27 -3.75 270) (size 1.65 7.5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.27 -3.75 270) (size 1.65 7.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 1.27 -3.75 270) (size 1.65 7.5) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at 3.81 -3.75 270) (size 1.65 7.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 3.81 -3.75 270) (size 1.65 7.5) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad7)"))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 595AEA57)
    (at 147.828 99.06 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value LITEON-LTST-C170KGKT (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "Cedric Priscal\nJuly 2017" (at 143.002 99.314) (layer B.SilkS))
  (gr_line (start 152.4 95.25) (end 152.4 93.98) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 96.52) (end 152.4 97.79) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_text 6A (at 150.495 99.06 90) (layer F.SilkS))
  (dimension 10.16 (width 0.3) (layer Dwgs.User)
    (gr_text "0.4000 in" (at 156.29 99.06 270) (layer Dwgs.User))
    (feature1 (pts (xy 152.4 104.14) (xy 157.64 104.14)))
    (feature2 (pts (xy 152.4 93.98) (xy 157.64 93.98)))
    (crossbar (pts (xy 154.94 93.98) (xy 154.94 104.14)))
    (arrow1a (pts (xy 154.94 104.14) (xy 154.353579 103.013496)))
    (arrow1b (pts (xy 154.94 104.14) (xy 155.526421 103.013496)))
    (arrow2a (pts (xy 154.94 93.98) (xy 154.353579 95.106504)))
    (arrow2b (pts (xy 154.94 93.98) (xy 155.526421 95.106504)))
  )
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 139.7 108.03) (layer Dwgs.User))
    (feature1 (pts (xy 152.4 104.14) (xy 152.4 109.38)))
    (feature2 (pts (xy 127 104.14) (xy 127 109.38)))
    (crossbar (pts (xy 127 106.68) (xy 152.4 106.68)))
    (arrow1a (pts (xy 152.4 106.68) (xy 151.273496 107.266421)))
    (arrow1b (pts (xy 152.4 106.68) (xy 151.273496 106.093579)))
    (arrow2a (pts (xy 127 106.68) (xy 128.126504 107.266421)))
    (arrow2b (pts (xy 127 106.68) (xy 128.126504 106.093579)))
  )
  (gr_line (start 152.4 93.98) (end 127.4064 93.98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 104.14) (end 152.4 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.4064 104.14) (end 152.4 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 103.7336) (end 127.4064 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 94.3864) (end 127 103.7336) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.4064 93.98) (end 127 94.3864) (layer Edge.Cuts) (width 0.15))
)
