(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 39)
    (no_connects 0)
    (area 119.431999 52.629999 148.538001 99.135001)
    (thickness 1.6)
    (drawings 29)
    (tracks 129)
    (zones 0)
    (modules 34)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.25)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 SCART_Red)
  (net 5 "Net-(C3-Pad1)")
  (net 6 SCART_Green)
  (net 7 "Net-(C5-Pad1)")
  (net 8 SCART_Sync)
  (net 9 "Net-(R1-Pad1)")
  (net 10 Jamma_Red)
  (net 11 "Net-(R2-Pad1)")
  (net 12 Jamma_Blue)
  (net 13 "Net-(R3-Pad1)")
  (net 14 Jamma_Green)
  (net 15 "Net-(R4-Pad1)")
  (net 16 Jamma_Sync)
  (net 17 "Net-(R9-Pad2)")
  (net 18 "Net-(R10-Pad2)")
  (net 19 "Net-(C4-Pad1)")
  (net 20 "Net-(R11-Pad2)")
  (net 21 "Net-(R12-Pad2)")
  (net 22 SCART_Blue)
  (net 23 "Net-(P1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Jamma_Blue)
    (add_net Jamma_Green)
    (add_net Jamma_Red)
    (add_net Jamma_Sync)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net SCART_Blue)
    (add_net SCART_Green)
    (add_net SCART_Red)
    (add_net SCART_Sync)
  )
  (net_class +5V ""
    (clearance 0.2)
    (trace_width 0.45)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (net_class GND ""
    (clearance 0.2)
    (trace_width 0.45)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B0D435D)
    (at 133.985 78.74)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5B0D219B)
    (at 124.46 65.405 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C2 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value 220uF (at 0 -5.4483 90) (layer F.Fab))
    (fp_text user + (at -2.3114 -0.0762 90) (layer F.Fab))
    (fp_text user + (at -4.826 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 SCART_Red))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5B0D21A8)
    (at 133.985 65.405 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C3 (at 0 2.667 90) (layer F.SilkS))
    (fp_text value 220uF (at 0 -5.4483 90) (layer F.Fab))
    (fp_text user + (at -2.3114 -0.0762 90) (layer F.Fab))
    (fp_text user + (at -4.826 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 SCART_Green))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5B0D21BA)
    (at 143.637 65.405 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C4 (at 0 2.667 90) (layer F.SilkS))
    (fp_text value 220uF (at 0 -5.4483 90) (layer F.Fab))
    (fp_text user + (at -2.3114 -0.0762 90) (layer F.Fab))
    (fp_text user + (at -4.826 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 SCART_Blue))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 5B0D21B2)
    (at 143.637 76.708 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C5 (at -0.127 2.667 90) (layer F.SilkS))
    (fp_text value 220uF (at 0 -5.4483 90) (layer F.Fab))
    (fp_text user + (at -2.3114 -0.0762 90) (layer F.Fab))
    (fp_text user + (at -4.826 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 SCART_Sync))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Solderpads:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 5B0D1F09)
    (at 146.685 89.535 90)
    (fp_text reference P1 (at 0 1.905 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P1-Pad2)"))
  )
  (module Solderpads:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 5B0D1EFC)
    (at 146.685 86.36 90)
    (fp_text reference P2 (at 0 1.905 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P1-Pad2)"))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D42D7)
    (at 122.555 90.805)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 6k8 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 Jamma_Red))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D5839)
    (at 128.27 90.805)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 6k8 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 Jamma_Green))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D4254)
    (at 133.985 90.805)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 6k8 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Jamma_Blue))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D4266)
    (at 139.7 90.805)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 6k8 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 Jamma_Sync))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D217E)
    (at 139.7 87.63)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 430 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D4243)
    (at 133.985 87.63)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 1k4 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D427B)
    (at 128.27 87.63)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 1k4 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D42AF)
    (at 122.555 87.63)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 1k4 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D21DA)
    (at 122.555 72.39 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 1.397 180) (layer F.SilkS))
    (fp_text value 75R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D2161)
    (at 128.27 72.39 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -0.127 1.397 180) (layer F.SilkS))
    (fp_text value 75R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D4322)
    (at 134.112 72.39 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.397 180) (layer F.SilkS))
    (fp_text value 75R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B0D434A)
    (at 134.112 75.438 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.397 180) (layer F.SilkS))
    (fp_text value 75R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R12-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-14_5.3x6.2mm_Pitch0.65mm (layer F.Cu) (tedit 5B0D4335)
    (at 125.095 80.01 90)
    (descr "SSOP14: plastic shrink small outline package; 14 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot337-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -4.2 90) (layer F.SilkS))
    (fp_text value THS7374 (at 0 4.2 90) (layer F.Fab))
    (pad 1 smd rect (at -3.45 -1.95 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -3.45 -1.3 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 3 smd rect (at -3.45 -0.65 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 4 smd rect (at -3.45 0 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R4-Pad1)"))
    (pad 5 smd rect (at -3.45 0.65 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -3.45 1.3 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -3.45 1.95 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.45 1.95 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 3.45 1.3 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P1-Pad2)"))
    (pad 10 smd rect (at 3.45 0.65 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 11 smd rect (at 3.45 0 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R12-Pad2)"))
    (pad 12 smd rect (at 3.45 -0.65 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R11-Pad2)"))
    (pad 13 smd rect (at 3.45 -1.3 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R10-Pad2)"))
    (pad 14 smd rect (at 3.45 -1.95 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R9-Pad2)"))
    (model Housings_SSOP.3dshapes/SSOP-14_5.3x6.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 121.285 96.52)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W1 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value Jamma_Red (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 10 Jamma_Red))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 131.445 96.52)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W2 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value Jamma_Blue (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 12 Jamma_Blue))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 126.365 96.52)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W3 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value Jamma_Green (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 14 Jamma_Green))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 136.525 96.52)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W4 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value "Jamma Sync" (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 16 Jamma_Sync))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 121.285 55.245)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W5 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value SCART_Red (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 4 SCART_Red))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 126.365 55.245)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W6 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value SCART_Blue (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 6 SCART_Green))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 131.445 55.245)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W7 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value SCART_Green (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 22 SCART_Blue))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 136.525 55.245)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W8 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value SCART_Sync (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 8 SCART_Sync))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 141.605 96.52)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W9 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value GND_IN (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 141.605 55.245)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W10 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value GND_OUT (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 146.685 96.52)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W11 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value +5V_IN (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Solderpads:SolderWirePad_single_SMD_3x5mm (layer F.Cu) (tedit 5B051DC6)
    (at 146.685 55.245)
    (descr "Wire Pad, Square, SMD Pad,  2mm x 3mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W12 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value +5V_OUT (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 132.08 83.058 90)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0 90) (layer F.Fab) hide)
  )
  (module cmvs-rgb:logo (layer B.Cu) (tedit 0)
    (at 140.97 64.135 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (gr_text . (at 122.555 81.28) (layer F.SilkS))
  (gr_text "Part:\nU1\nR1,R2,R3,R4\nR5\nR6,R7,R8\nR9,R10,R11,R12\nC1\nC2,C3,C4\n" (at 127 59.69 90) (layer B.SilkS))
  (gr_text "SCART Output" (at 133.985 55.499 180) (layer B.SilkS))
  (gr_text "Jamma Input" (at 134.112 96.266) (layer B.SilkS))
  (gr_line (start 119.507 99.06) (end 148.463 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.507 52.705) (end 119.507 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.463 52.705) (end 119.507 52.705) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.463 99.06) (end 148.463 52.705) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text +5V (at 146.685 58.801 180) (layer F.SilkS))
  (gr_text Gnd (at 141.605 58.801 180) (layer F.SilkS))
  (gr_text S (at 136.525 58.801 180) (layer F.SilkS))
  (gr_text B (at 131.445 58.801 180) (layer F.SilkS))
  (gr_text G (at 126.365 58.801 180) (layer F.SilkS))
  (gr_text R (at 121.285 58.801 180) (layer F.SilkS))
  (gr_text +5V (at 146.558 93.091) (layer F.SilkS))
  (gr_text Gnd (at 141.605 93.091) (layer F.SilkS))
  (gr_text S (at 136.525 93.091) (layer F.SilkS))
  (gr_text B (at 131.445 93.091) (layer F.SilkS))
  (gr_text G (at 126.365 93.091) (layer F.SilkS))
  (gr_text R (at 121.285 93.091) (layer F.SilkS))
  (gr_text OFF (at 144.78 89.408 90) (layer F.SilkS))
  (gr_text ON (at 144.78 86.614 90) (layer F.SilkS))
  (gr_text LPF (at 142.875 88.265 90) (layer F.SilkS))
  (gr_text "Value:\nTHS7374\n6k8\n430R\n1k4\n75R\n0.1uF\n220uF\n" (at 127 73.025 90) (layer B.SilkS))
  (gr_text "Footprint:\nSSOP14\n0805\n0805\n0805\n0805\n0805\n8x10" (at 127 80.645 90) (layer B.SilkS))
  (gr_text " philenotfound \n<phil@zankapfel.net>" (at 145.415 85.725 90) (layer B.SilkS))
  (gr_text "CMVS-RGB\nV2" (at 139.065 84.836 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.463 99.06) (xy 119.507 99.06) (xy 119.507 52.705) (xy 148.463 52.705)
      )
    )
  )
)
