<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="9.99998125" y1="0" x2="89.99981875" y2="0" width="0" layer="20"/>
<wire x1="89.99981875" y1="0" x2="89.99981875" y2="19.999959375" width="0" layer="20"/>
<wire x1="89.99981875" y1="19.999959375" x2="9.99998125" y2="19.999959375" width="0" layer="20"/>
<wire x1="9.99998125" y1="19.999959375" x2="9.99998125" y2="0" width="0" layer="20"/>
<text>PlayVideo
Interface V1.1</text>
<text>1</text>
<text>1</text>
<text>2</text>
<text>STOP</text>
<text>START</text>
<text>REV</text>
<text>FWD</text>
<text>K</text>
<text>K</text>
<text>+</text>
<text>+</text>
<text>Green</text>
<text>Red</text>
<text>C  NO  NC</text>
<text>C  NO  NC</text>
</plain>
<libraries>
<library name="Newlib">
<description>&lt;b&gt;Harting Ribbon Cable Connectors&lt;/b&gt;&lt;p&gt;
This library includes the former libraries ribcon.lbr and ribcon4.lbr.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MONOJACK3_5MM">
<description>Schurter 3.5 mm mono phone jack 4832.2211</description>
</package>
<package name="ESWITCH700SP7B10M2QEH">
<description>E-Switch PCB terminals (e.g., 700SP7B10M2QEH)</description>
</package>
<package name="SIMPLERF">
<description>Adafruit Simple RF receiver for KEYFOB</description>
</package>
<package name="TO92-2N7000">
<description>&lt;b&gt;TO-92 for 2N7000&lt;/b&gt; Pads Triangle</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA05-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FWD" library="Newlib" package="MONOJACK3_5MM" value="Mono Jack"/>
<element name="LED1" library="led" package="LED3MM" value="RED">
<attribute name="MF" value="VISHAY SEMICONDUCTOR"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1612435"/>
<attribute name="POPULARITY" value="7"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED3MM" value="GREEN">
<attribute name="MF" value="VISHAY SEMICONDUCTOR"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1612435"/>
<attribute name="POPULARITY" value="7"/>
<attribute name="VALUE"/>
</element>
<element name="PUSHBUTTON1" library="Newlib" package="ESWITCH700SP7B10M2QEH" value="START"/>
<element name="PUSHBUTTON2" library="Newlib" package="ESWITCH700SP7B10M2QEH" value="STOP"/>
<element name="Q1" library="Newlib" package="TO92-2N7000" value="2N7000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Newlib" package="TO92-2N7000" value="2N7000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0207/10" value="2.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="REV" library="Newlib" package="MONOJACK3_5MM" value="Mono Jack"/>
<element name="RF1" library="Newlib" package="SIMPLERF" value="M4 Receiver">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-lstb" package="MA05-2" value="DIP Header">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="14"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0207/10" value="2.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="Q2" pad="1"/>
<contactref element="LED2" pad="K"/>
<contactref element="Q1" pad="1"/>
<contactref element="LED1" pad="K"/>
<contactref element="FWD" pad="P1"/>
<contactref element="REV" pad="P1"/>
<contactref element="PUSHBUTTON2" pad="P2"/>
<contactref element="RF1" pad="GND"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="RF1" pad="D2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="RF1" pad="D3"/>
<contactref element="Q2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="FWD" pad="P3"/>
<contactref element="Q1" pad="3"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="REV" pad="P3"/>
<contactref element="Q2" pad="3"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="RF1" pad="5V"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="SV1" pad="7"/>
<contactref element="PUSHBUTTON2" pad="P1"/>
</signal>
<signal name="N$10">
<contactref element="PUSHBUTTON1" pad="P1"/>
<contactref element="SV1" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="PUSHBUTTON1" pad="P2"/>
<contactref element="SV1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
