(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 27)
    (no_connects 0)
    (area 120.424999 95.924999 162.575001 123.575001)
    (thickness 1.6)
    (drawings 9)
    (tracks 62)
    (zones 0)
    (modules 17)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.86406)
    (user_trace_width 1)
    (user_trace_width 1.86406)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.6 5.6)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(L3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(L3-Pad2)")
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5991CFFC)
    (at 136 104.25 270)
    (attr smd)
    (fp_text reference C1 (at 3.37 -0.12 360) (layer F.SilkS))
    (fp_text value 18pF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5991D00C)
    (at 147 104.25 270)
    (attr smd)
    (fp_text reference C2 (at 3.35 -0.13 360) (layer F.SilkS))
    (fp_text value 18pF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5991D108)
    (at 132 116.75)
    (attr smd)
    (fp_text reference C3 (at 0.02 2.53) (layer F.SilkS))
    (fp_text value 4.7pF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5991D109)
    (at 142.5 116.75)
    (attr smd)
    (fp_text reference C4 (at 0.22 2.26) (layer F.SilkS))
    (fp_text value 2.7pF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5991D103)
    (at 152 116.75)
    (attr smd)
    (fp_text reference C5 (at 0.13 2.19) (layer F.SilkS))
    (fp_text value 4.7pF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module 2m&70cm_diplexer:Vishay_1008 (layer F.Cu) (tedit 5991CFF6)
    (at 130.25 103.25)
    (fp_text reference L1 (at 1.45 1.52) (layer F.SilkS))
    (fp_text value 68nH (at 0.75 -3) (layer F.Fab))
    (pad 1 smd rect (at 0.25 -1) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2.25 -1) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module 2m&70cm_diplexer:Vishay_1008 (layer F.Cu) (tedit 5991D000)
    (at 140 103.25)
    (fp_text reference L2 (at 1.38 1.08) (layer F.SilkS))
    (fp_text value 100nH (at 0.75 -3) (layer F.Fab))
    (pad 1 smd rect (at 0.25 -1) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.25 -1) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module 2m&70cm_diplexer:Vishay_1008 (layer F.Cu) (tedit 5991D00F)
    (at 150.5 103.25)
    (fp_text reference L3 (at 1.24 1.08) (layer F.SilkS))
    (fp_text value 68nH (at 0.75 -3) (layer F.Fab))
    (pad 1 smd rect (at 0.25 -1) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2.25 -1) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(L3-Pad2)"))
  )
  (module 2m&70cm_diplexer:Vishay_1008 (layer F.Cu) (tedit 5991CFE4)
    (at 138 117 90)
    (fp_text reference L4 (at 3.52 -0.85 180) (layer F.SilkS))
    (fp_text value 15nH (at 0.75 -3 90) (layer F.Fab))
    (pad 1 smd rect (at 0.25 -1 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 2.25 -1 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module 2m&70cm_diplexer:Vishay_1008 (layer F.Cu) (tedit 5991CFDB)
    (at 148 117 90)
    (fp_text reference L5 (at 3.74 -1.01 180) (layer F.SilkS))
    (fp_text value 15nH (at 0.75 -3 90) (layer F.Fab))
    (pad 1 smd rect (at 0.25 -1 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 2.25 -1 90) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5991D728)
    (at 152.2 109.6)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5991D808)
    (at 124.5 119.5)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5991D724)
    (at 124.5 99.5)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module 2m&70cm_diplexer:LOGO (layer B.Cu) (tedit 5991E257)
    (at 136.75 108.85 270)
    (fp_text reference G*** (at 10 -8 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at -8 -8 270) (layer B.SilkS) hide)
  )
  (module 2m&70cm_diplexer:SMAEndLaunch (layer F.Cu) (tedit 59946DFA)
    (at 159.6 102.2 90)
    (fp_text reference SMA2m1 (at 0.05 -3.65 90) (layer B.SilkS))
    (fp_text value 2m (at 0.05 3.5 90) (layer F.Fab))
    (pad 2 smd rect (at -2.75 0.15 90) (size 1.6 4.9) (layers *.Paste *.Mask B.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 2.75 0.15 90) (size 1.6 4.9) (layers *.Paste *.Mask B.Cu)
      (net 2 GND))
    (pad 2 smd rect (at -2.75 0.15 90) (size 1.6 4.9) (layers *.Paste *.Mask F.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 2.75 0.15 90) (size 1.6 4.9) (layers *.Paste *.Mask F.Cu)
      (net 2 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.5 5.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(L3-Pad2)"))
  )
  (module 2m&70cm_diplexer:SMAEndLaunch (layer F.Cu) (tedit 59946DFF)
    (at 159.6 117.2 90)
    (fp_text reference SMA70cm1 (at -0.05 -3.9 90) (layer B.SilkS))
    (fp_text value 70cm (at 0.05 3.5 90) (layer F.Fab))
    (pad 2 smd rect (at -2.75 0.15 90) (size 1.6 4.9) (layers *.Paste *.Mask B.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 2.75 0.15 90) (size 1.6 4.9) (layers *.Paste *.Mask B.Cu)
      (net 2 GND))
    (pad 2 smd rect (at -2.75 0.15 90) (size 1.6 4.9) (layers *.Paste *.Mask F.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 2.75 0.15 90) (size 1.6 4.9) (layers *.Paste *.Mask F.Cu)
      (net 2 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.5 5.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
  )
  (module 2m&70cm_diplexer:SMAEndLaunch (layer F.Cu) (tedit 59946E06)
    (at 123.35 109.25 270)
    (fp_text reference Radio1 (at -0.05 -3.55 270) (layer B.SilkS))
    (fp_text value Radio1 (at 0.05 3.5 270) (layer F.Fab))
    (pad 2 smd rect (at -2.75 0.15 270) (size 1.6 4.9) (layers *.Paste *.Mask B.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 2.75 0.15 270) (size 1.6 4.9) (layers *.Paste *.Mask B.Cu)
      (net 2 GND))
    (pad 2 smd rect (at -2.75 0.15 270) (size 1.6 4.9) (layers *.Paste *.Mask F.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 2.75 0.15 270) (size 1.6 4.9) (layers *.Paste *.Mask F.Cu)
      (net 2 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.5 5.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (gr_text "Dr.Squeakerton : 2m - 7cm Diplexer" (at 148.3 109.75 90) (layer B.SilkS))
  (gr_line (start 160.5 123.5) (end 122.5 123.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.5 96) (end 160.5 96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.5 121.5) (end 120.5 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 122.5 98) (end 120.5 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 122.5 121.5) (end 122.5 123.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.5 121.5) (end 162.5 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.5 98) (end 160.5 96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.5 121.5) (end 162.5 121.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164 124) (xy 118 124) (xy 118 95) (xy 164 95)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164 124) (xy 118 124) (xy 118 95) (xy 164 95)
      )
    )
  )
)
