<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="18.80949375" x2="0" y2="1.40746875" width="0" layer="20"/>
<wire x1="0" y1="1.40746875" x2="1.40746875" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.40746875" y1="0" x2="45.57210625" y2="0" width="0" layer="20"/>
<wire x1="45.57210625" y1="0" x2="46.914" y2="1.34189375" width="0" layer="20" curve="90"/>
<wire x1="46.914" y1="1.34189375" x2="46.914" y2="18.98454375" width="0" layer="20"/>
<wire x1="46.914" y1="18.98454375" x2="45.58854375" y2="20.31" width="0" layer="20" curve="90"/>
<wire x1="45.58854375" y1="20.31" x2="1.50050625" y2="20.31" width="0" layer="20"/>
<wire x1="1.50050625" y1="20.31" x2="0" y2="18.80949375" width="0" layer="20" curve="90"/>
<text>12v</text>
<text>LIMIT</text>
<text>RV-Project.Com PWM LED Dimmer
</text>
<text>V2.2   4/21/2019</text>
<text>GND</text>
<text>LIMIT</text>
<text>12v</text>
<text>GND</text>
<text>Low Power Option</text>
<text>High Power Option</text>
<text>LED-</text>
<text>LED+</text>
<text>1.4A Max</text>
<text>2A Max</text>
<text>Order 2Oz Copper</text>
<text>NE555</text>
<text>Low Power Option: 250mA</text>
<text>High Power Option: 1.4A</text>
<text>Low Side Switching</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="SOD-123">
<description>Suitable for 4148
&lt;br&gt;Pad Size:  0.55"x0.8"</description>
</package>
<package name="1X02">
<description>Pitch: 0.1" (2.54mm)&lt;br&gt;Drill: 0.040" dia</description>
</package>
<package name="1X03">
<description>Pitch: 0.1" (2.54mm)
&lt;br&gt;Drill: 0.040" dia</description>
</package>
<package name="1206-RES">
</package>
<package name="FUSE476">
<description>Pad Size: 0.38"x0.15"</description>
</package>
<package name="RV097NS">
</package>
</packages>
</library>
<library name="a-lib_SMD">
<description>All SMD Devices; Actives, Passives, Connectors</description>
<packages>
<package name="SOIC-8(.150MM)">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;SMA diode.&lt;br&gt;
Pad Size: 0.225"x0.07"</description>
</package>
<package name="SOT23-3">
<description>SMD MMBT2222, BAV90, etc.</description>
</package>
<package name="1206-CAP">
</package>
<package name="SOT223-(SC73)">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_MEDIUM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="a-lib" package="SOD-123" value="TVS-SSOD123">
<attribute name="NAME"/>
</element>
<element name="J2" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="J3" library="a-lib" package="1X03" value="M3HEADER"/>
<element name="R4" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="a-lib" package="FUSE476" value="2.5A">
<attribute name="NAME"/>
</element>
<element name="R2" library="a-lib" package="RV097NS" value="50k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="U1" library="a-lib_SMD" package="SOIC-8(.150MM)" value=""/>
<element name="D2" library="a-lib_SMD" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="a-lib_SMD" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="a-lib_SMD" package="SOT23-3" value="">
<attribute name="PARTNO" value="MBT2222"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="a-lib_SMD" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="a-lib_SMD" package="1206-CAP" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="a-lib_SMD" package="SOT223-(SC73)" value="BUK98150"/>
<element name="U$1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_MEDIUM" value=""/>
<element name="C3" library="a-lib_SMD" package="1206-CAP" value="1nF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="P$1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="P$3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="F1" pad="P$2"/>
<contactref element="D1" pad="C"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="P$8"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="P$4"/>
<contactref element="R2" pad="S2"/>
<contactref element="R5" pad="1"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="2"/>
<contactref element="F1" pad="P$1"/>
<contactref element="R2" pad="S1"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="C"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="D3" pad="A"/>
<contactref element="D2" pad="C"/>
<contactref element="U1" pad="P$7"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="P$6"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="P$5"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="P$3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="P$1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="P$4"/>
<contactref element="Q2" pad="P$2"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="J3" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
