(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 53)
    (zones 0)
    (modules 2)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad4)")
  (net 2 "Net-(J1-Pad6)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
  )
  (module Custom:gb-link-socket-nolabel (layer F.Cu) (tedit 5DE590F2)
    (at 56.4489 136.017 270)
    (fp_text reference J1 (at 0 -3.25374 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 0.5 4 90) (layer F.Fab))
    (pad 4 connect rect (at 0 0 270) (size 1 5) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 6 connect rect (at 2 0 270) (size 1 5) (layers F.Cu F.Mask)
      (net 2 "Net-(J1-Pad6)"))
    (pad 2 connect rect (at -2 0 270) (size 1 5) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 5 connect rect (at 2 0 270) (size 1 5) (layers B.Cu B.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 3 connect rect (at 0 0 270) (size 1 5) (layers B.Cu B.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 1 connect rect (at -2 0 270) (size 1 5) (layers B.Cu B.Mask)
      (net 6 "Net-(J1-Pad1)"))
  )
  (module Custom:gb-link-socket-nolabel (layer F.Cu) (tedit 5DE590F2)
    (at 67.7151 136.017 90)
    (fp_text reference J2 (at 0 -3.25374 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 0.5 4.5 90) (layer F.Fab))
    (pad 1 connect rect (at -2 0 90) (size 1 5) (layers B.Cu B.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 3 connect rect (at 0 0 90) (size 1 5) (layers B.Cu B.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 5 connect rect (at 2 0 90) (size 1 5) (layers B.Cu B.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 2 connect rect (at -2 0 90) (size 1 5) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 6 connect rect (at 2 0 90) (size 1 5) (layers F.Cu F.Mask)
      (net 2 "Net-(J1-Pad6)"))
    (pad 4 connect rect (at 0 0 90) (size 1 5) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-Pad4)"))
  )
  (gr_line (start 61.082043 133.01682) (end 63.082043 133.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.082043 132.01682) (end 63.082043 133.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 61.082043 139.01682) (end 63.082043 139.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.082043 140.01682) (end 65.082043 140.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 61.082043 139.01682) (end 61.082043 140.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.082043 140.01682) (end 63.082043 139.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 61.082043 132.01682) (end 61.082043 133.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 61.082043 132.01682) (end 59.082043 132.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 61.082043 140.01682) (end 59.082043 140.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.082043 132.01682) (end 63.082043 132.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.082043 132.01682) (end 65.082043 133.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.082043 139.01682) (end 65.082043 140.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 59.082043 139.01682) (end 59.082043 140.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 59.082043 132.01682) (end 59.082043 133.01682) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 70.582043 133.01682) (end 65.082043 133.01682) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 70.582043 138.51682) (end 71.082043 138.51682) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 70.582043 133.51682) (end 70.582043 133.01682) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 71.082043 133.51682) (end 71.082043 138.51682) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 70.582043 139.01682) (end 65.082043 139.01682) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53.582043 133.01682) (end 59.082043 133.01682) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53.582043 139.01682) (end 59.082043 139.01682) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 53.582043 138.51682) (end 53.582043 139.01682) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53.082043 138.51682) (end 53.082043 133.51682) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 53.582043 133.51682) (end 53.082043 133.51682) (angle 90) (layer Edge.Cuts) (width 0.05))
)
