(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 97)
    (zones 0)
    (modules 4)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4064)
    (trace_clearance 0)
    (zone_clearance 0.4)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFDFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "1.27mm to 2.54mm adapter/"))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0)
    (trace_width 0.4064)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch1.27mm (layer F.Cu) (tedit 5C9BC653)
    (at 139.5 100.25 270)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (solder_mask_margin 0.01)
    (fp_text reference 1.27mm (at -0.25 8.25 90) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_2x05_Pitch1.27mm (at 0.635 6.775 270) (layer F.Fab))
    (fp_text user %R (at 0.635 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 1.27 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.27 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 1.27 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 1.27 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Tag-Connect_EC-10 (layer F.Cu) (tedit 5C9AEE79)
    (at 152.35 102.35 180)
    (descr http://www.tag-connect.com/Materials/Edge-Connect/EC-10_RevA.PDF)
    (tags "tag connect programming header edge connector")
    (solder_mask_margin 0.01)
    (attr virtual)
    (fp_text reference PF1 (at 0 2.7 180) (layer F.SilkS) hide)
    (fp_text value EC-10 (at -2.9 0.8 180) (layer F.Fab) hide)
    (fp_text user %R (at 2 0.8 180) (layer F.Fab))
    (pad 1r smd rect (at 6.35 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 2r smd rect (at 5.08 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 3r smd rect (at 3.81 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 4r smd rect (at 2.54 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 5r smd rect (at 1.27 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 6r smd rect (at -1.27 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 7r smd rect (at -2.54 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 8r smd rect (at -3.81 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 9r smd rect (at -5.08 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 10r smd rect (at -6.35 -0.75 180) (size 1 0.5) (layers B.Cu F.Paste F.Mask))
    (pad 10r smd rect (at -6.35 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 10 thru_hole circle (at -6.35 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -5.08 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 9r smd rect (at -5.08 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 8r smd rect (at -3.81 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 8 thru_hole circle (at -3.81 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -2.54 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 7r smd rect (at -2.54 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 6r smd rect (at -1.27 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 5r smd rect (at 1.27 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 4r smd rect (at 2.54 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 3r smd rect (at 3.81 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 2r smd rect (at 5.08 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 6 thru_hole circle (at -1.27 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 1.27 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 3.81 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5.08 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.35 -1 180) (size 1 1) (drill 0.81) (layers *.Cu *.Mask))
    (pad 1r smd rect (at 6.35 -0.75 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5C9AF30E)
    (at 133.75 93.25 90)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference 2.54mm (at -2.25 -0.25) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x12_Pitch2.54mm (at 0 30.27 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch1.27mm (layer F.Cu) (tedit 5C9AEF33)
    (at 146 100 90)
    (descr "Through hole straight pin header, 1x12, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x12 1.27mm single row")
    (solder_mask_margin 0.01)
    (fp_text reference 1.27mm (at 2.25 -0.25 180) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x12_Pitch1.27mm (at 0 15.665 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.985 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 6.35 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 8.89 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 11.43 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 13.97 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Gnd (at 137.75 97.25 90) (layer F.SilkS))
  (gr_text SDA (at 159 96.75 270) (layer F.SilkS))
  (gr_text SCL (at 157.25 96.75 280) (layer F.SilkS))
  (gr_text Rst (at 132 101.75) (layer F.SilkS))
  (gr_text - (at 135.75 98.5) (layer F.SilkS))
  (gr_text DIO (at 141.75 101.75) (layer F.SilkS))
  (gr_text Vt (at 139.75 98 90) (layer F.SilkS))
  (gr_text V (at 148.5 102) (layer F.SilkS))
  (gr_text R (at 149.75 102) (layer F.SilkS))
  (gr_text D (at 151 102) (layer F.SilkS))
  (gr_text O (at 156 102) (layer F.SilkS))
  (gr_text K (at 154.75 102) (layer F.SilkS))
  (gr_text G (at 153.5 102) (layer F.SilkS))
  (gr_line (start 129.54 103.378) (end 129.54 91.186) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.83 103.378) (end 129.54 103.378) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.83 91.186) (end 163.83 103.378) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 91.186) (end 163.83 91.186) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text EC-10 (at 163 100.75 90) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.83 103.378) (xy 129.5 103.346) (xy 129.5 91.154) (xy 163.83 91.186)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.83 103.378) (xy 129.5 103.346) (xy 129.5 91.154) (xy 163.83 91.186)
      )
    )
  )
)
