(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 185)
    (zones 0)
    (modules 23)
    (nets 41)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad16)")
  (net 2 "Net-(A1-Pad15)")
  (net 3 +12V)
  (net 4 "Net-(A1-Pad14)")
  (net 5 GND)
  (net 6 "Net-(A1-Pad13)")
  (net 7 "Net-(A1-Pad28)")
  (net 8 "Net-(A1-Pad12)")
  (net 9 "Net-(A1-Pad11)")
  (net 10 "Net-(A1-Pad26)")
  (net 11 "Net-(A1-Pad10)")
  (net 12 "Net-(A1-Pad25)")
  (net 13 "Net-(A1-Pad9)")
  (net 14 "Net-(A1-Pad24)")
  (net 15 "Net-(A1-Pad8)")
  (net 16 "Net-(A1-Pad23)")
  (net 17 "Net-(A1-Pad7)")
  (net 18 "Net-(A1-Pad22)")
  (net 19 "Net-(A1-Pad6)")
  (net 20 "Net-(A1-Pad21)")
  (net 21 "Net-(A1-Pad5)")
  (net 22 "Net-(A1-Pad20)")
  (net 23 "Net-(A1-Pad19)")
  (net 24 "Net-(A1-Pad3)")
  (net 25 "Net-(A1-Pad18)")
  (net 26 "Net-(A1-Pad2)")
  (net 27 "Net-(A1-Pad17)")
  (net 28 "Net-(A1-Pad1)")
  (net 29 "Net-(BTN1-Pad2)")
  (net 30 "Net-(BTN2-Pad2)")
  (net 31 "Net-(BTN3-Pad2)")
  (net 32 "Net-(BTN4-Pad2)")
  (net 33 "Net-(BTN5-Pad2)")
  (net 34 "Net-(BTN6-Pad2)")
  (net 35 "Net-(BTN7-Pad2)")
  (net 36 "Net-(BTN8-Pad2)")
  (net 37 +5V)
  (net 38 "Net-(R7-Pad2)")
  (net 39 "Net-(J1-Pad1)")
  (net 40 "Net-(J1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(BTN1-Pad2)")
    (add_net "Net-(BTN2-Pad2)")
    (add_net "Net-(BTN3-Pad2)")
    (add_net "Net-(BTN4-Pad2)")
    (add_net "Net-(BTN5-Pad2)")
    (add_net "Net-(BTN6-Pad2)")
    (add_net "Net-(BTN7-Pad2)")
    (add_net "Net-(BTN8-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(R7-Pad2)")
  )
  (module digikey-footprints:RJ45_8-[E5J88-00LJG2-L] (layer F.Cu) (tedit 61AE151B)
    (at 138.43 52.07 90)
    (tags RJ45)
    (fp_text reference J1 (at 2.92 -11.18 90) (layer F.SilkS))
    (fp_text value 8P8C (at 3.32 -6.25 270) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 9.9 -2.54 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -2.8 -2.54 90) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 1.02 1.78 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at 2.04 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 3.06 1.78 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 5 thru_hole circle (at 4.08 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 6 thru_hole circle (at 5.1 1.78 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad3)"))
    (pad 7 thru_hole circle (at 6.12 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 8 thru_hole circle (at 7.14 1.78 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad15)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/RJ45_8.wrl
      (offset (xyz 4.571999931335449 -6.349999904632568 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SW_PUSH_6mm-[TS02-66-60-BK-100-SCR-D-ND] (layer F.Cu) (tedit 5923F252)
    (at 193.04 53.34)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference Rec1 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SW_PUSH_6mm-[TS02-66-60-BK-100-SCR-D-ND] (layer F.Cu) (tedit 5923F252)
    (at 193.04 66.04)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BTN8 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(BTN8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(BTN8-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SW_PUSH_6mm-[TS02-66-60-BK-100-SCR-D-ND] (layer F.Cu) (tedit 5923F252)
    (at 182.88 66.04)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BTN7 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(BTN7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(BTN7-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SW_PUSH_6mm-[TS02-66-60-BK-100-SCR-D-ND] (layer F.Cu) (tedit 5923F252)
    (at 172.72 66.04)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BTN6 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(BTN6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(BTN6-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SW_PUSH_6mm-[TS02-66-60-BK-100-SCR-D-ND] (layer F.Cu) (tedit 5923F252)
    (at 162.56 66.04)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BTN5 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.42 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(BTN5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(BTN5-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SW_PUSH_6mm-[TS02-66-60-BK-100-SCR-D-ND] (layer F.Cu) (tedit 5923F252)
    (at 152.4 66.04)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BTN4 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(BTN4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(BTN4-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SW_PUSH_6mm-[TS02-66-60-BK-100-SCR-D-ND] (layer F.Cu) (tedit 5923F252)
    (at 142.24 66.04)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BTN3 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(BTN3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(BTN3-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SW_PUSH_6mm-[TS02-66-60-BK-100-SCR-D-ND] (layer F.Cu) (tedit 5923F252)
    (at 132.08 66.04)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BTN2 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "Net-(BTN2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "Net-(BTN2-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SW_PUSH_6mm-[TS02-66-60-BK-100-SCR-D-ND] (layer F.Cu) (tedit 5923F252)
    (at 121.92 66.04)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BTN1 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 "Net-(BTN1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 "Net-(BTN1-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 162.56 46.99 180)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R12 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(A1-Pad1)"))
    (pad 2 smd rect (at 2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J1-Pad1)"))
    (pad 1 thru_hole rect (at -5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad1)"))
    (pad 2 thru_hole rect (at 5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 162.56 50.8 180)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R11 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(A1-Pad2)"))
    (pad 2 smd rect (at 2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J1-Pad3)"))
    (pad 1 thru_hole rect (at -5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad2)"))
    (pad 2 thru_hole rect (at 5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad3)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 152.33904 59.69 180)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R10 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(A1-Pad7)"))
    (pad 2 smd rect (at 2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(BTN3-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad7)"))
    (pad 2 thru_hole rect (at 5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 31 "Net-(BTN3-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 140.97 62.23 180)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R9 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(A1-Pad6)"))
    (pad 2 smd rect (at 2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(BTN2-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad6)"))
    (pad 2 thru_hole rect (at 5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 30 "Net-(BTN2-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 127 62.23 180)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R8 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(A1-Pad5)"))
    (pad 2 smd rect (at 2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(BTN1-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad5)"))
    (pad 2 thru_hole rect (at 5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 29 "Net-(BTN1-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 182.88 48.32096 90)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R7 (at 0.09906 -2.4003 90) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0 90) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(A1-Pad14)"))
    (pad 2 smd rect (at 2.60096 0 90) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R7-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad14)"))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 38 "Net-(R7-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 194.24904 62.23)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R6 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 2 smd rect (at 2.60096 0) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(BTN8-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 36 "Net-(BTN8-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 184.08904 59.69)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R5 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(A1-Pad11)"))
    (pad 2 smd rect (at 2.60096 0) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(BTN7-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad11)"))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 35 "Net-(BTN7-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 177.86096 62.23)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R4 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(A1-Pad10)"))
    (pad 2 smd rect (at 2.60096 0) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(BTN6-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad10)"))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 34 "Net-(BTN6-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 168.97096 59.69)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R3 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(A1-Pad9)"))
    (pad 2 smd rect (at 2.60096 0) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(BTN5-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad9)"))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 33 "Net-(BTN5-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 160.08096 62.23 180)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R2 (at 0.09906 -2.4003) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(A1-Pad8)"))
    (pad 2 smd rect (at 2.60096 0 180) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(BTN4-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad8)"))
    (pad 2 thru_hole rect (at 5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 32 "Net-(BTN4-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 149.86 48.32096 90)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R1 (at 0.09906 -2.4003 90) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002 90) (layer F.Fab))
    (pad 1 smd rect (at -2.60096 0 90) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(A1-Pad15)"))
    (pad 2 smd rect (at 2.60096 0 90) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 37 +5V))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad15)"))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 37 +5V))
  )
  (module Modules:Arduino_Nano (layer F.Cu) (tedit 58ACAF70)
    (at 149.86 55.88 90)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference A1 (at 7.62 -5.08 90) (layer F.SilkS))
    (fp_text value Arduino_Nano_v3.x (at 8.89 19.05) (layer F.Fab))
    (fp_text user %R (at 6.35 19.05) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad17)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad2)"))
    (pad 18 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad18)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad3)"))
    (pad 19 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad19)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 20 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad20)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad5)"))
    (pad 21 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad21)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad6)"))
    (pad 22 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad22)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad7)"))
    (pad 23 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad23)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad8)"))
    (pad 24 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad24)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad9)"))
    (pad 25 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad25)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad10)"))
    (pad 26 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad26)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad11)"))
    (pad 27 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 +5V))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 28 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad28)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad13)"))
    (pad 29 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad14)"))
    (pad 30 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad15)"))
    (pad 16 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad16)"))
  )
  (gr_text "OCTOFIELD: ARDUINO OCTOBANGER  FIELD PROGRAMMER\nBY: JAMES MANLEY\nORG: SCARE FOR A CURE\nV: 0.0.0.1 2021/11/17\n" (at 177.8 48.26) (layer B.SilkS))
  (gr_text "OCTOFIELD\nUSED TO PROGRAM\nOCTOBANGER\nIN THE FIELD" (at 196.85 44.45) (layer F.SilkS))
  (gr_text USB (at 190.5 48.26 270) (layer F.SilkS))
  (gr_text "ARDUINO \nNANO" (at 175.26 50.8) (layer F.SilkS))
  (gr_line (start 204.47 38.1) (end 118.11 38.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 204.47 73.66) (end 204.47 38.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.11 73.66) (end 204.47 73.66) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.11 38.1) (end 118.11 73.66) (layer Edge.Cuts) (width 0.05))
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.36 33.02) (xy 209.55 82.55) (xy 107.95 76.2) (xy 105.41 50.8) (xy 115.57 31.75)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.52 27.94) (xy 215.9 90.17) (xy 72.39 83.82) (xy 81.28 60.96) (xy 99.06 25.4)
      )
    )
  )
)
