<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.7" y2="0" width="0" layer="20"/>
<wire x1="15.7" y1="0" x2="15.7" y2="15.6" width="0" layer="20"/>
<wire x1="15.7" y1="15.6" x2="0" y2="15.6" width="0" layer="20"/>
<wire x1="0" y1="15.6" x2="0" y2="0" width="0" layer="20"/>
<text>Rev 1</text>
<text>TLV2361 Breakout</text>
<text>V+</text>
<text>GND</text>
<text>5V</text>
<text>IN+</text>
<text>V-</text>
<text>IN-</text>
<text>-1.8V</text>
<text>+1.8V</text>
<text>OUT</text>
</plain>
<libraries>
<library name="_capacitors">
<packages>
<package name="CAPC1005X55_SMD-0402">
<description>CHIP, 1 X 0.5 X 0.55 mm body
&lt;p&gt;CHIP package with body size 1 X 0.5 X 0.55 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_inductors">
<packages>
<package name="INDC1608X60-0603">
<description>CHIP, 1.6 X 0.8 X 0.6 mm body
&lt;p&gt;CHIP package with body size 1.6 X 0.8 X 0.6 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_op_amps">
<packages>
<package name="SOT95P280X145-5">
<description>5-SOT23, 0.95 mm pitch, 2.80 mm span, 2.90 X 1.60 X 1.45 mm body
&lt;p&gt;5-pin SOT23 package with 0.95 mm pitch, 2.80 mm span with body size 2.90 X 1.60 X 1.45 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_ic_power">
<packages>
<package name="SOT95P275X100-6">
<description>6-SOT23, 0.95 mm pitch, 2.75 mm span, 3.00 X 1.50 X 1.00 mm body
&lt;p&gt;6-pin SOT23 package with 0.95 mm pitch, 2.75 mm span with body size 3.00 X 1.50 X 1.00 mm&lt;/p&gt;</description>
</package>
<package name="SOT95P280X145-5">
<description>5-SOT23, 0.95 mm pitch, 2.8 mm span, 2.9 X 1.6 X 1.45 mm body
&lt;p&gt;5-pin SOT23 package with 0.95 mm pitch, 2.8 mm span with body size 2.9 X 1.6 X 1.45 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_connectors">
<packages>
<package name="HDRV6W64P254_1X6_1524X254X838B">
<description>Single-row, 6-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 15.24 X 2.54 X 8.38 mm body
&lt;p&gt;Single-row (1X6), 6-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.05 mm tail length and 5.84 mm mating length with overall size 15.24 X 2.54 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="HDRV3W64P254_1X3_762X254X838B">
<description>Single-row, 3-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 7.62 X 2.54 X 8.38 mm body
&lt;p&gt;Single-row (1X3), 3-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.05 mm tail length and 5.84 mm mating length with overall size 7.62 X 2.54 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="_capacitors" package="CAPC1005X55_SMD-0402" value="4.7uF/10V/0402">
<attribute name="DATASHEET" value="http://www.samsungsem.com/kr/support/product-search/mlcc/CL05A475MP5NRNC.jsp"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=1276-1482-1-ND"/>
<attribute name="DISTPN" value="1276-1482-1-ND"/>
<attribute name="MFR" value="Samsung Electro-Mechanics"/>
<attribute name="MPN" value="CL05A475MP5NRNC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="_capacitors" package="CAPC1005X55_SMD-0402" value="10uF/6.3V">
<attribute name="DATASHEET" value="https://www.murata.com/~/media/webrenewal/support/library/catalog/products/capacitor/mlcc/c02e.ashx"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-13233-1-ND"/>
<attribute name="DISTPN" value="490-13233-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM155C80J106ME11D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="_inductors" package="INDC1608X60-0603" value="10uH/380mA">
<attribute name="DATASHEET" value="http://ds.yuden.co.jp/TYCOMPAS/ut/detail.do?productNo=CBMF1608T100K&amp;fileName=CBMF1608T100K_SS&amp;mode=specSheetDownload"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=587-1720-1-ND"/>
<attribute name="DISTPN" value="587-1720-1-ND"/>
<attribute name="MFR" value="Taiyo Yuden"/>
<attribute name="MPN" value="Taiyo Yuden"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OPAMP1" library="_op_amps" package="SOT95P280X145-5" value="TLV2361_GP_20MA_7MHZ">
<attribute name="DATASHEET" value="http://www.ti.com/lit/ds/symlink/tlv2361.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=296-13745-1-ND"/>
<attribute name="DISTPN" value="296-13745-1-ND"/>
<attribute name="MFR" value="Texas Instruments"/>
<attribute name="MPN" value="TLV2361IDBVR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUR" value="TLV2361"/>
</element>
<element name="VREG1" library="_ic_power" package="SOT95P275X100-6" value="NCP1729 50mA">
<attribute name="DATASHEET" value="https://www.onsemi.com/pub/Collateral/NCP1729-D.PDF"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=NCV1729SN35T1GOSCT-ND"/>
<attribute name="DISTPN" value="NCV1729SN35T1GOSCT-ND"/>
<attribute name="MFR" value="ON Semiconductor"/>
<attribute name="MPN" value="NCV1729SN35T1G"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VREG2" library="_ic_power" package="SOT95P280X145-5" value="TPS62202 300mA 1.8V">
<attribute name="DATASHEET" value="http://www.ti.com/lit/ds/symlink/tps62200.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=296-16730-1-ND"/>
<attribute name="DISTPN" value="296-16730-1-ND"/>
<attribute name="MFR" value="Texas Instruments"/>
<attribute name="MPN" value="TPS62202DBVR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="_connectors" package="HDRV6W64P254_1X6_1524X254X838B" value="PTH VERT MALE">
<attribute name="DATASHEET" value="https://drawings-pdf.s3.amazonaws.com/C10436.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=PEC06SAAN"/>
<attribute name="DISTPN" value="S1012E-06-ND"/>
<attribute name="MFR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PEC06SAAN"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="_connectors" package="HDRV3W64P254_1X3_762X254X838B" value="PTH VERT MALE">
<attribute name="DATASHEET" value="https://drawings-pdf.s3.amazonaws.com/C10436.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=S1012E-03-ND"/>
<attribute name="DISTPN" value="S1012E-03-ND"/>
<attribute name="MFR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PEC03SAAN"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="V-">
<contactref element="OPAMP1" pad="2"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="V+">
<contactref element="OPAMP1" pad="5"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="IN+">
<contactref element="OPAMP1" pad="1"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="IN-">
<contactref element="OPAMP1" pad="3"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="OUT">
<contactref element="OPAMP1" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="C-">
<contactref element="VREG1" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="C+">
<contactref element="VREG1" pad="6"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="VREG1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="VREG1" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="VREG2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="VREG2" pad="5"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="C4" pad="1"/>
<contactref element="VREG2" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="VREG2" pad="3"/>
</signal>
<signal name="1.8V">
<contactref element="VREG2" pad="4"/>
<contactref element="L1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="VREG1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="-1.8V">
<contactref element="VREG1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
