(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu17.04.1)
  (general
    (links 26)
    (no_connects 3)
    (area 135.383199 76.582199 163.955801 105.662801)
    (thickness 1.6)
    (drawings 19)
    (tracks 101)
    (zones 0)
    (modules 8)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.16)
    (user_trace_width 0.16)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.1)
    (pcb_text_size 0.5 0.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 CSN)
  (net 5 SCK)
  (net 6 MOSI)
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J2-Pad3)")
  (net 10 "Net-(J2-Pad4)")
  (net 11 "Net-(J2-Pad5)")
  (net 12 "Net-(J3-Pad2)")
  (net 13 "Net-(J3-Pad3)")
  (net 14 "Net-(J3-Pad4)")
  (net 15 "Net-(J3-Pad6)")
  (net 16 "Net-(U2-Pad1)")
  (net 17 "Net-(U2-Pad2)")
  (net 18 "Net-(U2-Pad3)")
  (net 19 "Net-(U2-Pad13)")
  (net 20 "Net-(U2-Pad14)")
  (net 21 "Net-(U2-Pad17)")
  (net 22 "Net-(U2-Pad18)")
  (net 23 "Net-(U2-Pad19)")
  (net 24 "Net-(U2-Pad20)")
  (net 25 "Net-(U2-Pad21)")
  (net 26 "Net-(U2-Pad22)")
  (net 27 CE)
  (net 28 "Net-(U2-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net CE)
    (add_net CSN)
    (add_net GND)
    (add_net MOSI)
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad3)")
    (add_net SCK)
  )
  (net_class 6mil ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connect:USB_Mini-B (layer B.Cu) (tedit 59ADA4F1)
    (at 148.59 101.6 90)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference J3 (at -1.4986 -0.0762 90) (layer B.SilkS))
    (fp_text value USB_OTG (at -0.65 7.1 90) (layer B.Fab))
    (pad 1 smd rect (at 2.8 1.6 90) (size 2.3 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2.8 0.8 90) (size 2.3 0.5) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 2.8 0 90) (size 2.3 0.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at 2.8 -0.8 90) (size 2.3 0.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at 2.8 -1.6 90) (size 2.3 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.7 4.45 90) (size 2.5 2) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at -2.8 4.45 90) (size 2.5 2) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at 2.7 -4.45 90) (size 2.5 2) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J3-Pad6)"))
    (pad 6 smd rect (at -2.8 -4.45 90) (size 2.5 2) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J3-Pad6)"))
    (pad "" np_thru_hole circle (at 0.2 2.2 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.2 -2.2 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
  )
  (module ESP8266:ESP-12E_SMD (layer F.Cu) (tedit 58FB7FFE)
    (at 138.43 83.82)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U2 (at 8.89 6.35 90) (layer F.SilkS))
    (fp_text value ESP-12E (at 5.08 6.35 90) (layer F.Fab) hide)
    (fp_text user "No Copper" (at 6.892 -5.4) (layer F.CrtYd))
    (pad 1 smd rect (at 0 0) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at 0 2) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at 0 4) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at 0 6) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 27 CE))
    (pad 5 smd rect (at 0 8) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 SCK))
    (pad 6 smd rect (at 0 10) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 7 smd rect (at 0 12) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 8 smd rect (at 0 14) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 9 smd rect (at 14 14) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 14 12) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 4 CSN))
    (pad 11 smd rect (at 14 10) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 14 8) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad3)"))
    (pad 13 smd rect (at 14 6) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at 14 4) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 14 2) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad4)"))
    (pad 16 smd rect (at 14 0) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad5)"))
    (pad 17 smd rect (at 1.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 3.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad18)"))
    (pad 19 smd rect (at 5.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 7.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 9.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 11.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad22)"))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 59ADBBCB)
    (at 140.843 92.3036 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.1524 -1.651 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 59ADBBD1)
    (at 151.13 90.17 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.254 -1.27 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 159.893 102.5144 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x04_Odd_Even (at 1.27 9.95 180) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 CE))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 CSN))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 SCK))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 MOSI))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3Lead_TabPin2 (layer B.Cu) (tedit 59ADBBDA)
    (at 146.05 90.17 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 2.794 2.794 90) (layer B.SilkS))
    (fp_text value LM1117-3.3 (at 0 -4.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 158.7246 88.8746 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x05_Female (at 0 12.49 180) (layer F.Fab))
    (fp_text user %R (at 0 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59ADBB77)
    (at 139.7 102.87 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 3.81 0.508 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 163.576 76.708) (end 135.128 76.708) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.576 105.664) (end 163.576 76.708) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.128 105.664) (end 163.576 105.664) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.128 76.708) (end 135.128 105.664) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 3V (at 155.0924 102.3112 90) (layer F.SilkS))
  (gr_text CSN (at 155.0416 99.7458 90) (layer F.SilkS))
  (gr_text MOSI (at 155.067 97.282 90) (layer F.SilkS))
  (gr_text MISO (at 162.3568 94.742 90) (layer F.SilkS))
  (gr_text SCK (at 162.4076 97.4852 90) (layer F.SilkS))
  (gr_text CSN (at 162.4076 99.9744 90) (layer F.SilkS))
  (gr_text GND (at 162.433 102.362 90) (layer F.SilkS))
  (gr_text GND (at 137.2108 100.584) (layer F.SilkS))
  (gr_text 5V (at 142.4178 102.8446 90) (layer F.SilkS))
  (gr_text 3V (at 161.7472 88.9254) (layer F.SilkS))
  (gr_text TX (at 161.8234 78.7908) (layer F.SilkS))
  (gr_text RX (at 161.7726 81.2292) (layer F.SilkS))
  (gr_text IO0 (at 161.7726 83.82) (layer F.SilkS))
  (gr_text GP (at 155.829 83.8708) (layer F.SilkS))
  (gr_text GND (at 162.052 86.4616) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.83 105.41) (xy 134.62 105.41) (xy 134.62 82.55) (xy 154.94 82.55) (xy 154.94 76.9112)
        (xy 163.83 76.9112)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.83 105.41) (xy 134.62 105.41) (xy 134.62 82.55) (xy 154.94 82.55) (xy 154.94 76.9112)
        (xy 163.83 76.9112)
      )
    )
  )
)
