<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="30.48" x2="30.15" y2="30.48" width="0" layer="20"/>
<wire x1="30.15" y1="30.48" x2="30.15" y2="80" width="0" layer="20"/>
<wire x1="30.15" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="30.48" width="0" layer="20"/>
<text>+  D  -</text>
<text>flitelights v0.1</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains footprints for SparkFun breakout boards, microcontrollers (Arduino, Particle, Teensy, etc.),  breadboards, non-RF modules, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_PRO_MINI">
<description>&lt;h3&gt;Arduino Pro Mini Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 34&lt;/li&gt;
&lt;li&gt;Area: 1.7 x 0.3 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Pro Mini&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="-" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND1" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="GND2" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="GND3" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="MCU" library="SparkFun-Boards" package="ARDUINO_PRO_MINI" value="ARDUINO_PRO_MINI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWM1" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PWM2" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PWM3" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="+" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCC1" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="VCC2" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="VCC3" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="MCU" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="MCU" pad="7"/>
<contactref element="MCU" pad="24"/>
<contactref element="PWM1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="MCU" pad="8"/>
<contactref element="PWM2" pad="1"/>
<contactref element="MCU" pad="22"/>
</signal>
<signal name="N$1">
<contactref element="MCU" pad="23"/>
<contactref element="-" pad="1"/>
<contactref element="GND1" pad="1"/>
<contactref element="GND2" pad="1"/>
<contactref element="GND3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="+" pad="1"/>
<contactref element="MCU" pad="21"/>
<contactref element="VCC1" pad="1"/>
<contactref element="VCC2" pad="1"/>
<contactref element="VCC3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="MCU" pad="5"/>
<contactref element="D" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="MCU" pad="9"/>
<contactref element="PWM3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
