(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.598)
  )
  (paper "A")
  (title_block
    (title "i2c Signal Bridge N-Scale")
    (date "2024-01-01")
    (rev "1")
    (company "John Raid")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user "F.Silk.Hidden")
    (51 "User.2" user "B.Silk.Hidden")
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.508) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 112.014 99.06)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3V3")
  (net 2 "GND")
  (net 3 "Net-(D1-A)")
  (net 4 "Net-(D2-A)")
  (net 5 "Net-(D3-A)")
  (net 6 "Net-(J2-Pin_1)")
  (net 7 "Net-(J3-Pin_1)")
  (net 8 "Net-(J4-Pin_1)")
  (net 9 "Net-(J5-Pin_1)")
  (net 10 "Net-(J6-Pin_1)")
  (net 11 "Net-(U1-P00)")
  (net 12 "Net-(U1-P01)")
  (net 13 "Net-(J2-Pin_2)")
  (net 14 "Net-(U1-P02)")
  (net 15 "Net-(J2-Pin_3)")
  (net 16 "Net-(U1-P03)")
  (net 17 "Net-(U1-P04)")
  (net 18 "Net-(J3-Pin_2)")
  (net 19 "Net-(U1-P05)")
  (net 20 "Net-(J3-Pin_3)")
  (net 21 "Net-(U1-P06)")
  (net 22 "Net-(U1-P07)")
  (net 23 "Net-(J4-Pin_2)")
  (net 24 "Net-(U1-P10)")
  (net 25 "Net-(J4-Pin_3)")
  (net 26 "Net-(U1-P11)")
  (net 27 "Net-(U1-P12)")
  (net 28 "Net-(J5-Pin_2)")
  (net 29 "Net-(U1-P13)")
  (net 30 "Net-(J5-Pin_3)")
  (net 31 "Net-(U1-P14)")
  (net 32 "Net-(U1-P15)")
  (net 33 "Net-(J6-Pin_2)")
  (net 34 "Net-(U1-P16)")
  (net 35 "Net-(J6-Pin_3)")
  (net 36 "Net-(U1-P17)")
  (net 37 "Net-(J1-Pin_3)")
  (net 38 "Net-(J1-Pin_2)")
  (net 39 "Net-(J12-Pin_6)")
  (net 40 "Net-(J7-Pin_3)")
  (net 41 "Net-(J12-Pin_5)")
  (net 42 "Net-(J7-Pin_2)")
  (net 43 "unconnected-(U1-~{INT}-Pad22)")
  (net 44 "Net-(U1-A2)")
  (net 45 "Net-(U1-A1)")
  (net 46 "Net-(U1-A0)")
  (net 47 "Net-(U2-IO1)")
  (net 48 "Net-(U2-IO0)")
  (net 49 "Net-(D4-K)")
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 112.141 49.911)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J11" (at 0.762 2.921 90) (layer "User.1"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.119048)
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector:Signal_i2c_4" (layer "F.Cu")
    (at 115.443 96.901)
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J1" (at -1.524 0 unlocked) (layer "User.1"))
    (fp_text value "Conn_01x04_Pin" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect (at 1.016 0 90) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect (at 2.032 0 90) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" thru_hole roundrect (at 3.048 0 90) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Connector:Signal_i2c+2_6" (layer "F.Cu")
    (at 114.427 33.02)
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J12" (at 0.127 1.905 unlocked) (layer "User.1"))
    (fp_text value "Conn_01x06_Pin" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1 0.7) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect (at 1.016 0 90) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect (at 2.032 0 90) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" thru_hole roundrect (at 3.048 0 90) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" thru_hole roundrect (at 4.064 0 90) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J12-Pin_5)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" thru_hole roundrect (at 5.08 0 90) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J12-Pin_6)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 112.141 89.281)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J10" (at 1.016 -3.175 270) (layer "User.1"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.119048)
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector:Signal_3_color" (layer "F.Cu")
    (at 121.031 74.803 -90)
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J4" (at 1.27 1.905 90 unlocked) (layer "User.1"))
    (fp_text value "Conn_01x03_Pin" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J4-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect (at 1.016 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J4-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect (at 2.032 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J4-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Connector:Signal_3_color" (layer "F.Cu")
    (at 121.031 83.693 -90)
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J5" (at 1.524 2.032 90 unlocked) (layer "User.1"))
    (fp_text value "Conn_01x03_Pin" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J5-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect (at 1.016 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J5-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect (at 2.032 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J5-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 121.539 80.264)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J9" (at -2.413 -0.635 90) (layer "User.1"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.119048)
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector:Signal_3_color" (layer "F.Cu")
    (at 112.649 41.402 90)
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J7" (at 4.318 -0.381 270 unlocked) (layer "User.1"))
    (fp_text value "Conn_01x03_Pin" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(D4-K)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect (at 1.016 0 180) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J7-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect (at 2.032 0 180) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J7-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Connector:Signal_3_color" (layer "F.Cu")
    (at 112.649 94.869 90)
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J6" (at -2.159 0.762 270 unlocked) (layer "User.1"))
    (fp_text value "Conn_01x03_Pin" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J6-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect (at 1.016 0 180) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J6-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect (at 2.032 0 180) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(J6-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 119.888 38.34 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D4" (at -0.395 -1.397 90) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 121.539 41.656)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J8" (at -0.635 -2.54 90) (layer "User.1"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.119048)
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector:Signal_3_color" (layer "F.Cu")
    (at 121.031 50.546 -90)
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J3" (at 1.143 2.286 90 unlocked) (layer "User.1"))
    (fp_text value "Conn_01x03_Pin" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J3-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect (at 1.016 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J3-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect (at 2.032 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J3-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Connector:Signal_3_color" (layer "F.Cu")
    (at 121.031 45.974 -90)
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J2" (at 1.27 2.159 90 unlocked) (layer "User.1"))
    (fp_text value "Conn_01x03_Pin" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J2-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect (at 1.016 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J2-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect (at 2.032 0) (size 1 0.75) (drill 0.305) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J2-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.126 46.99)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -2.159 0 90) (layer "B.SilkS"))
    (fp_text value "150" (at 3.9135 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U1-P01)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J2-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.5305 50.038)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at -2.3095 0) (layer "B.SilkS"))
    (fp_text value "150" (at 3.9135 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U1-P03)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J3-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.5305 53.086)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at -2.3095 0) (layer "B.SilkS"))
    (fp_text value "150" (at 3.9135 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(U1-P05)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J3-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.38 74.295)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -0.381 -1.27) (layer "B.SilkS"))
    (fp_text value "150" (at 2.5165 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U1-P06)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J4-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (at 115.57 84.328 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D1" (at -2.286 -1.016 -90) (layer "B.SilkS"))
    (fp_text value "IR" (at -0.254 1.397 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.173 46.736 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D2" (at 2.413 -0.254 90) (layer "B.SilkS"))
    (fp_text value "IR" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:WQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm" (layer "B.Cu")
    (at 117.094 69.449 180)
    (descr "WQFN, 24 Pin (http://www.ti.com/lit/ds/symlink/ts3a27518e.pdf#page=33), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "WQFN NoLead")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ pull-ups, QFN-24")
    (property "ki_keywords" "ti parallel port")
    (attr smd)
    (fp_text reference "U1" (at -3.3345 2.012) (layer "B.SilkS"))
    (fp_text value "TCA9555RTWR" (at -7.5255 -0.02) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "" smd roundrect (at -0.61 -0.61 180) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.61 0.61 180) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.61 -0.61 180) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.61 0.61 180) (size 0.99 0.99) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -1.9375 1.25 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1-P00)") (pinfunction "P00") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -1.9375 0.75 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U1-P01)") (pinfunction "P01") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.9375 0.25 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1-P02)") (pinfunction "P02") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -1.9375 -0.25 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U1-P03)") (pinfunction "P03") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -1.9375 -0.75 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U1-P04)") (pinfunction "P04") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -1.9375 -1.25 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(U1-P05)") (pinfunction "P05") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -1.25 -1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U1-P06)") (pinfunction "P06") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -0.75 -1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U1-P07)") (pinfunction "P07") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -0.25 -1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "10" smd roundrect (at 0.25 -1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1-P10)") (pinfunction "P10") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 0.75 -1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U1-P11)") (pinfunction "P11") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 1.25 -1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U1-P12)") (pinfunction "P12") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.9375 -1.25 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U1-P13)") (pinfunction "P13") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.9375 -0.75 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U1-P14)") (pinfunction "P14") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 1.9375 -0.25 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(U1-P15)") (pinfunction "P15") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 1.9375 0.25 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(U1-P16)") (pinfunction "P16") (pintype "bidirectional"))
    (pad "17" smd roundrect (at 1.9375 0.75 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(U1-P17)") (pinfunction "P17") (pintype "bidirectional"))
    (pad "18" smd roundrect (at 1.9375 1.25 180) (size 0.875 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(U1-A0)") (pinfunction "A0") (pintype "input"))
    (pad "19" smd roundrect (at 1.25 1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J1-Pin_3)") (pinfunction "SCL") (pintype "input"))
    (pad "20" smd roundrect (at 0.75 1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J1-Pin_2)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 0.25 1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "22" smd roundrect (at -0.25 1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "unconnected-(U1-~{INT}-Pad22)") (pinfunction "~{INT}") (pintype "open_collector"))
    (pad "23" smd roundrect (at -0.75 1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(U1-A1)") (pinfunction "A1") (pintype "input"))
    (pad "24" smd roundrect (at -1.25 1.9375 180) (size 0.3 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(U1-A2)") (pinfunction "A2") (pintype "input"))
    (pad "25" smd rect (at 0 0 180) (size 2.45 2.45) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "EPAD") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/WQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.046 95.377 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 0.635 -1.27) (layer "B.SilkS"))
    (fp_text value "150" (at 2.1355 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U1-P14)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J6-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.2765 38.862 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 0.7385 1.27) (layer "B.SilkS"))
    (fp_text value "150" (at 2.5165 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(U2-IO0)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J7-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 117.8325 60.325 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at -2.6905 0) (layer "B.SilkS"))
    (fp_text value "10k" (at -5.6115 0.127) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(U1-A0)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 117.8325 58.801 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at -2.6905 0) (layer "B.SilkS"))
    (fp_text value "10k" (at -5.4845 0.127) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(U1-A1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 116.3085 63.373 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at -2.8175 0) (layer "B.SilkS"))
    (fp_text value "10k" (at 2.3895 -0.127) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J1-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.4035 83.185)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0.1035 -1.27) (layer "B.SilkS"))
    (fp_text value "150" (at 3.5795 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U1-P11)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J5-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 116.3085 61.849 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at -2.8175 -0.127) (layer "B.SilkS"))
    (fp_text value "10k" (at 2.3895 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J1-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.4035 86.233)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at -0.0235 1.397) (layer "B.SilkS"))
    (fp_text value "150" (at 3.5795 0.127) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U1-P13)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J5-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.5305 45.466)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.3095 0) (layer "B.SilkS"))
    (fp_text value "150" (at 3.9135 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1-P00)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J2-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.126 84.709)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -2.1825 0 90) (layer "B.SilkS"))
    (fp_text value "150" (at 3.5795 0.127) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U1-P12)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J5-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.046 92.329 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at -1.143 1.27) (layer "B.SilkS"))
    (fp_text value "150" (at 2.2625 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(U1-P16)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(J6-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.126 75.819)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at -1.905 0 90) (layer "B.SilkS"))
    (fp_text value "150" (at 2.667 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U1-P07)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J4-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-8_3x3mm_P0.65mm" (layer "B.Cu")
    (at 119.167 37.093 -90)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "4-bit I2C-bus and SMBus IO port, TSSOP-8")
    (property "ki_keywords" "i2c io port")
    (attr smd)
    (fp_text reference "U2" (at -0.39 2.454 180) (layer "B.SilkS"))
    (fp_text value "PCA9536DP" (at -0.263 -7.198 -180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -2.15 0.975 270) (size 1.1 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "Net-(U2-IO0)") (pinfunction "IO0") (pintype "bidirectional"))
    (pad "2" smd rect (at -2.15 0.325 270) (size 1.1 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "Net-(U2-IO1)") (pinfunction "IO1") (pintype "bidirectional"))
    (pad "3" smd rect (at -2.15 -0.325 270) (size 1.1 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "Net-(J12-Pin_5)") (pinfunction "IO2") (pintype "bidirectional"))
    (pad "4" smd rect (at -2.15 -0.975 270) (size 1.1 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "5" smd rect (at 2.15 -0.975 270) (size 1.1 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "Net-(J12-Pin_6)") (pinfunction "IO3") (pintype "bidirectional"))
    (pad "6" smd rect (at 2.15 -0.325 270) (size 1.1 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "Net-(J1-Pin_3)") (pinfunction "SCL") (pintype "input"))
    (pad "7" smd rect (at 2.15 0.325 270) (size 1.1 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "Net-(J1-Pin_2)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "8" smd rect (at 2.15 0.975 270) (size 1.1 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.2765 41.91 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at -0.4045 -1.27) (layer "B.SilkS"))
    (fp_text value "150" (at 2.5165 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(U1-P17)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(D4-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.38 77.343)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at -0.508 1.27) (layer "B.SilkS"))
    (fp_text value "150" (at 2.667 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1-P10)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J4-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 116.205 87.884 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at -0.1035 -1.27 90) (layer "B.SilkS"))
    (fp_text value "150" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 117.856 64.897)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 2.413 0 180) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.43 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 118.364 94.742 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at -0.0235 1.143 90) (layer "B.SilkS"))
    (fp_text value "150" (at -1.5005 -1.143 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D3-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.681 40.386 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at -2.6905 0) (layer "B.SilkS"))
    (fp_text value "150" (at 2.5165 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(U2-IO1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J7-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 115.697 46.736 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at -2.794 0 90) (layer "B.SilkS"))
    (fp_text value "150" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.126 51.562)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -2.3095 0) (layer "B.SilkS"))
    (fp_text value "150" (at 3.9135 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U1-P04)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J3-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.554 93.853 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at -2.667 1.143) (layer "B.SilkS"))
    (fp_text value "150" (at 2.1355 -0.127) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(U1-P15)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J6-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.3235 57.277 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 1.016 3.302) (layer "B.SilkS"))
    (fp_text value "0" (at 2.921 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(U1-A2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.5305 48.514)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -2.3095 0) (layer "B.SilkS"))
    (fp_text value "150" (at 3.9135 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1-P02)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J2-Pin_3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (at 117.207 98.2218 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol, filled shape")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D3" (at 2.427 0.127) (layer "B.SilkS"))
    (fp_text value "IR" (at -0.24 -1.651) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.3235 60.325 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at 1.0395 4.318) (layer "B.SilkS"))
    (fp_text value "0" (at 3.0715 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(U1-A0)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.3235 58.801 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at 1.0395 3.81) (layer "B.SilkS"))
    (fp_text value "0" (at 2.9445 0.127) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(U1-A1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 117.8325 57.277 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at -2.6905 0) (layer "B.SilkS"))
    (fp_text value "10k" (at -5.6115 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(U1-A2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 118.4675 42.037 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Signal Bridge.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at -0.2775 -1.27) (layer "B.SilkS"))
    (fp_text value "150" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J12-Pin_6)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(D4-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_poly
    (pts
      (xy 121.666 32.385)
      (xy 121.666 40.005)
      (xy 122.809 40.64)
      (xy 122.809 42.545)
      (xy 121.666 43.18)
      (xy 121.666 78.74)
      (xy 122.809 79.375)
      (xy 122.809 81.28)
      (xy 121.666 81.915)
      (xy 121.666 99.06)
      (xy 112.014 99.06)
      (xy 112.014 90.805)
      (xy 110.871 90.17)
      (xy 110.871 88.265)
      (xy 112.014 87.63)
      (xy 112.014 51.435)
      (xy 110.871 50.8)
      (xy 110.871 48.895)
      (xy 112.014 48.26)
      (xy 112.014 32.385)
    )
    (fill none) (layer "Edge.Cuts"))
  (gr_text "631-1024-001" (at 121.539 89.662 90) (layer "B.Cu"))
  (gr_text "3V3" (at 112.9284 35.941 -90) (layer "B.SilkS"))
  (gr_text "ASSY" (at 119.253 89.789 90) (layer "B.SilkS"))
  (gr_text "651-1024-001" (at 120.269 89.662 90) (layer "B.SilkS"))
  (gr_text "SDA" (at 114.1984 35.941 -90) (layer "B.SilkS"))
  (gr_text "SN" (at 115.189 81.407 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 116.5098 36.068 -90) (layer "B.SilkS"))
  (gr_text "J RAID" (at 121.031 56.134) (layer "B.SilkS"))
  (gr_text "©2024" (at 121.158 54.991) (layer "B.SilkS"))
  (gr_text "OTTUMWA SUB" (at 112.4712 81.6864 270) (layer "B.SilkS"))
  (gr_text "SCL" (at 115.4684 35.941 -90) (layer "B.SilkS"))
  (gr_text "SCL" (at 117.10404 93.98 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 118.237 93.853 -90) (layer "F.SilkS"))
  (gr_text "SDA" (at 115.83404 93.98 -90) (layer "F.SilkS"))
  (gr_text "3V3" (at 114.56404 93.98 -90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 121.666 99.06) (xy 112.014 99.06))
    (height -3.175)
    (gr_text "0.380 in" (at 116.84 101.323) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 121.539 80.264) (xy 121.539 41.656))
    (height 5.08)
    (gr_text "1.520 in" (at 125.707 60.96 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 121.666 99.06) (xy 121.666 80.264))
    (height 4.699)
    (gr_text "0.740 in" (at 125.453 89.662 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 112.014 99.06) (xy 112.014 89.281))
    (height -3.048)
    (gr_text "0.385 in" (at 108.054 94.1705 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 121.666 99.06) (xy 121.666 32.385))
    (height 8.001)
    (gr_text "2.625 in" (at 128.755 65.7225 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 112.141 89.281) (xy 112.141 49.911))
    (height -3.429)
    (gr_text "1.550 in" (at 107.8 69.596 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 122.809 40.64) (xy 110.871 40.64))
    (height 12.445999)
    (gr_text "0.470 in" (at 116.84 27.282001) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 121.666 99.06)
        (xy 112.014 99.06)
        (xy 112.014 32.385)
        (xy 121.666 32.385)
      )
    )
  )
)
