(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 62)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 4)
    (tracks 171)
    (zones 0)
    (modules 23)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(uC1-Pad14)")
  (net 2 "Net-(uC1-Pad15)")
  (net 3 "Net-(uC1-Pad22)")
  (net 4 "Net-(uC1-Pad24)")
  (net 5 VCC)
  (net 6 A3)
  (net 7 GND)
  (net 8 A2)
  (net 9 A1)
  (net 10 A0)
  (net 11 SCL)
  (net 12 SDA)
  (net 13 D5)
  (net 14 D6)
  (net 15 D9)
  (net 16 D10)
  (net 17 D4)
  (net 18 D7)
  (net 19 D8)
  (net 20 D15)
  (net 21 RX)
  (net 22 TX)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net D10)
    (add_net D15)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net D9)
    (add_net GND)
    (add_net "Net-(uC1-Pad14)")
    (add_net "Net-(uC1-Pad15)")
    (add_net "Net-(uC1-Pad22)")
    (add_net "Net-(uC1-Pad24)")
    (add_net RX)
    (add_net SCL)
    (add_net SDA)
    (add_net TX)
    (add_net VCC)
  )
  (module Housings_DIP:DIP-24_W15.24mm_Socket (layer B.Cu) (tedit 5A6CB1ED)
    (at 229.235 107.315 180)
    (descr "24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
    (fp_text reference uC1 (at 13.335 0 450) (layer B.SilkS))
    (fp_text value PROMICRO (at 7.62 -30.27 180) (layer B.Fab))
    (fp_text user %R (at 7.62 -13.97 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 TX))
    (pad 13 thru_hole oval (at 15.24 -27.94 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 D10))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 RX))
    (pad 14 thru_hole oval (at 15.24 -25.4 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(uC1-Pad14)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 15 thru_hole oval (at 15.24 -22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(uC1-Pad15)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 16 thru_hole oval (at 15.24 -20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 D15))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 SDA))
    (pad 17 thru_hole oval (at 15.24 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 A0))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 SCL))
    (pad 18 thru_hole oval (at 15.24 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 A1))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 D4))
    (pad 19 thru_hole oval (at 15.24 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 A2))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 D5))
    (pad 20 thru_hole oval (at 15.24 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 A3))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 D6))
    (pad 21 thru_hole oval (at 15.24 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 D7))
    (pad 22 thru_hole oval (at 15.24 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(uC1-Pad22)"))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 D8))
    (pad 23 thru_hole oval (at 15.24 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 D9))
    (pad 24 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(uC1-Pad24)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-24_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 217.805 139.7 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J17 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBB92)
    (at 205.74 133.35 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference A0 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 A0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBB94)
    (at 205.74 125.095 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference A1 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 A1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBBB5)
    (at 205.74 116.84 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference A2 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 A2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBBB6)
    (at 205.74 108.458 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference A3 (at -4.572 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 A3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBBA7)
    (at 232.41 116.84 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference D5 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 D5))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBB9F)
    (at 232.41 125.095 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference D6 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 D6))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBB9A)
    (at 219.075 133.35 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference D9 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 D9))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBBA2)
    (at 219.075 125.095 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference D10 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 D10))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBBA9)
    (at 232.41 108.585 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference D4 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 D4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBB9D)
    (at 232.41 133.35 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference D7 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 D7))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBBAE)
    (at 219.075 116.84 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference D8 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 D8))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors:Fan_Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A6CBBB1)
    (at 219.075 108.585 90)
    (descr "3-pin CPU fan Through hole pin header")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference D15 (at -4.445 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 D15))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Connectors.3dshapes\Fan_Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 236.855 131.445 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 18 D7))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 210.185 123.19 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 A1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 223.52 114.935 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 19 D8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 210.185 114.935 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 A2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 210.185 106.68 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 A3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 236.855 106.68 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 17 D4))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 210.185 131.445 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 A0))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 223.52 106.68 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 1.25 180) (layer B.SilkS))
    (fp_text value C_Small (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 20 D15))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 229.87 139.7 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J16 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 RX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 TX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 204.47 140.97) (end 238.76 140.97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.47 106.045) (end 204.47 140.97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 238.76 106.045) (end 204.47 106.045) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 238.76 140.97) (end 238.76 106.045) (angle 90) (layer Edge.Cuts) (width 0.15))
)
