(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 64)
    (zones 0)
    (modules 3)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.5 4.5)
    (pad_drill 3.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /+12)
  (net 2 /GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+12)
    (add_net /GND)
  )
  (module pads:PS2_FAT_CON (layer F.Cu) (tedit 5C2FFF2E)
    (at 77.5 73)
    (fp_text reference J1 (at 8 -15) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 16 -15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 /+12))
    (pad 2 thru_hole circle (at 5.08 0) (size 2.5 2.5) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 /+12))
    (pad 3 thru_hole circle (at 10.16 0) (size 2.5 2.5) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 4 thru_hole circle (at 15.24 0) (size 2.5 2.5) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 /GND))
  )
  (module pads:PS2_FAT_PWR (layer F.Cu) (tedit 5C300568)
    (at 90.25 80)
    (fp_text reference J2 (at -7.5 -5) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 -5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 5) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 0 8) (size 5 5) (layers B.Cu B.Paste B.Mask)
      (net 1 /+12))
  )
  (module pads:Via_Large (layer F.Cu) (tedit 5C30148D)
    (at 65.5 66)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value "Via Large" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.5 -0.5) (size 4.5 4.5) (drill 3.8) (layers *.Cu))
  )
  (gr_line (start 55 92.5) (end 55 60) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 63 61) (end 63 60) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 63 61) (end 66 61) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 99.5 90) (end 99.5 86) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.5 90) (end 99.5 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.5 86) (end 105.5 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.5 86) (end 105.5 86) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.5 82) (end 99.5 78) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.5 82) (end 99.5 82) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.5 78) (end 105.5 82) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.5 78) (end 105.5 78) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66 60) (end 108.5 60) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 66 61) (end 66 60) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 108.5 92.5) (end 55 92.5) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 108.5 60) (end 108.5 92.5) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 55 60) (end 63 60) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 86 71) (xy 94.5 71) (xy 94.5 83.5) (xy 86 83.5)
      )
    )
  )
  (zone (net 1) (net_name /+12) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 84.5 71) (xy 84.5 84.5) (xy 94.5 84.5) (xy 94.5 91.5) (xy 83.5 91.5)
        (xy 75.5 91.5) (xy 75.5 81.25) (xy 75.5 71)
      )
    )
  )
  (zone (net 2) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 86 71) (xy 94.5 71) (xy 94.5 83.5) (xy 86 83.5)
      )
    )
  )
  (zone (net 1) (net_name /+12) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 84.5 71) (xy 84.5 84.5) (xy 94.5 84.5) (xy 94.5 91.5) (xy 83.5 91.5)
        (xy 75.5 91.5) (xy 75.5 81.25) (xy 75.5 71)
      )
    )
  )
)
