<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<text>GAMEBUINO</text>
<text>BY DUNCAN YOUNG</text>
<text>BY DUNCAN YOUNG</text>
<text>- BATTERY+</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="USB-MINIB">
<description>Surface Mount USB Mini-B Connector</description>
</package>
<package name="AVRISP-BOX">
</package>
<package name="PUSHBUTTON_SMD_SJ">
</package>
<package name="PS603">
</package>
</packages>
</library>
<library name="ftdichip">
<description>&lt;b&gt;FTDI (TM) CHIP&lt;/b&gt; Future Technology Devices International Ltd.&lt;p&gt;
http://www.ftdichip.com</description>
<packages>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt; SSOP-28&lt;p&gt;
http://www.ftdichip.com/Documents/DataSheets/DS_FT232R_v104.pdf</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="5110-lcd">
<description>&lt;b&gt;LPH-7366: PCD8544-based Nokia 5110 monochrome LCD display&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="LPH-7366">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="QS">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="255SB">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
distributor Buerklin, 11G810</description>
</package>
</packages>
</library>
<library name="speaker">
<packages>
<package name="SMS-1308MS-2-R">
<description>&lt;b&gt;Speaker 13 x 13mm&lt;/b&gt;, 8 Ohm, 0.7W&lt;p&gt;
Source: pui audio inc. SMS-1308MS-2-R.pdf</description>
</package>
</packages>
</library>
<library name="thecustomgeek">
<description>A humble collection of custom parts.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="2.2uF">
<attribute name="MPN" value=""/>
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value=""/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value=""/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="0.1u">
<attribute name="MPN" value=""/>
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="CN1" library="adafruit" package="USB-MINIB" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="IC1" library="ftdichip" package="SSOP28" value="FT232RL">
<attribute name="MPN" value="FT232RL"/>
<attribute name="OC_FARNELL" value="1146032"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="91K9918"/>
</element>
<element name="ISP1" library="adafruit" package="AVRISP-BOX" value="AVRISP-BOX">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="JP1" library="pinhead" package="1X06/90" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="LCD1" library="5110-lcd" package="LPH-7366" value="LPH-7366">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="LED1" library="led" package="SML0805" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="LED2" library="led" package="SML0805" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="LED3" library="led" package="SML0805" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="LED4" library="led" package="SML0805" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="Q2" library="special" package="QS" value="16mhz">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="S1" library="switch" package="255SB" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="S2" library="switch" package="255SB" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SP1" library="speaker" package="SMS-1308MS-2-R" value="SMS-1308MS-2-R">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SW1" library="adafruit" package="PUSHBUTTON_SMD_SJ" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SW2" library="adafruit" package="PUSHBUTTON_SMD_SJ" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SW3" library="adafruit" package="PUSHBUTTON_SMD_SJ" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SW4" library="adafruit" package="PUSHBUTTON_SMD_SJ" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SW5" library="adafruit" package="PUSHBUTTON_SMD_SJ" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SW6" library="adafruit" package="PUSHBUTTON_SMD_SJ" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SW7" library="adafruit" package="PUSHBUTTON_SMD_SJ" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="U$1" library="adafruit" package="PS603" value="PS603SPK">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="U1" library="thecustomgeek" package="TQFP32-08" value="ATMEGA328">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LCD1" pad="7"/>
<contactref element="C1" pad="1"/>
<contactref element="CN1" pad="GND"/>
<contactref element="ISP1" pad="6"/>
<contactref element="SW1" pad="P$2"/>
<contactref element="SW7" pad="P$2"/>
<contactref element="SW6" pad="P$2"/>
<contactref element="SW5" pad="P$2"/>
<contactref element="SW4" pad="P$2"/>
<contactref element="SW3" pad="P$2"/>
<contactref element="SW2" pad="P$2"/>
<contactref element="U$1" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="IC1" pad="26"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="N$2">
<contactref element="CN1" pad="D+"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$3">
<contactref element="CN1" pad="D-"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="30"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="CN1" pad="VBUS"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="20"/>
<contactref element="LCD1" pad="1"/>
<contactref element="LCD1" pad="6"/>
<contactref element="SP1" pad="+"/>
<contactref element="ISP1" pad="2"/>
<contactref element="JP1" pad="5"/>
<contactref element="S1" pad="2"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="JP1" pad="4"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="BUTTON/C">
<contactref element="U1" pad="26"/>
<contactref element="SW1" pad="P$1"/>
</signal>
<signal name="SCREENRESET">
<contactref element="U1" pad="23"/>
<contactref element="LCD1" pad="9"/>
</signal>
<signal name="BUTTON/0">
<contactref element="SW4" pad="P$1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="BUTTON/1">
<contactref element="SW5" pad="P$1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="BUTTON/2">
<contactref element="U1" pad="10"/>
</signal>
<signal name="BUTTON/3">
<contactref element="SW7" pad="P$1"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="CHIPSCREEN">
<contactref element="U1" pad="24"/>
<contactref element="LCD1" pad="5"/>
</signal>
<signal name="SCREENDC">
<contactref element="LCD1" pad="4"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="N$37">
<contactref element="LCD1" pad="8"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="U1" pad="8"/>
<contactref element="Q2" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="Q2" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="ISP1" pad="5"/>
<contactref element="U1" pad="29"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="BUTTON/B">
<contactref element="U1" pad="32"/>
<contactref element="SW2" pad="P$1"/>
</signal>
<signal name="BUTTON/A">
<contactref element="U1" pad="2"/>
<contactref element="SW3" pad="P$1"/>
</signal>
<signal name="BACKLIGHT">
<contactref element="LED1" pad="A"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="SOUND">
<contactref element="U1" pad="1"/>
<contactref element="SP1" pad="-"/>
</signal>
<signal name="MOSI">
<contactref element="LCD1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="SCK">
<contactref element="LCD1" pad="3"/>
<contactref element="U1" pad="17"/>
<contactref element="ISP1" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="31"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="CHIPSD">
<contactref element="U1" pad="14"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="2"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="ISP1" pad="1"/>
<contactref element="S2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
