Altium Designer Pick and Place Locations
Y:\I\IT1335\Engineering\Altium Files\Project Outputs for IT1335\Pick Place\Pick Place for IT1335-900X2.txt

========================================================================================================================
File Design Information:

Date:       18/11/21
Time:       16:55
Revision:   Not in VersionControl
Variant:    No variations
Units used: mil

Designator Comment          Layer       Footprint      Center-X(mil) Center-Y(mil) Rotation Description                                           
C2         C0805C105K5RACTU BottomLayer C0805          -1045.000     2712.500      270      "Capacitor (Semiconductor SIM Model)"                 
C1         C0805C105K5RACTU BottomLayer C0805          140.000       2712.500      270      "Capacitor (Semiconductor SIM Model)"                 
F1         33V/750mA        BottomLayer 1812           -480.000      2596.654      180      "PTC RESET FUSE 33V 750MA 1812"                       
J7         PC-1727566       TopLayer    1727566        -1448.898     2817.716      0        "Header, EURO TERM BLOCK, 2-Pin, Female, Right-Angle" 
R15        200              BottomLayer 6-0805_N       1360.472      885.000       90       Resistor                                              
R14        200              BottomLayer 6-0805_N       1161.890      885.000       90       Resistor                                              
D2         8V/50uA          BottomLayer SMC            1360.472      1335.000      90       "Diode, TVS, Bi-directional, ESD"                     
D1         8V/50uA          BottomLayer SMC            1161.890      1335.000      90       "Diode, TVS, Bi-directional, ESD"                     
R5         15               TopLayer    AXIAL-0.3      1635.000      2365.000      90       Resistor                                              
R6         10K              TopLayer    AXIAL-0.3      385.000       2265.000      360      Resistor                                              
R11        4.7K             TopLayer    AXIAL-0.3      -15.000       2265.000      360      Resistor                                              
R13        15               TopLayer    AXIAL-0.3      -1000.000     1475.000      270      Resistor                                              
R12        15               TopLayer    AXIAL-0.3      515.000       2395.000      360      Resistor                                              
R10        10K              TopLayer    AXIAL-0.3      763.000       1535.000      270      Resistor                                              
R9         10K              TopLayer    AXIAL-0.3      1270.000      2365.000      90       Resistor                                              
R8         10K              TopLayer    AXIAL-0.3      970.000       1535.000      270      Resistor                                              
R7         10K              TopLayer    AXIAL-0.3      1450.000      2365.000      90       Resistor                                              
R4         6.8K             TopLayer    AXIAL-0.3      -1300.000     1475.000      270      Resistor                                              
R3         6.8K             TopLayer    AXIAL-0.3      -1195.000     1055.000      315      Resistor                                              
R2         6.8K             TopLayer    AXIAL-0.3      -1600.000     1475.000      270      Resistor                                              
R1         6.8K             TopLayer    AXIAL-0.3      -1495.000     1055.000      315      Resistor                                              
J3         "2.5x5.5 Barrel" TopLayer    BARREL-25_55F  355.512       2710.827      360      "CONN PWR JACK 2.5X5.5MM SOLDER"                      
J5         "Header 7X2"     BottomLayer HDR2X7         -1400.000     1980.000      180      "Header, 7-Pin, Dual row"                             
J4         "Header 7X2"     BottomLayer HDR2X7         1310.000      1980.000      180      "Header, 7-Pin, Dual row"                             
J6         "Header 7X2"     BottomLayer HDR2X7         -1400.000     2340.000      180      "Header, 7-Pin, Dual row"                             
J1         DB-37M-RA        BottomLayer DSUB1.385-2H37 0.000         377.937       360      "Receptacle Assembly, 37 Position, Right Angle"       
J2         DB9-USB-F        TopLayer    DSUB1.385-2H9  1415.000      2737.984      360      "USB to RS-232 Adapter, DB-9F Replacement"            
