(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 24)
    (no_connects 1)
    (area 148.260999 70.028999 186.511001 105.231001)
    (thickness 1.6)
    (drawings 5)
    (tracks 74)
    (zones 0)
    (modules 11)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu jumper)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad6)")
  (net 2 VCC)
  (net 3 "Net-(IC1-Pad5)")
  (net 4 "Net-(IC1-Pad1)")
  (net 5 GND)
  (net 6 "Net-(IC1-Pad2)")
  (net 7 "Net-(U1-Pad2)")
  (net 8 "Net-(U2-Pad2)")
  (net 9 "Net-(IC1-Pad3)")
  (net 10 "Net-(IC1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U2-Pad2)")
    (add_net VCC)
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 179.07 94.234 270)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at 0 -3.68 270) (layer F.SilkS))
    (fp_text value ATTINY85-S (at 0 3.68 270) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -3.65 -0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -3.65 0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -3.65 1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 5 smd rect (at 3.65 1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at 3.65 0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at 3.65 -0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at 3.65 -1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 57F08351)
    (at 170.688 93.472 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 1.016 -2.54 180) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(IC1-Pad6)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC1-Pad7)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(IC1-Pad5)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(IC1-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ExplodingLemur:photocell (layer F.Cu) (tedit 57F08396)
    (at 160.02 83.82)
    (fp_text reference R1 (at 0 2.794) (layer F.SilkS))
    (fp_text value Photores (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57F08378)
    (at 164.846 86.36 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.524 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 57BABF74)
    (at 160.782 94.488 180)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 -2 180) (layer F.SilkS))
    (fp_text value SW_PUSH_SMALL_H (at 3.75 6.7 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(IC1-Pad7)"))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(IC1-Pad7)"))
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 56C9C7F7)
    (at 179.07 82.804 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U1 (at 0 -3.5 180) (layer F.SilkS))
    (fp_text value WS2812B (at 0 4 180) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 4 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad3)"))
    (pad 2 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 56C9C7F7)
    (at 179.07 75.438 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U2 (at 0 -3.5 180) (layer F.SilkS))
    (fp_text value WS2812B (at 0 4 180) (layer F.Fab))
    (pad 3 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 4 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad2)"))
    (pad 2 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U2-Pad2)"))
    (pad 1 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57F0835C)
    (at 172.466 81.534)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference W1 (at 0 2.54) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57F0835F)
    (at 167.386 81.534)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference W2 (at 0 2.54) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(IC1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ExplodingLemur:LOGO (layer B.Cu) (tedit 0)
    (at 182.88 73.406 180)
    (fp_text reference G*** (at 0 -2.1209 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 2.1209 180) (layer B.SilkS) hide)
  )
  (module ExplodingLemur:Battery_Holder_AAA (layer B.Cu) (tedit 57F089DF)
    (at 148.844 104.648)
    (fp_text reference BT1 (at 27.94 -1.27) (layer B.SilkS))
    (fp_text value Battery (at 0 0.5) (layer B.Fab))
    (pad 2 thru_hole circle (at 18.27 -2.64) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 30.17 -2.64) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 VCC))
  )
  (gr_text "JAR OF FIREFLIES TEST\nCC-BY-SA\ngithub.com/explodinglemur" (at 166.624 74.93) (layer B.SilkS))
  (gr_line (start 148.336 105.156) (end 148.336 70.104) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.436 70.104) (end 186.436 105.156) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.436 70.104) (end 148.336 70.104) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.436 105.156) (end 148.336 105.156) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.928 70.358) (xy 148.844 70.358) (xy 148.844 104.648) (xy 185.928 104.648)
      )
    )
  )
)
