(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 0.8)
    (drawings 15)
    (tracks 689)
    (zones 0)
    (modules 17)
    (nets 70)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 2.1)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "MicroGerbers/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /XIN)
  (net 3 /A7)
  (net 4 /A6)
  (net 5 /A5)
  (net 6 /RESET)
  (net 7 "Net-(LED1-Pad1)")
  (net 8 /A9)
  (net 9 /WR)
  (net 10 /RD)
  (net 11 /CS)
  (net 12 /A0)
  (net 13 /A1)
  (net 14 /A2)
  (net 15 /A3)
  (net 16 /A4)
  (net 17 /A8)
  (net 18 /A10)
  (net 19 /A11)
  (net 20 /A12)
  (net 21 /A13)
  (net 22 /A14)
  (net 23 /A15)
  (net 24 /D0)
  (net 25 /D1)
  (net 26 /D2)
  (net 27 /D3)
  (net 28 /D4)
  (net 29 /D5)
  (net 30 /D6)
  (net 31 /D7)
  (net 32 /RST)
  (net 33 /RWLED)
  (net 34 GND)
  (net 35 /SNDAIN)
  (net 36 "Net-(C3-Pad2)")
  (net 37 FLASH)
  (net 38 "Net-(J1-PadA4|B9)")
  (net 39 "Net-(J1-PadB8)")
  (net 40 "Net-(J1-PadA5)")
  (net 41 D-)
  (net 42 D+)
  (net 43 "Net-(J1-PadA8)")
  (net 44 "Net-(J1-PadB5)")
  (net 45 "Net-(LED2-Pad2)")
  (net 46 "Net-(R4-Pad1)")
  (net 47 "Net-(U1-Pad5)")
  (net 48 "Net-(U1-Pad6)")
  (net 49 "Net-(U1-Pad7)")
  (net 50 "Net-(U1-Pad14)")
  (net 51 "Net-(U1-Pad17)")
  (net 52 "Net-(U1-Pad26)")
  (net 53 "Net-(U1-Pad27)")
  (net 54 "Net-(U1-Pad28)")
  (net 55 "Net-(U1-Pad29)")
  (net 56 "Net-(U1-Pad39)")
  (net 57 "Net-(U2-Pad2)")
  (net 58 "Net-(U2-Pad3)")
  (net 59 "Net-(U2-Pad6)")
  (net 60 "Net-(U2-Pad9)")
  (net 61 "Net-(U2-Pad10)")
  (net 62 "Net-(U2-Pad11)")
  (net 63 "Net-(U2-Pad12)")
  (net 64 "Net-(U2-Pad13)")
  (net 65 "Net-(U2-Pad14)")
  (net 66 "Net-(U2-Pad22)")
  (net 67 "Net-(U2-Pad23)")
  (net 68 "Net-(U2-Pad28)")
  (net 69 "Net-(X1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CS)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /RD)
    (add_net /RESET)
    (add_net /RST)
    (add_net /RWLED)
    (add_net /SNDAIN)
    (add_net /WR)
    (add_net /XIN)
    (add_net D+)
    (add_net D-)
    (add_net FLASH)
    (add_net GND)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(J1-PadA4|B9)")
    (add_net "Net-(J1-PadA5)")
    (add_net "Net-(J1-PadA8)")
    (add_net "Net-(J1-PadB5)")
    (add_net "Net-(J1-PadB8)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(X1-Pad1)")
  )
  (module Custom:DSL_Cartridge_Reader_Nano (layer F.Cu) (tedit 5DE96C8B)
    (at 133.188 65.3009)
    (fp_text reference J0 (at 0 1.7272 180) (layer F.SilkS))
    (fp_text value CartBus (at 0 -11) (layer F.Fab))
    (fp_text user %R (at 0 -1) (layer F.Fab))
    (fp_text user CartBus (at 0 -11) (layer F.Fab))
    (pad GND smd rect (at -12.68204 -12.82) (size 4.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -23.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 17 smd rect (at 0.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /A11))
    (pad 20 smd rect (at 5.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 /A14))
    (pad "" np_thru_hole circle (at 12.93204 -2.04724) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 15 smd rect (at -2.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /A9))
    (pad 13 smd rect (at -5.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /A7))
    (pad 32 smd rect (at 23.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 26 smd rect (at 14.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 /D4))
    (pad 23 smd rect (at 9.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /D1))
    (pad 8 smd rect (at -12.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /A2))
    (pad 27 smd rect (at 15.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /D5))
    (pad 28 smd rect (at 17.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /D6))
    (pad 25 smd rect (at 12.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /D3))
    (pad 30 smd rect (at 20.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 32 /RST))
    (pad 2 smd rect (at -21.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 37 FLASH))
    (pad 7 smd rect (at -14.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /A1))
    (pad 10 smd rect (at -9.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /A4))
    (pad 11 smd rect (at -8.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /A5))
    (pad 12 smd rect (at -6.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /A6))
    (pad 18 smd rect (at 2.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /A12))
    (pad 22 smd rect (at 8.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 24 /D0))
    (pad 31 smd rect (at 21.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /SNDAIN))
    (pad GND smd rect (at 12.68204 -12.82) (size 4.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 3 smd rect (at -20.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /WR))
    (pad 5 smd rect (at -17.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /CS))
    (pad "" np_thru_hole circle (at -12.93204 -2.04724) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 14 smd rect (at -3.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /A8))
    (pad 6 smd rect (at -15.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /A0))
    (pad 24 smd rect (at 11.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /D2))
    (pad 4 smd rect (at -18.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /RD))
    (pad 16 smd rect (at -0.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /A10))
    (pad 21 smd rect (at 6.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 23 /A15))
    (pad 9 smd rect (at -11.25 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 15 /A3))
    (pad 29 smd rect (at 18.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 31 /D7))
    (pad 19 smd rect (at 3.75 5) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /A13))
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 155.0289 54.1274 90)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference X1 (at -2.794 -0.00254 180) (layer B.SilkS))
    (fp_text value 6MHz (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 4 smd rect (at -1.1 0.85 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 1.1 0.85 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 /XIN))
    (pad 2 smd rect (at 1.1 -0.85 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.1 -0.85 90) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(X1-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 118.311 52.6517)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.28346 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 118.311 54.2696)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -2.28346 0) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 131.034 70.0557)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.1684) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5A3EABFC)
    (at 112.078 68.2704)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference Flash1 (at 0 1.8) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9) (layer B.Fab))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 6 /RESET))
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 37 FLASH))
  )
  (module LED_SMD:LED_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 135.995 52.4993 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED1 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(LED1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 130.843 52.4993 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED2 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(LED2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 /RWLED))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 110.912 54.0004 270)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference F1 (at -0.00254 -1.54432 90) (layer B.SilkS))
    (fp_text value 500mA (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(J1-PadA4|B9)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 135.997 54.2163)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(LED1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.846 54.2163)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(LED2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.098 66.3778 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.16586 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /RESET))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 119.07 69.7306 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.33426 0) (layer B.SilkS))
    (fp_text value 5.1K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(J1-PadA5)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 119.07 68.039 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.33426 0) (layer B.SilkS))
    (fp_text value 5.1K (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(R4-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(J1-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-44_10x10mm_P0.8mm (layer B.Cu) (tedit 5A02F146)
    (at 145.837 61.3232 90)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 0 180) (layer B.SilkS))
    (fp_text value ATmega8515L-8AU (at 0 -7.45 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -5.7 4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /A5))
    (pad 2 smd rect (at -5.7 3.2 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 /A6))
    (pad 3 smd rect (at -5.7 2.4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 3 /A7))
    (pad 4 smd rect (at -5.7 1.6 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /RESET))
    (pad 5 smd rect (at -5.7 0.8 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -5.7 0 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -5.7 -0.8 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -5.7 -1.6 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 33 /RWLED))
    (pad 9 smd rect (at -5.7 -2.4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 9 /WR))
    (pad 10 smd rect (at -5.7 -3.2 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 /RD))
    (pad 11 smd rect (at -5.7 -4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 11 /CS))
    (pad 12 smd rect (at -4 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 32 /RST))
    (pad 13 smd rect (at -3.2 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 /SNDAIN))
    (pad 14 smd rect (at -2.4 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at -1.6 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 /XIN))
    (pad 16 smd rect (at -0.8 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 17 smd rect (at 0 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 0.8 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 24 /D0))
    (pad 19 smd rect (at 1.6 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 25 /D1))
    (pad 20 smd rect (at 2.4 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 26 /D2))
    (pad 21 smd rect (at 3.2 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 27 /D3))
    (pad 22 smd rect (at 4 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 28 /D4))
    (pad 23 smd rect (at 5.7 -4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 29 /D5))
    (pad 24 smd rect (at 5.7 -3.2 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 30 /D6))
    (pad 25 smd rect (at 5.7 -2.4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 31 /D7))
    (pad 26 smd rect (at 5.7 -1.6 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 5.7 -0.8 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 5.7 0 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at 5.7 0.8 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 5.7 1.6 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 /A15))
    (pad 31 smd rect (at 5.7 2.4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 22 /A14))
    (pad 32 smd rect (at 5.7 3.2 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /A13))
    (pad 33 smd rect (at 5.7 4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 20 /A12))
    (pad 34 smd rect (at 4 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 19 /A11))
    (pad 35 smd rect (at 3.2 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 18 /A10))
    (pad 36 smd rect (at 2.4 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /A9))
    (pad 37 smd rect (at 1.6 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 17 /A8))
    (pad 38 smd rect (at 0.8 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 39 smd rect (at 0 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(U1-Pad39)"))
    (pad 40 smd rect (at -0.8 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 12 /A0))
    (pad 41 smd rect (at -1.6 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 13 /A1))
    (pad 42 smd rect (at -2.4 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 14 /A2))
    (pad 43 smd rect (at -3.2 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 15 /A3))
    (pad 44 smd rect (at -4 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 16 /A4))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SSOP-28_5.3x10.2mm_P0.65mm (layer B.Cu) (tedit 5A02F25C)
    (at 128.341 62.2986 270)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 0 180) (layer B.SilkS))
    (fp_text value FT232RL (at 0 -6.25 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 28 smd rect (at 3.6 4.225 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(U2-Pad28)"))
    (pad 27 smd rect (at 3.6 3.575 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 /XIN))
    (pad 26 smd rect (at 3.6 2.925 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 25 smd rect (at 3.6 2.275 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 24 smd rect (at 3.6 1.625 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 23 smd rect (at 3.6 0.975 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(U2-Pad23)"))
    (pad 22 smd rect (at 3.6 0.325 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(U2-Pad22)"))
    (pad 21 smd rect (at 3.6 -0.325 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 20 smd rect (at 3.6 -0.975 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 19 smd rect (at 3.6 -1.625 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 18 smd rect (at 3.6 -2.275 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 17 smd rect (at 3.6 -2.925 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(C3-Pad2)"))
    (pad 16 smd rect (at 3.6 -3.575 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 41 D-))
    (pad 15 smd rect (at 3.6 -4.225 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 42 D+))
    (pad 14 smd rect (at -3.6 -4.225 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(U2-Pad14)"))
    (pad 13 smd rect (at -3.6 -3.575 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(U2-Pad13)"))
    (pad 12 smd rect (at -3.6 -2.925 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(U2-Pad12)"))
    (pad 11 smd rect (at -3.6 -2.275 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(U2-Pad11)"))
    (pad 10 smd rect (at -3.6 -1.625 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(U2-Pad10)"))
    (pad 9 smd rect (at -3.6 -0.975 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(U2-Pad9)"))
    (pad 8 smd rect (at -3.6 -0.325 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -3.6 0.325 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 6 smd rect (at -3.6 0.975 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at -3.6 1.625 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U1-Pad7)"))
    (pad 4 smd rect (at -3.6 2.275 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -3.6 2.925 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at -3.6 3.575 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(U2-Pad2)"))
    (pad 1 smd rect (at -3.6 4.225 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U1-Pad5)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-28_5.3x10.2mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:TYPE-C-31-M-12 (layer B.Cu) (tedit 5DE96C9C)
    (at 115.418 61.191 90)
    (fp_text reference J1 (at 0.01016 -2.75082 -90) (layer B.SilkS))
    (fp_text value TYPE-C-31-M-12 (at -0.00254 -3.88112 -90) (layer B.Fab) hide)
    (pad A4|B9 smd rect (at -2.45 0 90) (size 0.6 1.45) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J1-PadA4|B9)"))
    (pad B8 smd rect (at -1.75 0 90) (size 0.3 1.45) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J1-PadB8)"))
    (pad A5 smd rect (at -1.25 0 90) (size 0.3 1.45) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J1-PadA5)"))
    (pad B7 smd rect (at -0.75 0 90) (size 0.3 1.45) (layers B.Cu B.Paste B.Mask)
      (net 41 D-))
    (pad A6 smd rect (at -0.25 0 90) (size 0.3 1.45) (layers B.Cu B.Paste B.Mask)
      (net 42 D+))
    (pad A7 smd rect (at 0.25 0 90) (size 0.3 1.45) (layers B.Cu B.Paste B.Mask)
      (net 41 D-))
    (pad B6 smd rect (at 0.75 0 90) (size 0.3 1.45) (layers B.Cu B.Paste B.Mask)
      (net 42 D+))
    (pad A8 smd rect (at 1.25 0 90) (size 0.3 1.45) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(J1-PadA8)"))
    (pad B5 smd rect (at 1.75 0 90) (size 0.3 1.45) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(J1-PadB5)"))
    (pad B4|A9 smd rect (at 2.45 0 90) (size 0.6 1.45) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J1-PadA4|B9)"))
    (pad B1|A12 smd rect (at 3.25 0 90) (size 0.6 1.45) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad A1|B12 smd rect (at -3.25 0 90) (size 0.6 1.45) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad GND thru_hole oval (at 4.32 -5.095 90) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad GND thru_hole oval (at 4.32 -0.915 90) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad GND thru_hole oval (at -4.32 -0.915 90) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad GND thru_hole oval (at -4.32 -5.095 90) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad "" np_thru_hole circle (at 2.89 -1.445 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 -1.445 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
  )
  (gr_line (start 109.31398 51.47056) (end 109.31398 70.92188) (layer Edge.Cuts) (width 0.2))
  (gr_text "GBFlasher Micro 1.5" (at 145.5166 69.9897) (layer B.SilkS))
  (gr_text R/W (at 126.50724 52.60086) (layer B.SilkS))
  (gr_text PWR (at 140.45184 52.60086) (layer B.SilkS))
  (gr_text https://github.com/HDR/ (at 133.07822 52.52466) (layer F.SilkS))
  (gr_line (start 157.03804 70.92188) (end 157.03804 51.47056) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 109.31398 70.92188) (end 157.03804 70.92188) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 157.03804 51.47056) (end 109.31398 51.47056) (layer Edge.Cuts) (width 0.2))
  (zone (net 34) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.36656 50.77714) (xy 157.49524 50.77714) (xy 157.49524 71.4248) (xy 108.3691 71.4248)
      )
    )
  )
  (zone (net 34) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.33862 50.77714) (xy 157.4673 50.77714) (xy 157.4673 71.4248) (xy 108.34116 71.4248)
      )
    )
  )
)
