(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 62)
    (zones 0)
    (modules 18)
    (nets 31)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.1 6.1)
    (pad_drill 3.05)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 110 107)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(SW3-Pad3)")
  (net 2 "Net-(SW3-Pad6)")
  (net 3 "Net-(SW3-Pad7)")
  (net 4 "Net-(SW3-Pad10)")
  (net 5 "Net-(SW4-Pad1)")
  (net 6 "Net-(SW4-Pad4)")
  (net 7 "Net-(SW4-Pad5)")
  (net 8 "Net-(SW4-Pad6)")
  (net 9 "Net-(J1-Pad1)")
  (net 10 "Net-(J1-Pad2)")
  (net 11 "Net-(J1-Pad3)")
  (net 12 "Net-(J2-Pad3)")
  (net 13 "Net-(J2-Pad2)")
  (net 14 "Net-(J2-Pad1)")
  (net 15 "Net-(J3-Pad1)")
  (net 16 "Net-(J3-Pad2)")
  (net 17 "Net-(J3-Pad3)")
  (net 18 "Net-(J4-Pad3)")
  (net 19 "Net-(J4-Pad2)")
  (net 20 "Net-(J4-Pad1)")
  (net 21 "Net-(J5-Pad1)")
  (net 22 "Net-(J6-Pad1)")
  (net 23 "Net-(J7-Pad1)")
  (net 24 "Net-(J8-Pad1)")
  (net 25 "Net-(J5-Pad2)")
  (net 26 "Net-(J6-Pad2)")
  (net 27 "Net-(J7-Pad2)")
  (net 28 "Net-(J8-Pad2)")
  (net 29 "Net-(J9-Pad1)")
  (net 30 "Net-(J9-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class audio ""
    (clearance 0.2)
    (trace_width 0.6069)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(J9-Pad2)")
    (add_net "Net-(SW3-Pad10)")
    (add_net "Net-(SW3-Pad3)")
    (add_net "Net-(SW3-Pad6)")
    (add_net "Net-(SW3-Pad7)")
    (add_net "Net-(SW4-Pad1)")
    (add_net "Net-(SW4-Pad4)")
    (add_net "Net-(SW4-Pad5)")
    (add_net "Net-(SW4-Pad6)")
  )
  (module push-sw:Alps_C&K_F_4PDT-1.3 (layer Top) (tedit 6076016C)
    (at 123 80.25 270)
    (descr "Switch, single pole double throw, illuminated paddle, http://www.nkkswitches.com/pdf/gwillum.pdf")
    (tags "switch single-pole double-throw spdt ON-ON illuminated LED")
    (fp_text reference SW3 (at -6.25 2.5) (layer F.SilkS))
    (fp_text value GAIN-Right (at 9.95 9.4 270) (layer F.SilkS))
    (fp_text user %R (at 2.54 1.27 90) (layer F.Fab))
    (pad 12 thru_hole circle (at 20 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 28 "Net-(J8-Pad2)"))
    (pad 10 thru_hole circle (at 12 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(SW3-Pad10)"))
    (pad 11 thru_hole circle (at 16 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 "Net-(J8-Pad1)"))
    (pad 9 thru_hole circle (at 20 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 23 "Net-(J7-Pad1)"))
    (pad 8 thru_hole circle (at 16 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 27 "Net-(J7-Pad2)"))
    (pad 7 thru_hole circle (at 12 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(SW3-Pad7)"))
    (pad 6 thru_hole circle (at 8 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(SW3-Pad6)"))
    (pad 3 thru_hole circle (at 8 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(SW3-Pad3)"))
    (pad 5 thru_hole circle (at 4 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad2)"))
    (pad 2 thru_hole circle (at 4 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J5-Pad1)"))
    (pad 4 thru_hole circle (at 0 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 25 "Net-(J5-Pad2)"))
    (model ${KIPRJMOD}/lib/3D/spun194700.stp
      (offset (xyz 10 -3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module push-sw:Alps_C&K_F_DPDT-1.3 (layer Top) (tedit 607601A0)
    (at 143 80.25 270)
    (descr "Switch, single pole double throw, illuminated paddle, http://www.nkkswitches.com/pdf/gwillum.pdf")
    (tags "switch single-pole double-throw spdt ON-ON illuminated LED")
    (fp_text reference SW4 (at -6.25 2.5) (layer F.SilkS))
    (fp_text value MONO (at 15.75 3 180) (layer F.SilkS))
    (fp_text user %R (at 2.54 1.27 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 8 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(SW4-Pad6)"))
    (pad 3 thru_hole circle (at 8 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 29 "Net-(J9-Pad1)"))
    (pad 5 thru_hole circle (at 4 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(SW4-Pad5)"))
    (pad 2 thru_hole circle (at 4 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 "Net-(J9-Pad2)"))
    (pad 4 thru_hole circle (at 0 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(SW4-Pad4)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(SW4-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/spun191400.stp
      (offset (xyz -10 -3 6))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Alps_C&K_F_DPDT-1.3 (layer Top) (tedit 607601A0)
    (at 103 80.25 270)
    (descr "Switch, single pole double throw, illuminated paddle, http://www.nkkswitches.com/pdf/gwillum.pdf")
    (tags "switch single-pole double-throw spdt ON-ON illuminated LED")
    (fp_text reference SW2 (at -6.25 2.5) (layer F.SilkS))
    (fp_text value WARP (at 15.75 3) (layer F.SilkS))
    (fp_text user %R (at 2.54 1.27 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 8 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad3)"))
    (pad 3 thru_hole circle (at 8 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad3)"))
    (pad 5 thru_hole circle (at 4 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad2)"))
    (pad 2 thru_hole circle (at 4 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad2)"))
    (pad 4 thru_hole circle (at 0 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(J4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/spun191400.stp
      (offset (xyz -10 -3 6))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Alps_C&K_F_DPDT-1.3 (layer Top) (tedit 607601A0)
    (at 83 80.25 270)
    (descr "Switch, single pole double throw, illuminated paddle, http://www.nkkswitches.com/pdf/gwillum.pdf")
    (tags "switch single-pole double-throw spdt ON-ON illuminated LED")
    (fp_text reference SW1 (at -6.25 2.5) (layer F.SilkS))
    (fp_text value PHONO (at 15.75 3) (layer F.SilkS))
    (fp_text user %R (at 2.54 1.27 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 8 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad3)"))
    (pad 3 thru_hole circle (at 8 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 4 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 2 thru_hole circle (at 4 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 0 6 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/spun191400.stp
      (offset (xyz -10 -3 6))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm (layer Top) (tedit 56D1B4CB)
    (at 70 73.8)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0.1 -6.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer Top) (tedit 56D1B4CB)
    (at 90 73.8)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 -6.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer Top) (tedit 56D1B4CB)
    (at 110 73.8)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at -0.1 -6.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer Top) (tedit 56D1B4CB)
    (at 130 73.8)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at -0.1 -6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer Top) (tedit 56D1B4CB)
    (at 150 73.8)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H5 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at -0.1 -6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module push-sw:Molex_KK_1x03_P2.54mm_Horizontal (layer Top) (tedit 60776524)
    (at 77.5 102.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-03A example for new part number: 22-27-2031, 3 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J1 (at 2.54 -2.2) (layer F.SilkS) hide)
    (fp_text value Left (at 2.5 -3.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 2.4) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 9 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad3)"))
    (model ${KIPRJMOD}/lib/3D/022122031.stp
      (offset (xyz 2.54 0 1.65))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Molex_KK_1x03_P2.54mm_Horizontal (layer Top) (tedit 60776524)
    (at 69.5 102.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-03A example for new part number: 22-27-2031, 3 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J2 (at 2.54 -2.2) (layer F.SilkS) hide)
    (fp_text value Right (at 2.5 -3.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 2.4) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 14 "Net-(J2-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/022122031.stp
      (offset (xyz 2.54 0 1.65))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Molex_KK_1x02_P2.54mm_Horizontal (layer Top) (tedit 6077605A)
    (at 105.5 102.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J6 (at 1.1 -2) (layer F.SilkS) hide)
    (fp_text value 0dB (at 1.27 -2.25) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.4) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 22 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/022122021.stp
      (offset (xyz 1.27 0 1.65))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Molex_KK_1x02_P2.54mm_Horizontal (layer Top) (tedit 6077605A)
    (at 111 102.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J8 (at 1.1 -2) (layer F.SilkS) hide)
    (fp_text value 10dB (at 1.25 -2.25) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.4) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 "Net-(J8-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 24 "Net-(J8-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/022122021.stp
      (offset (xyz 1.27 0 1.65))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Molex_KK_1x03_P2.54mm_Horizontal (layer Top) (tedit 60776524)
    (at 95.5 102.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-03A example for new part number: 22-27-2031, 3 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J3 (at 2.54 -2.2) (layer F.SilkS) hide)
    (fp_text value Left (at 2.6 -3.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 2.4) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 15 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad3)"))
    (model ${KIPRJMOD}/lib/3D/022122031.stp
      (offset (xyz 2.54 0 1.65))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Molex_KK_1x03_P2.54mm_Horizontal (layer Top) (tedit 60776524)
    (at 87.5 102.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-03A example for new part number: 22-27-2031, 3 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J4 (at 2.54 -2.2) (layer F.SilkS) hide)
    (fp_text value Right (at 2.6 -3.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 2.4) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 20 "Net-(J4-Pad1)"))
    (model ${KIPRJMOD}/lib/3D/022122031.stp
      (offset (xyz 2.54 0 1.65))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Molex_KK_1x02_P2.54mm_Horizontal (layer Top) (tedit 6079CE35)
    (at 132 102.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J5 (at 1.1 -2) (layer F.SilkS) hide)
    (fp_text value 0dB (at 1.27 -2.25) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.4) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(J5-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.144)
      (net 21 "Net-(J5-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/022122021.stp
      (offset (xyz 1.27 0 1.65))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Molex_KK_1x02_P2.54mm_Horizontal (layer Top) (tedit 6079CE35)
    (at 126.5 102.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J7 (at 1.1 -2) (layer F.SilkS) hide)
    (fp_text value 10dB (at 1.27 -2.25) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.4) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.144)
      (net 23 "Net-(J7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(J7-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/022122021.stp
      (offset (xyz 1.27 0 1.65))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module push-sw:Molex_KK_1x02_P2.54mm_Horizontal (layer Top) (tedit 6079CE35)
    (at 143 102.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J9 (at 1.1 -2) (layer F.SilkS) hide)
    (fp_text value Mono (at 1.27 -2.25) (layer F.SilkS))
    (fp_text user %R (at 1.1 2.4) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.144)
      (net 29 "Net-(J9-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 30 "Net-(J9-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/022122021.stp
      (offset (xyz 1.27 0 1.65))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_text On (at 100.6 100.5) (layer F.SilkS))
  (gr_text On (at 92.6 100.5) (layer F.SilkS))
  (gr_text Off (at 95.5 100.5) (layer F.SilkS))
  (gr_text Off (at 87.5 100.5) (layer F.SilkS))
  (gr_text MC (at 82.6 100.5) (layer F.SilkS))
  (gr_text MM (at 77.5 100.5) (layer F.SilkS))
  (gr_text MC (at 74.6 100.5) (layer F.SilkS))
  (gr_text MM (at 69.5 100.5) (layer F.SilkS))
  (gr_text GAIN-Left (at 126.4 90.2 90) (layer F.SilkS))
  (gr_line (start 153 70) (end 67 70) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153 107) (end 153 70) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 67 107) (end 153 107) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 67 70) (end 67 107) (layer Edge.Cuts) (width 0.05))
)
