(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 127.700005 47.5334)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/GND")
  (net 2 "unconnected-(J1-Pad12)")
  (net 3 "unconnected-(J1-Pad13)")
  (net 4 "/SIG")
  (net 5 "unconnected-(J1-Pad21)")
  (net 6 "unconnected-(J1-Pad22)")
  (footprint "Library:CONN_XF3M-3315-1B_OMR" (layer "F.Cu")
    (at 135.200005 73.033399 -90)
    (tags "XF3M-3315-1B ")
    (property "Sheetfile" "CoaxBreakoutSymmetric.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "XF3M-3315-1B")
    (clearance 0.2)
    (attr smd)
    (fp_text reference "J1" (at -8 2.5 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "XF3M-3315-1B" (at -7.999999 4.5 -90 unlocked) (layer "F.Fab"))
    (fp_text user "XF3M-3315-1B" (at -8 2.5 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -15.999999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at -15.5 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at -15.000001 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "3") (pintype "unspecified"))
    (pad "4" smd rect (at -14.499999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "4") (pintype "unspecified"))
    (pad "5" smd rect (at -14 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "5") (pintype "unspecified"))
    (pad "6" smd rect (at -13.499998 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "6") (pintype "unspecified"))
    (pad "7" smd rect (at -12.999999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "7") (pintype "unspecified"))
    (pad "8" smd rect (at -12.5 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "8") (pintype "unspecified"))
    (pad "9" smd rect (at -11.999999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "9") (pintype "unspecified"))
    (pad "10" smd rect (at -11.5 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "10") (pintype "unspecified"))
    (pad "11" smd rect (at -10.999998 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "11") (pintype "unspecified"))
    (pad "12" smd rect (at -10.499999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "unconnected-(J1-Pad12)") (pinfunction "12") (pintype "unspecified"))
    (pad "13" smd rect (at -10 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "unconnected-(J1-Pad13)") (pinfunction "13") (pintype "unspecified"))
    (pad "14" smd rect (at -9.499999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SIG") (pinfunction "14") (pintype "unspecified"))
    (pad "15" smd rect (at -9 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SIG") (pinfunction "15") (pintype "unspecified"))
    (pad "16" smd rect (at -8.499998 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SIG") (pinfunction "16") (pintype "unspecified"))
    (pad "17" smd rect (at -7.999999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SIG") (pinfunction "17") (pintype "unspecified"))
    (pad "18" smd rect (at -7.5 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SIG") (pinfunction "18") (pintype "unspecified"))
    (pad "19" smd rect (at -6.999999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SIG") (pinfunction "19") (pintype "unspecified"))
    (pad "20" smd rect (at -6.5 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SIG") (pinfunction "20") (pintype "unspecified"))
    (pad "21" smd rect (at -5.999998 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(J1-Pad21)") (pinfunction "21") (pintype "unspecified"))
    (pad "22" smd rect (at -5.499999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(J1-Pad22)") (pinfunction "22") (pintype "unspecified"))
    (pad "23" smd rect (at -5 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "23") (pintype "unspecified"))
    (pad "24" smd rect (at -4.499999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "24") (pintype "unspecified"))
    (pad "25" smd rect (at -4 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "25") (pintype "unspecified"))
    (pad "26" smd rect (at -3.499998 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "26") (pintype "unspecified"))
    (pad "27" smd rect (at -2.999999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "27") (pintype "unspecified"))
    (pad "28" smd rect (at -2.5 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "28") (pintype "unspecified"))
    (pad "29" smd rect (at -1.999999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "29") (pintype "unspecified"))
    (pad "30" smd rect (at -1.5 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "30") (pintype "unspecified"))
    (pad "31" smd rect (at -0.999998 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "31") (pintype "unspecified"))
    (pad "32" smd rect (at -0.499999 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "32") (pintype "unspecified"))
    (pad "33" smd rect (at 0 0 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "33") (pintype "unspecified"))
    (pad "34" smd rect (at -17.9 3.250001 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "35" smd rect (at 1.900001 3.250001 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "Library:LINX_CONSMA020.062-G" (layer "F.Cu")
    (at 146.382505 65.0334 90)
    (property "Description" "SMA Jack 50 Ohm .062 PCB Edge Mount")
    (property "MF" "Linx Technologies")
    (property "MP" "CONSMA020.062-G")
    (property "Sheetfile" "CoaxBreakoutSymmetric.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at -2.468 -8.2864 90) (layer "F.SilkS") hide)
    (fp_text value "CONSMA020.062-G" (at 3.628 -7.2464 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 -2.8 90) (size 1.5 5.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SIG") (pintype "passive") (solder_mask_margin 0.102))
    (pad "S1" smd rect (at -4.26 -2.45 90) (size 1.6 4.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pintype "passive") (solder_mask_margin 0.102))
    (pad "S2" smd rect (at 4.26 -2.45 90) (size 1.6 4.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (solder_mask_margin 0.102))
    (pad "S3" smd rect (at -4.26 -2.45 90) (size 1.6 4.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.102))
    (pad "S4" smd rect (at 4.26 -2.45 90) (size 1.6 4.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.102))
  )
  (gr_rect (start 129.700005 53.7834) (end 146.700005 76.2834)
    (fill none) (layer "Edge.Cuts"))
  (zone (net 1) (net_name "/GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.25))
    (min_thickness 0) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 127.700005 47.7834)
        (xy 146.700005 47.2834)
        (xy 147.200005 77.0334)
        (xy 127.700005 76.2834)
      )
    )
  )
  (zone (net 4) (net_name "/SIG") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 134.400005 63.3834)
        (xy 137.050005 63.3834)
        (xy 138.550005 64.8834)
        (xy 138.550005 65.0834)
        (xy 136.950005 66.6834)
        (xy 134.400005 66.6834)
      )
    )
  )
)
