<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40.62" y2="0" width="0" layer="20"/>
<wire x1="40.62" y1="0" x2="40.62" y2="46.66" width="0" layer="20"/>
<wire x1="40.62" y1="46.66" x2="0" y2="46.66" width="0" layer="20"/>
<wire x1="0" y1="46.66" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="2.54" drill="2.2"/>
<hole x="38.1" y="2.54" drill="2.2"/>
<hole x="38.1" y="44.45" drill="2.2"/>
<hole x="2.54" y="44.45" drill="2.2"/>
<text>RED</text>
<text>BLUE</text>
<text>GREEN</text>
<text>VERA ARDUINO
GATEWAY</text>
<text>www.mysensors.org</text>
<text>PCB Layout
(C) 2014
Ross Kinard
4/18/2014</text>
</plain>
<libraries>
<library name="MyLibrary">
<packages>
<package name="ARDUINO_NANO">
<description>Footprint for representing an Arduino Nano board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="E2-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2 mm, diameter 4 mm</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PCB1" library="MyLibrary" package="ARDUINO_NANO" value="ARDUINO_NANO"/>
<element name="RF_CARD" library="MyLibrary" package="2X04" value=""/>
<element name="C1" library="MyLibrary" package="E2-4" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INCLUDE" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH"/>
<element name="RX" library="MyLibrary" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX" library="MyLibrary" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ERR" library="MyLibrary" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0207/10" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0207/10" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0207/10" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0207/10" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="PCB1" pad="5V"/>
<contactref element="INCLUDE" pad="1"/>
<contactref element="ERR" pad="A"/>
<contactref element="TX" pad="A"/>
<contactref element="RX" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="1"/>
<contactref element="INCLUDE" pad="3"/>
<contactref element="PCB1" pad="D3"/>
</signal>
<signal name="N$4">
<contactref element="RX" pad="K"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="TX" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="ERR" pad="K"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="PCB1" pad="D4"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="PCB1" pad="D5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="PCB1" pad="D6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="PCB1" pad="GND"/>
<contactref element="RF_CARD" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="PCB1" pad="GND."/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="PCB1" pad="3V3"/>
<contactref element="RF_CARD" pad="2"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="N$12">
<contactref element="PCB1" pad="D9"/>
<contactref element="RF_CARD" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="PCB1" pad="D10"/>
<contactref element="RF_CARD" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="RF_CARD" pad="5"/>
<contactref element="PCB1" pad="D13"/>
</signal>
<signal name="N$15">
<contactref element="RF_CARD" pad="6"/>
<contactref element="PCB1" pad="D11"/>
</signal>
<signal name="N$16">
<contactref element="RF_CARD" pad="7"/>
<contactref element="PCB1" pad="D12"/>
</signal>
<signal name="N$17">
<contactref element="RF_CARD" pad="8"/>
<contactref element="PCB1" pad="D2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
