(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" jumper)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.058)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plots/")
		)
	)
	(net 0 "")
	(net 1 "/A8")
	(net 2 "/D2")
	(net 3 "/A9")
	(net 4 "/D1")
	(net 5 "GND")
	(net 6 "/D0")
	(net 7 "VDD")
	(net 8 "/A0")
	(net 9 "/A10")
	(net 10 "/A1")
	(net 11 "Net-(U1-~{CS})")
	(net 12 "/A2")
	(net 13 "/D7")
	(net 14 "/A3")
	(net 15 "/D6")
	(net 16 "/A4")
	(net 17 "/D5")
	(net 18 "/A5")
	(net 19 "/D4")
	(net 20 "/A6")
	(net 21 "/D3")
	(net 22 "/A7")
	(net 23 "Net-(U1-~{OE})")
	(net 24 "Net-(U1-~{WE})")
	(footprint "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
		(layer "F.Cu")
		(at 153.4 99.255)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at 0 -9.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FM16W08-SG"
			(at 0 9.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.cypress.com/file/41731/download"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC?28*7.5x17.9mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "/home/dlebed/devel/pcb/3458a/fram/FRAM 3458A CAL/FRAM 3458A CAL.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 -8.255)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -4.65 -6.985)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pinfunction "A12")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -4.65 -5.715)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/A7")
			(pinfunction "A7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -4.65 -4.445)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/A6")
			(pinfunction "A6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -4.65 -3.175)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/A5")
			(pinfunction "A5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -4.65 -1.905)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/A4")
			(pinfunction "A4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -4.65 -0.635)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/A3")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -4.65 0.635)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/A2")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -4.65 1.905)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/A1")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -4.65 3.175)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/A0")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -4.65 4.445)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/D0")
			(pinfunction "DQ0")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -4.65 5.715)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/D1")
			(pinfunction "DQ1")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at -4.65 6.985)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/D2")
			(pinfunction "DQ2")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at -4.65 8.255)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 4.65 8.255)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/D3")
			(pinfunction "DQ3")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 4.65 6.985)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/D4")
			(pinfunction "DQ4")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 4.65 5.715)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/D5")
			(pinfunction "DQ5")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 4.65 4.445)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/D6")
			(pinfunction "DQ6")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 4.65 3.175)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/D7")
			(pinfunction "DQ7")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 4.65 1.905)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U1-~{CS})")
			(pinfunction "~{CE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 4.65 0.635)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/A10")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 4.65 -0.635)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U1-~{OE})")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 4.65 -1.905)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pinfunction "A11")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 4.65 -3.175)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/A9")
			(pinfunction "A9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 4.65 -4.445)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/A8")
			(pinfunction "A8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 4.65 -5.715)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 4.65 -6.985)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U1-~{WE})")
			(pinfunction "~{WE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 4.65 -8.255)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-24_W15.24mm_Socket"
		(layer "F.Cu")
		(at 145.75 86.5)
		(descr "24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
		(property "Reference" "U1"
			(at 7.62 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DS1220"
			(at 7.62 30.27 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/31579.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* PDIP*")
		(sheetname "Root")
		(sheetfile "/home/dlebed/devel/pcb/3458a/fram/FRAM 3458A CAL/FRAM 3458A CAL.sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 13.97 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/A7")
			(pinfunction "A7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/A6")
			(pinfunction "A6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/A5")
			(pinfunction "A5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/A4")
			(pinfunction "A4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/A3")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/A2")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/A1")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/A0")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/D0")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/D1")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/D2")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole oval
			(at 15.24 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/D3")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole oval
			(at 15.24 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/D4")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole oval
			(at 15.24 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/D5")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole oval
			(at 15.24 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/D6")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole oval
			(at 15.24 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/D7")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole oval
			(at 15.24 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(U1-~{CS})")
			(pinfunction "~{CS}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole oval
			(at 15.24 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/A10")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole oval
			(at 15.24 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(U1-~{OE})")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole oval
			(at 15.24 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(U1-~{WE})")
			(pinfunction "~{WE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole oval
			(at 15.24 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/A9")
			(pinfunction "A9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole oval
			(at 15.24 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/A8")
			(pinfunction "A8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole oval
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "VDD")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KISYS3DMOD}/Package_DIP.3dshapes/DIP-24_W15.24mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 157.2 89.1 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 3.2 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "/home/dlebed/devel/pcb/3458a/fram/FRAM 3458A CAL/FRAM 3458A CAL.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 157.2 87.4 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 3.2 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.43 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "/home/dlebed/devel/pcb/3458a/fram/FRAM 3458A CAL/FRAM 3458A CAL.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 145.6 116.1)
		(mid 144.53934 115.66066)
		(end 144.1 114.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.6 86.3)
		(end 162.6 114.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.6 84.8)
		(end 161.1 84.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.1 114.6)
		(end 144.1 86.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.1 116.1)
		(end 145.6 116.1)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.1 86.3)
		(mid 144.53934 85.23934)
		(end 145.6 84.8)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 161.1 84.8)
		(mid 162.16066 85.23934)
		(end 162.6 86.3)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 162.6 114.6)
		(mid 162.16066 115.66066)
		(end 161.1 116.1)
		(layer "Edge.Cuts")
	)
	(gr_text "3458A\nCAL RAM\nFM16W08"
		(at 153.4 112.1 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "/D2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.951989 106.113) (xy 149.951989 106.367) (xy 150.596927 106.619552) (xy 150.751 106.25) (xy 150.596927 105.880448)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/D1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.955967 104.843) (xy 149.955967 105.097) (xy 150.596927 105.369552) (xy 150.751 105) (xy 150.596927 104.630448)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/D5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.725 104.843) (xy 156.725 105.097) (xy 157.117597 105.258582) (xy 158.051 104.97) (xy 157.117597 104.681418)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.075 96.207) (xy 150.075 95.953) (xy 149.682403 95.791418) (xy 148.749 96.08) (xy 149.682403 96.368582)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.725 94.683) (xy 156.725 94.937) (xy 157.117597 95.098582) (xy 158.051 94.81) (xy 157.117597 94.521418)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/D4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.725 106.113) (xy 156.725 106.367) (xy 157.117597 106.528582) (xy 158.051 106.24) (xy 157.117597 105.951418)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/D6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.790054 103.827) (xy 156.790054 103.573) (xy 156.153073 103.380448) (xy 155.999 103.75) (xy 156.153073 104.119552)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.971172 103.238433) (xy 146.791567 103.058828) (xy 145.443853 103.540896) (xy 145.749293 104.280707)
				(xy 146.489104 104.586147)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.875 89.354) (xy 158.875 88.846) (xy 158.297887 88.65) (xy 157.974 89.1) (xy 158.297887 89.55)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.675807 99.763) (xy 159.675807 100.017) (xy 160.99 100) (xy 160.991 99.2) (xy 160.250896 98.893853)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.573382 97.118777) (xy 147.393777 97.298382) (xy 147.732637 97.538396) (xy 148.750707 97.350707)
				(xy 147.817597 97.061418)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/D5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.794033 105.097) (xy 156.794033 104.843) (xy 156.153073 104.630448) (xy 155.999 105) (xy 156.153073 105.369552)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.725 95.953) (xy 156.725 96.207) (xy 157.117597 96.368582) (xy 158.051 96.08) (xy 157.117597 95.791418)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/D3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.923 108.11) (xy 158.177 108.11) (xy 158.35 107.81) (xy 158.05 107.509) (xy 157.75 107.81)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.39 86.246) (xy 159.39 86.754) (xy 160.683853 87.239104) (xy 160.991 86.5) (xy 160.683853 85.760896)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(U1-~{CS})")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.375 101.287) (xy 159.375 101.033) (xy 158.982403 100.871418) (xy 158.049 101.16) (xy 158.982403 101.448582)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/D7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.948433 103.058828) (xy 159.768828 103.238433) (xy 160.250896 104.586147) (xy 160.990707 104.280707)
				(xy 161.296147 103.540896)
			)
		)
	)
	(zone
		(net 24)
		(net_name "Net-(U1-~{WE})")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.948433 92.898828) (xy 159.768828 93.078433) (xy 160.250896 94.426147) (xy 160.990707 94.120707)
				(xy 161.296147 93.380896)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.532638 91.126572) (xy 159.173428 90.767362) (xy 158.982403 90.711418) (xy 158.049293 91.000707)
				(xy 159.024005 91.260783)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/A3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.598278 98.328673) (xy 147.418673 98.508278) (xy 147.725 98.757674) (xy 148.750707 98.620707)
				(xy 147.875 98.32)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/A6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.961935 94.683) (xy 149.961935 94.937) (xy 150.596927 95.119552) (xy 150.751 94.75) (xy 150.596927 94.380448)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.788065 94.937) (xy 156.788065 94.683) (xy 156.153073 94.380448) (xy 155.999 94.75) (xy 156.153073 95.119552)
			)
		)
	)
	(zone
		(net 24)
		(net_name "Net-(U1-~{WE})")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.216367 92.525972) (xy 159.395972 92.346367) (xy 159.071495 92.102379) (xy 158.049293 92.269293)
				(xy 158.925 92.57)
			)
		)
	)
	(zone
		(net 23)
		(net_name "Net-(U1-~{OE})")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.768828 97.701567) (xy 159.948433 97.881172) (xy 161.296147 97.399104) (xy 160.990707 96.659293)
				(xy 160.250896 96.353853)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.386454 102.463941) (xy 147.566059 102.643546) (xy 147.817597 102.718582) (xy 148.750707 102.429293)
				(xy 147.735542 102.226997)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/D3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.948433 113.218828) (xy 159.768828 113.398433) (xy 160.250896 114.746147) (xy 160.990707 114.440707)
				(xy 161.296147 113.700896)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/D0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.959946 103.573) (xy 149.959946 103.827) (xy 150.596927 104.119552) (xy 150.751 103.75) (xy 150.596927 103.380448)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/A3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.791567 97.881172) (xy 146.971172 97.701567) (xy 146.489104 96.353853) (xy 145.749293 96.659293)
				(xy 145.443853 97.399104)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/D0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.075 103.827) (xy 150.075 103.573) (xy 149.682403 103.411418) (xy 148.749 103.7) (xy 149.682403 103.988582)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.721 88.325) (xy 158.229 88.325) (xy 158.407873 87.736104) (xy 157.975 87.399) (xy 157.542127 87.736104)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.707956 93.413) (xy 150.707956 93.667) (xy 151.346927 93.869552) (xy 151.501 93.5) (xy 151.346927 93.130448)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.375 100.017) (xy 159.375 99.763) (xy 158.982403 99.601418) (xy 158.049 99.89) (xy 158.982403 100.178582)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/A6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.075 94.937) (xy 150.075 94.683) (xy 149.682403 94.521418) (xy 148.749 94.81) (xy 149.682403 95.098582)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(U1-~{CS})")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.630244 101.033) (xy 159.630244 101.287) (xy 160.424315 102.305685) (xy 160.991 101.74) (xy 160.99 100.94)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.791567 95.341172) (xy 146.971172 95.161567) (xy 146.489104 93.813853) (xy 145.749293 94.119293)
				(xy 145.443853 94.859104)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.866916 86.867295) (xy 158.507705 86.508084) (xy 157.813604 86.925) (xy 157.974293 87.400707)
				(xy 158.425 87.586396)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.784087 96.207) (xy 156.784087 95.953) (xy 156.153073 95.630448) (xy 155.999 96) (xy 156.153073 96.369552)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.425 101.033) (xy 147.425 101.287) (xy 147.817597 101.448582) (xy 148.751 101.16) (xy 147.817597 100.871418)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.064193 100.017) (xy 147.064193 99.763) (xy 146.489104 98.893853) (xy 145.749 99.2) (xy 145.75 100)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.965913 95.953) (xy 149.965913 96.207) (xy 150.596927 96.369552) (xy 150.751 96) (xy 150.596927 95.630448)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/D6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.725 103.573) (xy 156.725 103.827) (xy 157.117597 103.988582) (xy 158.051 103.7) (xy 157.117597 103.411418)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/D2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.075 106.367) (xy 150.075 106.113) (xy 149.682403 105.951418) (xy 148.749 106.24) (xy 149.682403 106.528582)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/D7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.216367 102.685972) (xy 159.395972 102.506367) (xy 159.071495 102.262379) (xy 158.049293 102.429293)
				(xy 158.925 102.73)
			)
		)
	)
	(zone
		(net 23)
		(net_name "Net-(U1-~{OE})")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.376934 98.452671) (xy 159.197329 98.273066) (xy 158.021776 98.32) (xy 158.049293 98.620707)
				(xy 159.075 98.713494)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.075 93.667) (xy 150.075 93.413) (xy 149.682403 93.251418) (xy 148.749 93.54) (xy 149.682403 93.828582)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/D1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.075 105.097) (xy 150.075 104.843) (xy 149.682403 104.681418) (xy 148.749 104.97) (xy 149.682403 105.258582)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.425 99.763) (xy 147.425 100.017) (xy 147.817597 100.178582) (xy 148.751 99.89) (xy 147.817597 99.601418)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/D4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.798011 106.367) (xy 156.798011 106.113) (xy 156.153073 105.880448) (xy 155.999 106.25) (xy 156.153073 106.619552)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.109756 101.287) (xy 147.109756 101.033) (xy 145.75 100.94) (xy 145.749 101.74) (xy 146.315685 102.305685)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.229 88.175) (xy 157.721 88.175) (xy 157.542127 88.763896) (xy 157.975 89.101) (xy 158.407873 88.763896)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layers "F&B.Cu")
		(name "GND")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.25)
		)
		(polygon
			(pts
				(xy 144.6 85.3) (xy 162.1 85.3) (xy 162.1 115.7) (xy 144.6 115.7)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/D6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.948433 105.598828) (xy 159.768828 105.778433) (xy 160.250896 107.126147) (xy 160.990707 106.820707)
				(xy 161.296147 106.080896)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.146371 94.063234) (xy 155.966766 93.883629) (xy 155.630448 94.596927) (xy 155.999293 94.750707)
				(xy 156.369552 94.596927)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.10424 95.754634) (xy 149.924634 95.93424) (xy 150.596927 96.369552) (xy 150.750707 96.000707)
				(xy 150.596927 95.630448)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/D1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.907061 105.023334) (xy 150.086666 105.202939) (xy 150.596927 105.369552) (xy 150.750707 104.999293)
				(xy 150.596927 104.630448)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.768828 90.081567) (xy 159.948433 90.261172) (xy 161.296147 89.779104) (xy 160.990707 89.039293)
				(xy 160.250896 88.733853)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/D6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.8 103.877) (xy 156.8 103.623) (xy 156.153073 103.380448) (xy 155.999 103.75) (xy 156.153073 104.119552)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/D2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.971172 110.858433) (xy 146.791567 110.678828) (xy 145.443853 111.160896) (xy 145.749293 111.900707)
				(xy 146.489104 112.206147)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/A6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.776162 93.886558) (xy 150.596558 94.066162) (xy 150.380448 94.596927) (xy 150.750707 94.750707)
				(xy 151.119552 94.596927)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/A7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.627 92.7) (xy 151.373 92.7) (xy 151.130448 93.346927) (xy 151.5 93.501) (xy 151.869552 93.346927)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.791567 92.801172) (xy 146.971172 92.621567) (xy 146.489104 91.273853) (xy 145.749293 91.579293)
				(xy 145.443853 92.319104)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/D0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.971172 105.778433) (xy 146.791567 105.598828) (xy 145.443853 106.080896) (xy 145.749293 106.820707)
				(xy 146.489104 107.126147)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/D0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.95 103.623) (xy 149.95 103.877) (xy 150.596927 104.119552) (xy 150.751 103.75) (xy 150.596927 103.380448)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/D4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.948433 110.678828) (xy 159.768828 110.858433) (xy 160.250896 112.206147) (xy 160.990707 111.900707)
				(xy 161.296147 111.160896)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/D4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.873 107.05) (xy 156.127 107.05) (xy 156.369552 106.403073) (xy 156 106.249) (xy 155.630448 106.403073)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/D5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.948433 108.138828) (xy 159.768828 108.318433) (xy 160.250896 109.666147) (xy 160.990707 109.360707)
				(xy 161.296147 108.620896)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/D2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.623 107.05) (xy 150.877 107.05) (xy 151.119552 106.403073) (xy 150.75 106.249) (xy 150.380448 106.403073)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/A7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.025882 87.955487) (xy 147.205487 87.775882) (xy 146.55 86.16863) (xy 145.749293 86.499293)
				(xy 145.41863 87.3)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.655488 95.524117) (xy 156.475883 95.344512) (xy 155.846927 95.630448) (xy 155.999293 96.000707)
				(xy 156.369552 96.153073)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/D1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.971172 108.318433) (xy 146.791567 108.138828) (xy 145.443853 108.620896) (xy 145.749293 109.360707)
				(xy 146.489104 109.666147)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/A6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.791567 90.261172) (xy 146.971172 90.081567) (xy 146.489104 88.733853) (xy 145.749293 89.039293)
				(xy 145.443853 89.779104)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.572672 92.247723) (xy 159.752277 92.427328) (xy 160.99 92.38) (xy 160.990707 91.579293)
				(xy 160.424315 91.014315)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/D5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.660405 105.21001) (xy 156.84001 105.030405) (xy 156.153073 104.630448) (xy 155.999293 104.999293)
				(xy 156.153073 105.369552)
			)
		)
	)
)
