(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 25.5 28)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/motor_data")
	(net 3 "/uc_send")
	(net 4 "VDD")
	(net 5 "/uc_recv")
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 38.5 25.65 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.43 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PU"
			(at 2.25 -1.1 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/uc_send")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "BSS138W:BSS138W"
		(layer "F.Cu")
		(at 38.5 23.4)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "Q1"
			(at -0.05 -2.25 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BSS138W"
			(at 2.75 -1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "BSS138W:BSS138W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-MOSFET transistor, gate/source/drain"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "VDD")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/uc_send")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/motor_data")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/kicad-library/BSS138W/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "BSS138W:BSS138W"
		(layer "F.Cu")
		(at 38.5 28.65)
		(descr "SOT-323, SC-70")
		(tags "SOT-323 SC-70")
		(property "Reference" "Q2"
			(at -0.05 -2.25 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BSS138W"
			(at 2.5 1.85 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "BSS138W:BSS138W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-MOSFET transistor, gate/source/drain"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "VDD")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1 0.65 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/uc_recv")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/motor_data")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/kicad-library/BSS138W/SOT-323_SC-70.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TZ042101B000G:TZ042101B000G"
		(layer "F.Cu")
		(at 25.5 28 -90)
		(property "Reference" "J2"
			(at 0 5.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Screw_Terminal_01x04"
			(at 0 4.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TZ042101B000G:TZ042101B000G"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -8 0 270)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 8 0 270)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -5.25 -4.95 270)
			(size 1.4 5.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.75 -4.95 270)
			(size 1.4 5.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/uc_send")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.75 -4.95 270)
			(size 1.4 5.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/uc_recv")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 5.25 -4.95 270)
			(size 1.4 5.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/kicad-library/TZ042101B000G/691508110304_rev1.stp"
			(offset
				(xyz 0 0 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad"
		(layer "F.Cu")
		(at 53 39)
		(descr "Mounting Hole 2.2mm, M2, ISO14580")
		(tags "mounting hole 2.2mm m2 iso14580")
		(property "Reference" "H4"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 38.5 30.9 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.43 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PU"
			(at -2.25 -0.1 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/uc_recv")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad"
		(layer "F.Cu")
		(at 23.5 39)
		(descr "Mounting Hole 2.2mm, M2, ISO14580")
		(tags "mounting hole 2.2mm m2 iso14580")
		(property "Reference" "H2"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad"
		(layer "F.Cu")
		(at 23.5 17)
		(descr "Mounting Hole 2.2mm, M2, ISO14580")
		(tags "mounting hole 2.2mm m2 iso14580")
		(property "Reference" "H1"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad"
		(layer "F.Cu")
		(at 53 17)
		(descr "Mounting Hole 2.2mm, M2, ISO14580")
		(tags "mounting hole 2.2mm m2 iso14580")
		(property "Reference" "H3"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "TZ022101B000G:TZ022101B000G"
		(layer "F.Cu")
		(at 51 28 90)
		(property "Reference" "J1"
			(at 0 5.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 0 4.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TZ022101B000G:TZ022101B000G"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "project-nrf-garage-remote.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -4.5 0 90)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 4.5 0 90)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -1.75 -4.95 90)
			(size 1.4 5.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.75 -4.95 90)
			(size 1.4 5.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/motor_data")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/kicad-library/TZ022101B000G/691508110302 (rev1).stp"
			(offset
				(xyz 0 0 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(gr_line
		(start 53 41.5)
		(end 23.5 41.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 23.5 14.5)
		(end 53 14.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.5 17)
		(end 55.5 39)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 53 14.5)
		(mid 54.767767 15.232233)
		(end 55.5 17)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 21 17)
		(mid 21.732233 15.232233)
		(end 23.5 14.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 21 39)
		(end 21 17)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 23.5 41.5)
		(mid 21.732233 40.767767)
		(end 21 39)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 55.5 39)
		(mid 54.767767 40.767767)
		(end 53 41.5)
		(layer "Edge.Cuts")
	)
	(gr_text "François Gervais\n17 oct. 2024\nv2.0.0"
		(at 50 22.5 0)
		(layer "B.SilkS")
	)
	(gr_text "Motor"
		(at 44.5 18 0)
		(layer "F.SilkS")
	)
	(gr_text "Gnd"
		(at 30 32.75 0)
		(layer "F.SilkS")
	)
	(gr_text "MCU"
		(at 26 18 0)
		(layer "F.SilkS")
	)
	(gr_text "Recv"
		(at 30 29.25 0)
		(layer "F.SilkS")
	)
	(gr_text "Send"
		(at 30 25.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Gnd"
		(at 42 29.25 0)
		(layer "F.SilkS")
	)
	(gr_text "Data"
		(at 42 25.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Vdd"
		(at 30 22.25 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 21 41.5) (xy 21 14.5) (xy 55.5 14.5) (xy 55.5 41.5)
			)
		)
	)
)
