(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 11)
    (no_connects 0)
    (area -0.075001 -0.075001 73.735001 50.885001)
    (thickness 1.6)
    (drawings 9)
    (tracks 32)
    (zones 0)
    (modules 9)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 GND)
  (net 3 +3V3)
  (net 4 /GPIO_0)
  (net 5 "Net-(Q1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /GPIO_0)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(Q1-Pad1)")
  )
  (module Diodes_SMD:D_SMF (layer F.Cu) (tedit 5CC1ECDD)
    (at 136 92.55 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D1 (at 0 -1.8 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 1.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/D_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:TE-1-1734261-2 (layer F.Cu) (tedit 5CC1E4BA)
    (at 175.375 75)
    (fp_text reference J1 (at 10 1) (layer F.SilkS))
    (fp_text value 1-1734261-2 (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 6.875 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 5.625 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /GPIO_0))
    (pad 3 smd rect (at 4.375 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 3.125 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.875 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.625 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.625 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 8 smd rect (at -1.875 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -3.125 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -4.375 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -5.625 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -6.875 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" smd rect (at -9.425 -2.9) (size 2.1 3) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 9.425 -2.9) (size 2.1 3) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors_CUI:CUI-RCJ-017 (layer F.Cu) (tedit 5CC1E8CC)
    (at 127.5 95.4 90)
    (fp_text reference J2 (at 0 3 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -7.5 90) (layer F.Fab))
    (pad 2 thru_hole oval (at -5 0 90) (size 4 5) (drill 2.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -4.5 90) (size 5 4) (drill 2.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.4 3.4) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 5 0 90) (size 4 5) (drill 2.6) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC3991A)
    (at 123.81 73.81)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC39917)
    (at 123.81 116.99)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC3991F)
    (at 189.85 73.81)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC3991C)
    (at 189.85 116.99)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 180 84 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 2N7002-7-F (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 181 79 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /GPIO_0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Ettus B200/B205 mini external PTT interface\n4/26/2019 - Cedric Priscal" (at 163 105) (layer F.SilkS))
  (gr_arc (start 123.81 116.99) (end 123.81 120.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 189.85 117) (end 193.66 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 189.85 73.81) (end 189.85 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.81 73.81) (end 120 73.81) (angle 89.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.66 73.81) (end 193.66 116.99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120 73.81) (end 120 116.99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.81 120.8) (end 189.85 120.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.81 70) (end 189.85 70) (layer Edge.Cuts) (width 0.15))
)
