(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0)")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 71)
    (zones 0)
    (modules 8)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J2-Pad1)")
  (net 4 "Net-(J3-Pad4)")
  (net 5 "Net-(J3-Pad3)")
  (net 6 "Net-(J3-Pad2)")
  (net 7 "Net-(J3-Pad1)")
  (net 8 "Net-(J4-Pad3)")
  (net 9 "Net-(J4-Pad2)")
  (net 10 "Net-(J4-Pad1)")
  (net 11 "Net-(J5-Pad1)")
  (net 12 "Net-(J6-Pad1)")
  (net 13 "Net-(R1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(R1-Pad1)")
  )
  (module weird-disp:5991fixed (layer F.Cu) (tedit 60C951B5)
    (at 33.655 39.37 180)
    (attr virtual)
    (fp_text reference V1 (at 10.795 0.635 90) (layer F.SilkS) hide)
    (fp_text value B-5991 (at -10.795 0 270) (layer F.SilkS) hide)
    (pad 13 thru_hole circle (at 1.199889 5.19729 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 1.199889 -5.19729 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 180) (size 5 5) (drill 5) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0 8.636 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J6-Pad1)"))
    (pad 2 thru_hole circle (at 5.588 4.318 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 11 thru_hole circle (at -3.7846 7.7597 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 10 thru_hole circle (at -5.588 4.318 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 9 thru_hole circle (at -5.588 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad3)"))
    (pad 8 thru_hole circle (at -5.588 -4.318 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J3-Pad4)"))
    (pad 7 thru_hole circle (at -3.7846 -7.7597 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad3)"))
    (pad 6 thru_hole circle (at 0 -8.636 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad1)"))
    (pad 5 thru_hole circle (at 3.7846 -7.7597 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad2)"))
    (pad 4 thru_hole circle (at 5.588 -4.318 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at 5.588 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole oval (at 3.7846 7.7597 116) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(R1-Pad1)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 60C94D7A)
    (at 43.18 25.4)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 37.465 25.4 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.37) (layer F.SilkS))
    (fp_text value 30K (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 60C9175A)
    (at 25.4 25.4)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J5 (at 2.54 -0.635) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 60C9179D)
    (at 25.4 30.48)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 60C91AE1)
    (at 25.4 48.26)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2 (at -0.635 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 60C91B08)
    (at 43.18 30.48)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at -2.54 -0.635) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 60C91B1D)
    (at 43.18 43.18)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 3 (at 41.275 48.26) (layer F.SilkS))
  (gr_text 7 (at 41.275 45.72) (layer F.SilkS))
  (gr_text 6 (at 41.275 43.18) (layer F.SilkS))
  (gr_text "4\n" (at 41.275 38.1) (layer F.SilkS))
  (gr_text 2 (at 27.305 48.26) (layer F.SilkS))
  (gr_text 5 (at 41.275 35.56) (layer F.SilkS))
  (gr_text 1 (at 41.275 33.02) (layer F.SilkS))
  (gr_text 0 (at 41.275 30.48) (layer F.SilkS))
  (gr_text "DPL\n" (at 38.735 25.4) (layer F.SilkS))
  (gr_text 9 (at 27.305 33.02) (layer F.SilkS))
  (gr_text 8 (at 27.305 30.48) (layer F.SilkS))
  (gr_text "A\n" (at 27.305 25.4) (layer F.SilkS))
  (gr_line (start 24.13 24.13) (end 44.45 24.13) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 24.13 49.53) (end 24.13 24.13) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 44.45 49.53) (end 24.13 49.53) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 44.45 24.13) (end 44.45 49.53) (layer Edge.Cuts) (width 0.05))
)
