(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 6)
    (no_connects 0)
    (area 136.703999 102.921999 167.207001 119.582001)
    (thickness 1.6)
    (drawings 19)
    (tracks 11)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(GPS1-Pad1)")
  (net 2 "Net-(GPS1-Pad2)")
  (net 3 "Net-(GPS1-Pad3)")
  (net 4 "Net-(GPS1-Pad4)")
  (net 5 GND)
  (net 6 "Net-(GPS1-Pad6)")
  (net 7 "Net-(UART1-Pad1)")
  (net 8 "Net-(UART1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(GPS1-Pad1)")
    (add_net "Net-(GPS1-Pad2)")
    (add_net "Net-(GPS1-Pad3)")
    (add_net "Net-(GPS1-Pad4)")
    (add_net "Net-(GPS1-Pad6)")
    (add_net "Net-(UART1-Pad1)")
    (add_net "Net-(UART1-Pad4)")
  )
  (net_class Tracks ""
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5CD19EE6)
    (at 152.019 109.982 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference 1PPS (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(GPS1-Pad4)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x06_Pitch2.54mm (layer F.Cu) (tedit 5CD19E76)
    (at 157.099 117.602 180)
    (descr "Through hole angled socket strip, 1x06, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x06 2.54mm single row")
    (fp_text reference GPS (at -6.858 6.35 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x06_Female (at -4.38 14.97 180) (layer F.Fab))
    (fp_text user %R (at -4.38 -2.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(GPS1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(GPS1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(GPS1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(GPS1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(GPS1-Pad6)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x06_Pitch2.54mm (layer B.Cu) (tedit 5CD19E34)
    (at 146.812 117.602)
    (descr "Through hole angled socket strip, 1x06, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x06 2.54mm single row")
    (fp_text reference UART (at -5.842 -7.493) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at -4.38 -14.97) (layer B.Fab))
    (fp_text user %R (at -4.38 2.27) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(UART1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(GPS1-Pad3)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(GPS1-Pad2)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(UART1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(GPS1-Pad6)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_text GPS (at 163.068 117.602) (layer B.SilkS))
  (gr_text RX (at 163.068 115.062) (layer B.SilkS))
  (gr_text TX (at 163.068 112.522) (layer B.SilkS))
  (gr_text 1PPS (at 163.068 109.982) (layer B.SilkS))
  (gr_text GND (at 163.068 107.442) (layer B.SilkS))
  (gr_text VCC (at 163.068 104.902) (layer B.SilkS))
  (gr_text UART (at 140.97 117.602) (layer F.SilkS))
  (gr_text RX (at 140.97 115.062) (layer F.SilkS))
  (gr_text TX (at 140.97 112.522) (layer F.SilkS))
  (gr_text GND (at 140.97 107.442) (layer F.SilkS))
  (gr_text VCC (at 140.97 104.902) (layer F.SilkS))
  (gr_line (start 137.668 102.997) (end 166.243 102.997) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.779 118.618) (end 136.779 103.886) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.132 118.618) (end 167.132 103.886) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.668 119.507) (end 166.243 119.507) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.243 118.618) (end 167.132 118.618) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.668 118.618) (end 137.668 119.507) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.243 103.886) (end 166.243 102.997) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.668 103.886) (end 136.779 103.886) (angle 90) (layer Edge.Cuts) (width 0.15))
)
