<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.0">
<drawing>
<board>
<plain>
<text>Nevma board
rev. 2</text>
<wire x1="40.762" y1="40" x2="60" y2="40" width="0.1524" layer="20"/>
<wire x1="40.762" y1="20" x2="40.762" y2="40" width="0.1524" layer="20"/>
<wire x1="60" y1="20" x2="40.762" y2="20" width="0.1524" layer="20"/>
<wire x1="60" y1="40" x2="60" y2="20" width="0.1524" layer="20"/>
<text>3.3V
SCL
SDA
D1
D0
D6</text>
<text>VIN
GND
SCL
SDA
INT</text>
<text>GND</text>
<text>Designed by Dimitris Platis</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="SparkFun-Connectors" package="1X05_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="INT">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="D0">
<contactref element="J1" pad="5"/>
</signal>
<signal name="D6">
<contactref element="J1" pad="6"/>
</signal>
<signal name="5V">
<contactref element="J3" pad="2"/>
</signal>
<signal name="RST">
<contactref element="J3" pad="3"/>
</signal>
<signal name="D14">
<contactref element="J3" pad="4"/>
</signal>
<signal name="D15">
<contactref element="J3" pad="5"/>
</signal>
<signal name="D16">
<contactref element="J3" pad="6"/>
</signal>
<signal name="A2">
<contactref element="J4" pad="6"/>
</signal>
<signal name="A1">
<contactref element="J4" pad="5"/>
</signal>
<signal name="A0">
<contactref element="J4" pad="4"/>
</signal>
<signal name="D9">
<contactref element="J4" pad="3"/>
</signal>
<signal name="D10">
<contactref element="J4" pad="2"/>
</signal>
<signal name="D11">
<contactref element="J4" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
