(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 14)
    (no_connects 0)
    (area 132.004999 87.601666 204.560001 118.185001)
    (thickness 1.6)
    (drawings 9)
    (tracks 84)
    (zones 0)
    (modules 5)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad3)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad6)")
  (net 5 "Net-(D1-Pad5)")
  (net 6 "Net-(D1-Pad4)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D1-Pad5)")
    (add_net "Net-(D1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
  )
  (module Connect:RJ45_8 (layer F.Cu) (tedit 578A20F6)
    (at 194.945 104.14 90)
    (tags RJ45)
    (fp_text reference J1 (at 0.254 4.826 90) (layer F.SilkS))
    (fp_text value RJ45 (at 0.14224 -0.1016 180) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 5.93852 0 90) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0 90) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 -6.35 90) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at -3.175 -8.89 90) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad6)"))
    (pad 3 thru_hole circle (at -1.905 -6.35 90) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 4 thru_hole circle (at -0.635 -8.89 90) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D1-Pad5)"))
    (pad 5 thru_hole circle (at 0.635 -6.35 90) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad3)"))
    (pad 6 thru_hole circle (at 1.905 -8.89 90) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D1-Pad4)"))
    (pad 7 thru_hole circle (at 3.175 -6.35 90) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 4.445 -8.89 90) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 0)
    (at 169.545 111.76)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 184.785 92.71 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D1-Pad5)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad3)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D1-Pad4)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 0)
    (at 169.545 96.52)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -3.50012) (layer F.SilkS))
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module lighting:10wled (layer F.Cu) (tedit 578E284E)
    (at 149 105)
    (fp_text reference D1 (at 0 4) (layer F.SilkS))
    (fp_text value LED_RGB (at 0 -4) (layer F.Fab))
    (pad 2 smd oval (at -12.065 0) (size 3.81 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 3 smd oval (at -12.065 -2.54) (size 3.81 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad3)"))
    (pad 1 smd oval (at -12.065 2.54) (size 3.81 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 6 smd oval (at 12.065 2.54) (size 3.81 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad6)"))
    (pad 5 smd oval (at 12.065 0) (size 3.81 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad5)"))
    (pad 4 smd oval (at 12.065 -2.54) (size 3.81 1.524) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad4)"))
  )
  (gr_line (start 132.08 118.11) (end 204.47 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 90.17) (end 132.08 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.47 90.17) (end 132.08 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.47 118.11) (end 204.47 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "CUT OUT" (at 149.225 104.775) (layer F.SilkS))
  (gr_line (start 139 115) (end 139 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159 115) (end 139 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159 95) (end 159 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 95) (end 159 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139 95) (xy 159 95) (xy 159 115) (xy 139 115)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139 95) (xy 159 95) (xy 159 115) (xy 139 115)
      )
    )
  )
)
