(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 38)
    (no_connects 0)
    (area 143.180999 110.414999 151.967001 116.788001)
    (thickness 0.8)
    (drawings 12)
    (tracks 164)
    (zones 0)
    (modules 20)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.13)
    (zone_clearance 0.15)
    (zone_45_only no)
    (trace_min 0.13)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.775 1.24)
    (pad_drill 0)
    (pad_to_mask_clearance 0.08)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFE7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(C2-Pad1)")
  (net 4 VIDEO)
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(D1-Pad2)")
  (net 7 CONFIGURE)
  (net 8 +BATT)
  (net 9 "Net-(R1-Pad2)")
  (net 10 "Net-(R3-Pad2)")
  (net 11 "Net-(R5-Pad1)")
  (net 12 "Net-(R6-Pad1)")
  (net 13 "Net-(U1-Pad5)")
  (net 14 "Net-(U1-Pad9)")
  (net 15 "Net-(U1-Pad10)")
  (net 16 "Net-(J3-Pad1)")
  (net 17 "Net-(J4-Pad1)")
  (net 18 "Net-(J5-Pad1)")
  (net 19 "Net-(U1-Pad8)")
  (net 20 "Net-(R7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.13)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net CONFIGURE)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (net_class GND ""
    (clearance 0.12)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class ProgLine ""
    (clearance 0.13)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
  )
  (net_class Thin ""
    (clearance 0.13)
    (trace_width 0.13)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net VIDEO)
  )
  (net_class VCC ""
    (clearance 0.13)
    (trace_width 0.3)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VCC)
  )
  (module C_0603 (layer B.Cu) (tedit 593194D3)
    (at 151.13 113.538 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C_0603 (layer F.Cu) (tedit 593194B7)
    (at 144.907 113.284 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 2.2uf (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 4pin_SMD_small (layer F.Cu) (tedit 5931896A)
    (at 151.384 115.189 90)
    (fp_text reference J1 (at 1.27 2.54 90) (layer F.SilkS) hide)
    (fp_text value Camera (at 1.27 -2.54 90) (layer F.Fab) hide)
    (pad 4 smd rect (at 4 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 VIDEO))
    (pad 3 smd rect (at 2.5 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 +BATT))
  )
  (module D_SOD-523 (layer F.Cu) (tedit 59317AB2)
    (at 145.669 111.252)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D1 (at 0 -1.3) (layer F.SilkS) hide)
    (fp_text value 1N4148WT (at 0 1.4) (layer F.Fab))
    (fp_text user %R (at 0 -1.3) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Prog_pad (layer F.Cu) (tedit 5938F6E1)
    (at 149.225 110.871)
    (fp_text reference J3 (at 0.75 1.5) (layer F.SilkS) hide)
    (fp_text value RST (at 0 -1.75) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad1)") (solder_mask_margin 0.02))
  )
  (module MSOP-10_3x3mm_Pitch0.5mm locked (layer B.Cu) (tedit 5931761D)
    (at 147.32 113.411)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 2.6) (layer B.SilkS) hide)
    (fp_text value LMH1980 (at 0 -2.6) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.2 1) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at -2.2 0.5) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.2 0) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at -2.2 -0.5) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at -2.2 -1) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 2.2 -1) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R5-Pad1)"))
    (pad 7 smd rect (at 2.2 -0.5) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R6-Pad1)"))
    (pad 8 smd rect (at 2.2 0) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 2.2 0.5) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 2.2 1) (size 1.4 0.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U1-Pad10)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/MSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DFN-10-1EP_3x3mm_Pitch0.5mm locked (layer F.Cu) (tedit 597F1D53)
    (at 148.082 113.411 270)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U2 (at 0 -2.575 270) (layer F.SilkS) hide)
    (fp_text value ATTINY13A-MMF (at 0 2.575 270) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -1 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -1.55 -0.5 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -1.55 0 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.55 0.5 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 5 smd rect (at -1.55 1 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.55 1 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R7-Pad2)"))
    (pad 7 smd rect (at 1.55 0.5 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J4-Pad1)"))
    (pad 8 smd rect (at 1.55 0 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 1.55 -0.5 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J5-Pad1)"))
    (pad 10 smd rect (at 1.55 -1 270) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 11 smd rect (at 0.3875 0.62 270) (size 0.775 1.24) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at 0.3875 -0.62 270) (size 0.775 1.24) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.3875 0.62 270) (size 0.775 1.24) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.3875 -0.62 270) (size 0.775 1.24) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59314D84)
    (at 146.685 111.252)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 1.27) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.27) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 VIDEO))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 59316C49)
    (at 145.796 113.411 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0 -1.27 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59314DA3)
    (at 143.764 114.3 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 1.2 270) (layer B.SilkS) hide)
    (fp_text value "10K 1%" (at 0 -1.25 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 597EF9EE)
    (at 143.764 111.633 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 1.2 90) (layer B.SilkS) hide)
    (fp_text value 220 (at 0 -1.25 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VIDEO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59316C65)
    (at 150.114 114.046 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 -1.2 90) (layer F.SilkS) hide)
    (fp_text value 15K (at 0 1.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.2 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 +BATT))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59316C5A)
    (at 150.114 112.014 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.2 270) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.25 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.2 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 597EF9D9)
    (at 150.876 115.697 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 1.2 180) (layer B.SilkS) hide)
    (fp_text value 120 (at 0 -1.25 180) (layer B.Fab))
    (fp_text user %R (at 0 1.2 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Prog_pad (layer F.Cu) (tedit 5938F6D4)
    (at 146.177 116.078)
    (fp_text reference J4 (at 0.75 1.5) (layer F.SilkS) hide)
    (fp_text value MISO (at 0 -1.75) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J4-Pad1)") (solder_mask_margin 0.02))
  )
  (module .pretty:Prog_pad (layer F.Cu) (tedit 5938F6D9)
    (at 148.59 116.078)
    (fp_text reference J5 (at 0.75 1.5) (layer F.SilkS) hide)
    (fp_text value SCK (at 0 -1.75) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J5-Pad1)") (solder_mask_margin 0.02))
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 597EFA20)
    (at 147.828 115.29822 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.2 180) (layer B.SilkS) hide)
    (fp_text value 120 (at 0 -1.25 180) (layer B.Fab))
    (fp_text user %R (at 0 1.2 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:4pin_SMD_small (layer F.Cu) (tedit 5931896A)
    (at 143.764 115.189 90)
    (fp_text reference J2 (at 1.27 2.54 90) (layer F.SilkS) hide)
    (fp_text value VTX (at 1.27 -2.54 90) (layer F.Fab) hide)
    (pad 4 smd rect (at 4 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 VIDEO))
    (pad 3 smd rect (at 2.5 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 CONFIGURE))
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 597EFA02)
    (at 145.415 115.062)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.2) (layer F.SilkS) hide)
    (fp_text value 120 (at 0 1.25) (layer F.Fab))
    (fp_text user %R (at 0 -1.2) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 CONFIGURE))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 597EFCE9)
    (at 147.44954 113.38052)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 2) (layer B.SilkS) hide)
    (fp_text value Measurement_Point_Square-SMD-Pad_Small (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (gr_line (start 151.892 116.713) (end 151.892 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.256 110.49) (end 143.256 116.459) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.638 116.459) (end 151.638 116.713) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.256 116.459) (end 151.638 116.459) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.892 116.713) (end 151.638 116.713) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text B-uOSD (at 145.161 115.951 180) (layer B.SilkS))
  (gr_text B (at 150.241 115.824) (layer F.SilkS))
  (gr_text C (at 144.907 115.951) (layer F.SilkS))
  (gr_line (start 143.256 110.49) (end 151.892 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
)
