(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/Pin_1")
  (net 2 "/Pin_2")
  (net 3 "/Pin_3")
  (net 4 "/Pin_4")
  (net 5 "/Pin_5")
  (net 6 "/Pin_6")
  (net 7 "/Pin_7")
  (net 8 "/Pin_8")
  (net 9 "/Pin_9")
  (net 10 "/Pin_10")
  (footprint "N8FDY:MICRO10_3X3_ONS" (layer "F.Cu")
    (tedit 0)
    (at 146.05 86.36 90)
    (property "DIgi-Key Part Number" "NLAS4684MR2GOSCT-ND")
    (property "Description" "Analog Switch ICs Dual SPDT 0.5ohm Sw. Low R(on) Ind. Temp")
    (property "Digi-Key Price/Stock" "https://www.digikey.com/short/fn414d7b")
    (property "Manufacturer_Name" "onsemi")
    (property "Manufacturer_Part_Number" "NLAS4684MR2G")
    (property "Sheetfile" "File: Micro10 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "IC101" (at 0.254 2.7432 90) (layer "F.SilkS") hide)
    (fp_text value "Micro10" (at 7.62 0 180) (layer "F.SilkS"))
    (fp_text user "*" (at -2.3876 -1.4732 90) (layer "F.SilkS"))
    (pad "1" smd rect (at -2.1717 -1.000001 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Pin_1") (pinfunction "Vcc") (pintype "power_in"))
    (pad "2" smd rect (at -2.1717 -0.499999 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/Pin_2") (pinfunction "NO1") (pintype "passive"))
    (pad "3" smd rect (at -2.1717 0 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/Pin_3") (pinfunction "COM1") (pintype "passive"))
    (pad "4" smd rect (at -2.1717 0.499999 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/Pin_4") (pinfunction "IN1") (pintype "input"))
    (pad "5" smd rect (at -2.1717 1.000001 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/Pin_5") (pinfunction "NC1") (pintype "passive"))
    (pad "6" smd rect (at 2.1717 1.000001 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/Pin_6") (pinfunction "GND") (pintype "passive"))
    (pad "7" smd rect (at 2.1717 0.499999 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/Pin_7") (pinfunction "NC2") (pintype "passive"))
    (pad "8" smd rect (at 2.1717 0 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/Pin_8") (pinfunction "IN2") (pintype "input"))
    (pad "9" smd rect (at 2.1717 -0.499999 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/Pin_9") (pinfunction "COM2") (pintype "passive"))
    (pad "10" smd rect (at 2.1717 -1.000001 90) (size 1.27 0.254) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/Pin_10") (pinfunction "NO2") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 149.86 91.435)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "File: Micro10 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J102" (at 0.3 -12.58) (layer "B.SilkS") hide)
    (fp_text value "Pin 6-19" (at 0.1 2.72) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/Pin_6") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/Pin_7") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/Pin_8") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/Pin_9") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/Pin_10") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 142.24 81.285 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "File: Micro10 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J101" (at 0 2.33) (layer "B.SilkS") hide)
    (fp_text value "Pin 1-5" (at 0 -12.49) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/Pin_1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/Pin_2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/Pin_3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/Pin_4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/Pin_5") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 138.43 95.25) (end 153.67 77.47) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "10" (at 152.4 81.28 90) (layer "F.SilkS"))
  (gr_text "5" (at 139.7 91.44 -90) (layer "F.SilkS"))
  (gr_text "4" (at 139.7 88.9 -90) (layer "F.SilkS"))
  (gr_text "PCB 013, N8FDY" (at 146.05 93.98) (layer "F.SilkS"))
  (gr_text "1" (at 139.7 81.28 -90) (layer "F.SilkS"))
  (gr_text "9" (at 152.4 83.82 90) (layer "F.SilkS"))
  (gr_text "7" (at 152.4 88.9 90) (layer "F.SilkS"))
  (gr_text "6" (at 152.4 91.44 90) (layer "F.SilkS"))
  (gr_text "3" (at 139.7 86.36 -90) (layer "F.SilkS"))
  (gr_text "8" (at 152.4 86.36 90) (layer "F.SilkS"))
  (gr_text "2" (at 139.7 83.82 -90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 138.43 77.47) (xy 153.67 77.47))
    (height -3.81)
    (gr_text "15.2400 mm" (at 146.05 72.51) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 138.43 77.47) (xy 138.43 95.25))
    (height 5.08)
    (gr_text "17.7800 mm" (at 132.2 86.36 90) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 149.86 96.52) (xy 142.24 96.52))
    (height -2.54)
    (gr_text "7.6200 mm" (at 146.05 97.91) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
)
