(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 0.8)
    (drawings 30)
    (tracks 103)
    (zones 0)
    (modules 9)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.1 2.1)
    (pad_drill 2.1)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 /SV3)
  (net 4 /ESC)
  (net 5 /UBAT)
  (net 6 /Aux)
  (net 7 /SV4)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class ext ""
    (clearance 0.25)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net +5V)
    (add_net /Aux)
    (add_net /ESC)
    (add_net /SV3)
    (add_net /SV4)
    (add_net /UBAT)
    (add_net GND)
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x06_P2.00mm_Vertical (layer F.Cu) (tedit 5F5947EE)
    (at 105 99.06 90)
    (descr "Through hole straight pin header, 1x06, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.00mm single row")
    (fp_text reference J3 (at 0 -2.06 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 12.06 90) (layer F.Fab))
    (fp_text user %R (at 0 5 180) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /UBAT))
    (pad 4 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /Aux))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /ESC))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /SV4))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /SV3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x06_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5F5947CF)
    (at 114 121 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value ESC (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /ESC))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /UBAT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5F59479C)
    (at 121 111.252)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 7.62) (layer F.SilkS) hide)
    (fp_text value AUX (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Aux))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5F59473D)
    (at 121 103.632)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value SV4 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SV4))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5F594710)
    (at 99 107.46)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference SV3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value SV3 (at 0 7.41) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 90) (layer F.Fab) hide)
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SV3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 120 120)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 100 120)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 120 100)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 100 100)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (gr_text "CUT OUT" (at 110.49 109.982) (layer Dwgs.User))
  (gr_text @fab1anhu (at 101.854 117.348 -45) (layer F.SilkS))
  (gr_text 2020 (at 99.568 104.14 45) (layer B.SilkS))
  (gr_text @fab1anhu (at 102.87 103.124 45) (layer B.SilkS))
  (gr_text "NOXE\nWing" (at 102.362 117.602 -45) (layer B.SilkS))
  (gr_text 2 (at 119.38 111.252) (layer F.SilkS))
  (gr_text 4 (at 119.126 103.632) (layer F.SilkS))
  (gr_text 3412 (at 104.648 101.092) (layer F.SilkS))
  (gr_text B (at 113.03 100.838) (layer F.SilkS))
  (gr_text - (at 115.062 100.584) (layer F.SilkS))
  (gr_text + (at 119.38 106.172) (layer F.SilkS))
  (gr_text + (at 119.126 113.792) (layer F.SilkS))
  (gr_text - (at 119.38 108.712) (layer F.SilkS))
  (gr_text - (at 118.872 116.332) (layer F.SilkS))
  (gr_text 1 (at 111.76 119.38) (layer F.SilkS))
  (gr_text BAT (at 114.3 119.38) (layer F.SilkS))
  (gr_text + (at 108.712 119.38) (layer F.SilkS))
  (gr_text - (at 106.172 119.38) (layer F.SilkS))
  (gr_text - (at 100.584 112.522) (layer F.SilkS))
  (gr_text 3 (at 100.584 107.442) (layer F.SilkS))
  (gr_text + (at 100.584 109.982) (layer F.SilkS))
  (gr_circle (center 110 110) (end 118.8 110) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 120 100) (end 123 100) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 120 120) (end 120 123) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 100 120) (end 97 120) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 100 100) (end 100 97) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97 120) (end 97 100) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120 123) (end 100 123) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123 100) (end 123 120) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100 97) (end 120 97) (layer Edge.Cuts) (width 0.05))
)
