(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 0)
    (no_connects 0)
    (area 71.044999 53.264999 223.595001 155.015001)
    (thickness 1.6)
    (drawings 8)
    (tracks 0)
    (zones 0)
    (modules 3)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Mounting_Holes:MountingHole_8.4mm_M8_Pad_Via (layer F.Cu) (tedit 56DDC8DB)
    (at 213.36 144.78)
    (descr "Mounting Hole 8.4mm, M8")
    (tags "mounting hole 8.4mm m8")
    (attr virtual)
    (fp_text reference REF** (at 0 -9.4) (layer F.SilkS))
    (fp_text value MountingHole_8.4mm_M8_Pad_Via (at 0 9.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 16.8 16.8) (drill 8.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.3 0) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.454773 4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 6.3) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -4.454773 4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.3 0) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -4.454773 -4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -6.3) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.454773 -4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_8.4mm_M8_Pad_Via (layer F.Cu) (tedit 56DDC8DB)
    (at 81.28 63.5)
    (descr "Mounting Hole 8.4mm, M8")
    (tags "mounting hole 8.4mm m8")
    (attr virtual)
    (fp_text reference REF** (at 0 -9.4) (layer F.SilkS))
    (fp_text value MountingHole_8.4mm_M8_Pad_Via (at 0 9.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 16.8 16.8) (drill 8.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.3 0) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.454773 4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 6.3) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -4.454773 4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.3 0) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -4.454773 -4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -6.3) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.454773 -4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_8.4mm_M8_Pad_Via (layer F.Cu) (tedit 56DDC8DB)
    (at 213.36 63.5)
    (descr "Mounting Hole 8.4mm, M8")
    (tags "mounting hole 8.4mm m8")
    (attr virtual)
    (fp_text reference REF** (at 0 -9.4) (layer F.SilkS))
    (fp_text value MountingHole_8.4mm_M8_Pad_Via (at 0 9.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 16.8 16.8) (drill 8.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.3 0) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.454773 4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 6.3) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -4.454773 4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.3 0) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -4.454773 -4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -6.3) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.454773 -4.454773) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  )
  (gr_arc (start 213.36 63.5) (end 213.36 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 213.36 144.78) (end 223.52 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 81.28 144.78) (end 81.28 154.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 81.28 63.5) (end 71.12 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.28 53.34) (end 213.36 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.28 154.94) (end 213.36 154.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 223.52 63.5) (end 223.52 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.12 63.5) (end 71.12 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
)
